NAME=p= 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p= 0
EXPECT=<<EOF
EOF
RUN

NAME=p=b 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p=b 0
EXPECT=<<EOF
EOF
RUN

NAME=p=d 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p=d 0
EXPECT=<<EOF
EOF
RUN

NAME=p=e 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p=e 0
EXPECT=<<EOF
EOF
RUN

NAME=p=p 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p=p 0
EXPECT=<<EOF
EOF
RUN

NAME=p2 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p2 0
EXPECT=<<EOF
EOF
RUN

NAME=p8 0
FILE=bins/elf/analysis/hello-arm32
CMDS=p8 0
EXPECT=<<EOF
EOF
RUN

NAME=pb 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pb 0
EXPECT=<<EOF
EOF
RUN

NAME=pB 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pB 0
EXPECT=<<EOF
EOF
RUN

NAME=px 0
FILE=bins/elf/analysis/hello-arm32
CMDS=px 0
EXPECT=<<EOF
EOF
RUN

NAME=px/ 0
FILE=bins/elf/analysis/hello-arm32
CMDS=px/ 0
EXPECT=<<EOF
EOF
RUN

NAME=pxa 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxa 0
EXPECT=<<EOF
EOF
RUN

NAME=pxA 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxA 0
EXPECT=<<EOF
EOF
RUN

NAME=pxb 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxb 0
EXPECT=<<EOF
EOF
RUN

NAME=pxd1 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxd1 0
EXPECT=<<EOF
EOF
RUN

NAME=pxd2 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxd2 0
EXPECT=<<EOF
EOF
RUN

NAME=pxd4 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxd4 0
EXPECT=<<EOF
EOF
RUN

NAME=pxe 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxe 0
EXPECT=<<EOF
EOF
RUN

NAME=pxh 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxh 0
EXPECT=<<EOF
EOF
RUN

NAME=pxH 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxH 0
EXPECT=<<EOF
EOF
RUN

NAME=pxl 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxl 0
EXPECT=<<EOF
EOF
RUN

NAME=pxo 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxo 0
EXPECT=<<EOF
EOF
RUN

NAME=pxq 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxq 0
EXPECT=<<EOF
EOF
RUN

NAME=pxQ 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxQ 0
EXPECT=<<EOF
EOF
RUN

NAME=pxr 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxr 0
EXPECT=<<EOF
EOF
RUN

NAME=pxs 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxs 0
EXPECT=<<EOF
EOF
RUN

NAME=pxw 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxw 0
EXPECT=<<EOF
EOF
RUN

NAME=pxW 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pxW 0
EXPECT=<<EOF
EOF
RUN

NAME=pc 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pc 0
EXPECT=<<EOF
EOF
RUN

NAME=pc* 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pc* 0
EXPECT=<<EOF
EOF
RUN

NAME=pcw 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcw 0
EXPECT=<<EOF
EOF
RUN

NAME=pcd 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcd 0
EXPECT=<<EOF
EOF
RUN

NAME=pca 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pca 0
EXPECT=<<EOF
EOF
RUN

NAME=pcs 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcs 0
EXPECT=<<EOF
EOF
RUN

NAME=pcS 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcS 0
EXPECT=<<EOF
EOF
RUN

NAME=pcJ 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcJ 0
EXPECT=<<EOF
EOF
RUN

NAME=pcp 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pcp 0
EXPECT=<<EOF
EOF
RUN

NAME=pd 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pd 0
EXPECT=<<EOF
EOF
RUN

NAME=pD 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pD 0
EXPECT=<<EOF
EOF
RUN

NAME=pda 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pda 0
EXPECT=<<EOF
EOF
RUN

NAME=pdj 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pdj 0
EXPECT=<<EOF
EOF
RUN

NAME=pdr 0
FILE=bins/elf/analysis/hello-arm32
CMDS=<<EOF
aa
pdr 0
EOF
EXPECT=<<EOF
EOF
RUN

NAME=pdf 0
FILE=bins/elf/analysis/hello-arm32
CMDS=<<EOF
aa
pdf 0
EOF
EXPECT=<<EOF
EOF
RUN

NAME=pdi 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pdi 0
EXPECT=<<EOF
EOF
RUN

NAME=pdl 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pdl 0
EXPECT=<<EOF
EOF
RUN

NAME=pds 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pds 0
EXPECT=<<EOF
EOF
RUN

NAME=pdt 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pdt 0
EXPECT=<<EOF
EOF
RUN

NAME=pi 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pi 0
EXPECT=<<EOF
EOF
RUN

NAME=pid 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pid 0
EXPECT=<<EOF
EOF
RUN

NAME=pie 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pie 0
EXPECT=<<EOF
EOF
RUN

NAME=pI 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pI 0
EXPECT=<<EOF
EOF
RUN

NAME=pId 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pId 0
EXPECT=<<EOF
EOF
RUN

NAME=pr 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pr 0
EXPECT=<<EOF
EOF
RUN

NAME=prx 0
FILE=bins/elf/analysis/hello-arm32
CMDS=prx 0
EXPECT=<<EOF
EOF
RUN

NAME=prg 0
FILE=bins/elf/analysis/hello-arm32
CMDS=prg 0
EXPECT=<<EOF
EOF
RUN

NAME=pk 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pk 0
EXPECT=<<EOF
EOF
RUN

NAME=pK 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pK 0
EXPECT=<<EOF
EOF
RUN

NAME=ps 0
FILE=bins/elf/analysis/hello-arm32
CMDS=ps 0
EXPECT=<<EOF

EOF
RUN

NAME=psi 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psi 0
EXPECT=<<EOF
EOF
RUN

NAME=psb 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psb 0
EXPECT=<<EOF
EOF
RUN

NAME=psx 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psx 0
EXPECT=<<EOF
EOF
RUN

NAME=psz 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psz 0
EXPECT=<<EOF
EOF
RUN

NAME=psp 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psp 0
EXPECT=<<EOF
EOF
RUN

NAME=psu 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psu 0
EXPECT=<<EOF
EOF
RUN

NAME=psw 0
FILE=bins/elf/analysis/hello-arm32
CMDS=psw 0
EXPECT=<<EOF
EOF
RUN

NAME=pu 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pu 0
EXPECT=<<EOF
EOF
RUN

NAME=puw 0
FILE=bins/elf/analysis/hello-arm32
CMDS=puw 0
EXPECT=<<EOF
EOF
RUN

NAME=pz 0
FILE=bins/elf/analysis/hello-arm32
CMDS=pz 0
EXPECT=<<EOF
EOF
RUN
