ADCIC=io
ADCIC.address=0xff98
ADCIC.comment=A/D Converter End of Conversion Interrupt Control Register
ADCON=io
ADCON.address=0xffa0
ADCON.comment=A/D Converter Control Register
ADDAT=io
ADDAT.address=0xfea0
ADDAT.comment=A/D Converter Result Register
ADDAT2=io
ADDAT2.address=0xf0a0
ADDAT2.comment=A/D Converter 2 Result Register
ADDRSEL1=io
ADDRSEL1.address=0xfe18
ADDRSEL1.comment=Address Select Register 1
ADDRSEL2=io
ADDRSEL2.address=0xfe1a
ADDRSEL2.comment=Address Select Register 2
ADDRSEL3=io
ADDRSEL3.address=0xfe1c
ADDRSEL3.comment=Address Select Register 3
MAL=io
MAL.address=0xfe5c
MAL.comment=MAC Accumulator – Low Word
MAH=io
MAH.address=0xfe5e
MAH.comment=MAC Accumulator – High Word
ADDRSEL4=io
ADDRSEL4.address=0xfe1e
ADDRSEL4.comment=Address Select Register 4
IDX0=io
IDX0.address=0xff08
IDX0.comment=MAC Address Pointer 0
IDX1=io
IDX1.address=0xff0a
IDX1.comment=MAC Address Pointer 1
ADEIC=io
ADEIC.address=0xff9a
ADEIC.comment=A/D Converter Overrun Error Interrupt Control Register
BUSCON0=io
BUSCON0.address=0xff0c
BUSCON0.comment=Bus Configuration Register 0 (Stack Pointer Segment Register [SPSEG])
VECSEG=io
VECSEG.address=0xff12
VECSEG.comment=Bus Configuration Register 0
BUSCON1=io
BUSCON1.address=0xff14
BUSCON1.comment=Bus Configuration Register 1
BUSCON2=io
BUSCON2.address=0xff16
BUSCON2.comment=Bus Configuration Register 2
BUSCON3=io
BUSCON3.address=0xff18
BUSCON3.comment=Bus Configuration Register 3
BUSCON4=io
BUSCON4.address=0xff1a
BUSCON4.comment=Bus Configuration Register 4
MCW=io
MCW.address=0xffdc
MCW.comment=MAC Control Word
MRW=io
MRW.address=0xffda
MRW.comment=MAC Repeat Word
MSW=io
MSW.address=0xffde
MSW.comment=MAC Status Word
C1BTR=io
C1BTR.address=0xef04
C1BTR.comment=CAN1 Bit Timing Register
C1CSR=io
C1CSR.address=0xef00
C1CSR.comment=CAN1 Control / Status Register
C1GMS=io
C1GMS.address=0xef06
C1GMS.comment=CAN1 Global Mask Short
C1IR=io
C1IR.address=0xef02
C1IR.comment=CAN1 Interrupt Register
C1LGML=io
C1LGML.address=0xef0a
C1LGML.comment=CAN1 Lower Global Mask Long
C1LMLM=io
C1LMLM.address=0xef0e
C1LMLM.comment=CAN1 Lower Mask of Last Message
C1UAR=io
C1UAR.address=0xef02
C1UAR.comment=CAN1 Upper Arbitration Register (message n)
C1UGML=io
C1UGML.address=0xef08
C1UGML.comment=CAN1 Upper Global Mask Long
C1UMLM=io
C1UMLM.address=0xef0c
C1UMLM.comment=CAN1 Upper Mask of Last Message
CAPREL=io
CAPREL.address=0xfe4a
CAPREL.comment=GPT2 Capture/Reload Register
CC0=io
CC0.address=0xfe80
CC0.comment=CAPCOM Register 0
CC0IC=io
CC0IC.address=0xff78
CC0IC.comment=CAPCOM Register 0 Interrupt Ctrl. Reg.
CC1=io
CC1.address=0xfe82
CC1.comment=CAPCOM Register 1
CC10=io
CC10.address=0xfe94
CC10.comment=CAPCOM Register 10
CC10IC=io
CC10IC.address=0xff8c
CC10IC.comment=CAPCOM Reg. 10 Interrupt Ctrl. Reg.
CC11=io
CC11.address=0xfe96
CC11.comment=CAPCOM Register 11
CC11IC=io
CC11IC.address=0xff8e
CC11IC.comment=CAPCOM Reg. 11 Interrupt Ctrl. Reg.
CC12=io
CC12.address=0xfe98
CC12.comment=CAPCOM Register 12
CC12IC=io
CC12IC.address=0xff90
CC12IC.comment=CAPCOM Reg. 12 Interrupt Ctrl. Reg.
CC13=io
CC13.address=0xfe9a
CC13.comment=CAPCOM Register 13
CC13IC=io
CC13IC.address=0xff92
CC13IC.comment=CAPCOM Reg. 13 Interrupt Ctrl. Reg.
CC14=io
CC14.address=0xfe9c
CC14.comment=CAPCOM Register 14
CC14IC=io
CC14IC.address=0xff94
CC14IC.comment=CAPCOM Reg. 14 Interrupt Ctrl. Reg.
CC15=io
CC15.address=0xfe9e
CC15.comment=CAPCOM Register 15
CC15IC=io
CC15IC.address=0xff96
CC15IC.comment=CAPCOM Reg. 15 Interrupt Ctrl. Reg.
CC16=io
CC16.address=0xfe60
CC16.comment=CAPCOM Register 16
CC16IC=io
CC16IC.address=0xf160
CC16IC.comment=CAPCOM Reg. 16 Interrupt Ctrl. Reg.
CC17=io
CC17.address=0xfe62
CC17.comment=CAPCOM Register 17
CC17IC=io
CC17IC.address=0xf162
CC17IC.comment=CAPCOM Reg. 17 Interrupt Ctrl. Reg.
CC18=io
CC18.address=0xfe64
CC18.comment=CAPCOM Register 18
CC18IC=io
CC18IC.address=0xf164
CC18IC.comment=CAPCOM Reg. 18 Interrupt Ctrl. Reg.
CC19=io
CC19.address=0xfe66
CC19.comment=CAPCOM Register 19
CC19IC=io
CC19IC.address=0xf166
CC19IC.comment=CAPCOM Reg. 19 Interrupt Ctrl. Reg.
CC1IC=io
CC1IC.address=0xff7a
CC1IC.comment=CAPCOM Reg. 1 Interrupt Ctrl. Reg.
CC2=io
CC2.address=0xfe84
CC2.comment=FE84H 42H CAPCOM Register 2
CC20=io
CC20.address=0xfe68
CC20.comment=CAPCOM Register 20
CC20IC=io
CC20IC.address=0xf168
CC20IC.comment=CAPCOM Reg. 20 Interrupt Ctrl. Reg.
CC21=io
CC21.address=0xfe6a
CC21.comment=CAPCOM Register 21
CC21IC=io
CC21IC.address=0xf16a
CC21IC.comment=CAPCOM Reg. 21 Interrupt Ctrl. Reg.
CC22=io
CC22.address=0xfe6c
CC22.comment=CAPCOM Register 22
CC22IC=io
CC22IC.address=0xf16c
CC22IC.comment=CAPCOM Reg. 22 Interrupt Ctrl. Reg.
CC23=io
CC23.address=0xfe6e
CC23.comment=CAPCOM Register 23
CC23IC=io
CC23IC.address=0xf16e
CC23IC.comment=CAPCOM Reg. 23 Interrupt Ctrl. Reg.
CC24=io
CC24.address=0xfe70
CC24.comment=CAPCOM Register 24
CC24IC=io
CC24IC.address=0xf170
CC24IC.comment=CAPCOM Reg. 24 Interrupt Ctrl. Reg.
CC25=io
CC25.address=0xfe72
CC25.comment=CAPCOM Register 25
CC25IC=io
CC25IC.address=0xf172
CC25IC.comment=CAPCOM Reg. 25 Interrupt Ctrl. Reg.
CC26=io
CC26.address=0xfe74
CC26.comment=CAPCOM Register 26
CC26IC=io
CC26IC.address=0xf174
CC26IC.comment=CAPCOM Reg. 26 Interrupt Ctrl. Reg.
CC27=io
CC27.address=0xfe76
CC27.comment=CAPCOM Register 27
CC27IC=io
CC27IC.address=0xf176
CC27IC.comment=CAPCOM Reg. 27 Interrupt Ctrl. Reg.
CC28=io
CC28.address=0xfe78
CC28.comment=CAPCOM Register 28
CC28IC=io
CC28IC.address=0xf178
CC28IC.comment=CAPCOM Reg. 28 Interrupt Ctrl. Reg.
CC29=io
CC29.address=0xfe7a
CC29.comment=CAPCOM Register 29
CC29IC=io
CC29IC.address=0xf184
CC29IC.comment=CAPCOM Reg. 29 Interrupt Ctrl. Reg.
CC2IC=io
CC2IC.address=0xff7c
CC2IC.comment=CAPCOM Reg. 2 Interrupt Ctrl. Reg.
CC3=io
CC3.address=0xfe86
CC3.comment=CAPCOM Register 3
CC30=io
CC30.address=0xfe7c
CC30.comment=CAPCOM Register 30
CC30IC=io
CC30IC.address=0xf18c
CC30IC.comment=CAPCOM Reg. 30 Interrupt Ctrl. Reg.
CC31=io
CC31.address=0xfe7e
CC31.comment=CAPCOM Register 31
CC31IC=io
CC31IC.address=0xf194
CC31IC.comment=CAPCOM Reg. 31 Interrupt Ctrl. Reg.
CC3IC=io
CC3IC.address=0xff7e
CC3IC.comment=CAPCOM Reg. 3 Interrupt Ctrl. Reg.
CC4=io
CC4.address=0xfe88
CC4.comment=CAPCOM Register 4
CC4IC=io
CC4IC.address=0xff80
CC4IC.comment=CAPCOM Reg. 4 Interrupt Ctrl. Reg.
CC5=io
CC5.address=0xfe8a
CC5.comment=CAPCOM Register 5
CC5IC=io
CC5IC.address=0xff82
CC5IC.comment=CAPCOM Register 5 Interrupt Control Register
CC6=io
CC6.address=0xfe8c
CC6.comment=CAPCOM Register 6
CC6IC=io
CC6IC.address=0xff84
CC6IC.comment=CAPCOM Reg. 6 Interrupt Ctrl. Reg.
CC7=io
CC7.address=0xfe8e
CC7.comment=CAPCOM Register 7
CC7IC=io
CC7IC.address=0xff86
CC7IC.comment=CAPCOM Reg. 7 Interrupt Ctrl. Reg.
CC8=io
CC8.address=0xfe90
CC8.comment=CAPCOM Register 8
CC8IC=io
CC8IC.address=0xff88
CC8IC.comment=CAPCOM Reg. 8 Interrupt Ctrl. Reg.
CC9=io
CC9.address=0xfe92
CC9.comment=CAPCOM Register 9
CC9IC=io
CC9IC.address=0xff8a
CC9IC.comment=CAPCOM Reg. 9 Interrupt Ctrl. Reg.
CCM0=io
CCM0.address=0xff52
CCM0.comment=CAPCOM Mode Control Register 0
CCM1=io
CCM1.address=0xff54
CCM1.comment=CAPCOM Mode Control Register 1
CCM2=io
CCM2.address=0xff56
CCM2.comment=CAPCOM Mode Control Register 2
CCM3=io
CCM3.address=0xff58
CCM3.comment=CAPCOM Mode Control Register 3
CCM4=io
CCM4.address=0xff22
CCM4.comment=CAPCOM Mode Control Register 4
CCM5=io
CCM5.address=0xff24
CCM5.comment=CAPCOM Mode Control Register 5
CCM6=io
CCM6.address=0xff26
CCM6.comment=CAPCOM Mode Control Register 6
CCM7=io
CCM7.address=0xff28
CCM7.comment=CAPCOM Mode Control Register 7
CP=io
CP.address=0xfe10
CP.comment=CPU Context Pointer Register
CRIC=io
CRIC.address=0xff6a
CRIC.comment=GPT2 CAPREL Interrupt Ctrl. Register
CSP=io
CSP.address=0xfe08
CSP.comment=CPU Code Segment Pointer Register (read only)
DP0L=io
DP0L.address=0xf100
DP0L.comment=P0L Direction Control Register
DP0H=io
DP0H.address=0xf102
DP0H.comment=P0H Direction Control Register
DP1L=io
DP1L.address=0xf104
DP1L.comment=P1L Direction Control Register
DP1H=io
DP1H.address=0xf106
DP1H.comment=P1H Direction Control Register
DP2=io
DP2.address=0xffc2
DP2.comment=Port 2 Direction Control Register
ASC0_TIR=io
ASC0_TIR.address=0xffc6
ASC0_TIR.comment=ASC0_TIR
DP4=io
DP4.address=0xffca
DP4.comment=Port 4 Direction Control Register
DP6=io
DP6.address=0xffce
DP6.comment=Port 6 Direction Control Register
DP7=io
DP7.address=0xffd2
DP7.comment=Port 7 Direction Control Register
DP8=io
DP8.address=0xffd6
DP8.comment=Port 8 Direction Control Register
DPP0=io
DPP0.address=0xfe00
DPP0.comment=CPU Data Page Pointer 0 Reg. (10 bits)
DPP1=io
DPP1.address=0xfe02
DPP1.comment=CPU Data Page Pointer 1 Reg. (10 bits)
DPP2=io
DPP2.address=0xfe04
DPP2.comment=CPU Data Page Pointer 2 Reg. (10 bits)
DPP3=io
DPP3.address=0xfe06
DPP3.comment=CPU Data Page Pointer 3 Reg. (10 bits)
EXICON=io
EXICON.address=0xf1c0
EXICON.comment=External Interrupt Control Register
MDC=io
MDC.address=0xff0e
MDC.comment=Multiply Divide Control Register
MDH=io
MDH.address=0xfe0c
MDH.comment=Multiply Divide Register – High Word
MDL=io
MDL.address=0xfe0e
MDL.comment=Multiply Divide Register – Low Word
ODP2=io
ODP2.address=0xf1c2
ODP2.comment=Port 2 Open Drain Control Register
ODP3=io
ODP3.address=0xf1c6
ODP3.comment=Port 3 Open Drain Control Register
ODP6=io
ODP6.address=0xf1ce
ODP6.comment=Port 6 Open Drain Control Register
ODP7=io
ODP7.address=0xf1d2
ODP7.comment=Port 7 Open Drain Control Register
ODP8=io
ODP8.address=0xf1d6
ODP8.comment=Port 8 Open Drain Control Register
ONES=io
ONES.address=0xff1e
ONES.comment=Constant Value 1’s Register (read only)
P0H=io
P0H.address=0xff02
P0H.comment=Port 0 High Reg. (Upper half of PORT0)
P0L=io
P0L.address=0xff00
P0L.comment=Port 0 Low Reg. (Lower half of PORT0)
P1H=io
P1H.address=0xff06
P1H.comment=Port 1 High Reg. (Upper half of PORT1)
P1L=io
P1L.address=0xff04
P1L.comment=Port 1 Low Reg. (Lower half of PORT1)
P2=io
P2.address=0xffc0
P2.comment=Port 2 Register
P3=io
P3.address=0xffc4
P3.comment=Port 3 Register
P4=io
P4.address=0xffc8
P4.comment=Port 4 Register (8 bits)
P5=io
P5.address=0xffa2
P5.comment=Port 5 Register (read only)
P5DIDIS=io
P5DIDIS.address=0xffa4
P5DIDIS.comment=Port 5 Digital Input Disable Register
S1TBUF=io
S1TBUF.address=0xfeb8
S1TBUF.comment=Serial Channel 1 Transmit Buffer Register
S1RBUF=io
S1RBUF.address=0xfeba
S1RBUF.comment=Serial Channel 1 Receive Buffer Register
P6=io
P6.address=0xffcc
P6.comment=Port 6 Register (8 bits)
P7=io
P7.address=0xffd0
P7.comment=Port 7 Register (8 bits)
P8=io
P8.address=0xffd4
P8.comment=Port 8 Register (8 bits)
PECC0=io
PECC0.address=0xfec0
PECC0.comment=PEC Channel 0 Control Register
PECC1=io
PECC1.address=0xfec2
PECC1.comment=PEC Channel 1 Control Register
PECC2=io
PECC2.address=0xfec4
PECC2.comment=PEC Channel 2 Control Register
PECC3=io
PECC3.address=0xfec6
PECC3.comment=PEC Channel 3 Control Register
PECC4=io
PECC4.address=0xfec8
PECC4.comment=PEC Channel 4 Control Register
PECC5=io
PECC5.address=0xfeca
PECC5.comment=PEC Channel 5 Control Register
PECC6=io
PECC6.address=0xfecc
PECC6.comment=PEC Channel 6 Control Register
PECC7=io
PECC7.address=0xfece
PECC7.comment=PEC Channel 7 Control Register
PICON=io
PICON.address=0xf1c4
PICON.comment=Port Input Threshold Control Register
PDCR=io
PDCR.address=0xf0aa
PDCR.comment=Pin Driver Control Register
PP0=io
PP0.address=0xf038
PP0.comment=PWM Module Period Register 0
PP1=io
PP1.address=0xf03a
PP1.comment=PWM Module Period Register 1
PP2=io
PP2.address=0xf03c
PP2.comment=PWM Module Period Register 2
PP3=io
PP3.address=0xf03e
PP3.comment=PWM Module Period Register 3
PSW=io
PSW.address=0xff10
PSW.comment=CPU Program Status Word
PT0=io
PT0.address=0xf030
PT0.comment=PWM Module Up/Down Counter 0
PT1=io
PT1.address=0xf032
PT1.comment=PWM Module Up/Down Counter 1
PT2=io
PT2.address=0xf034
PT2.comment=PWM Module Up/Down Counter 2
PT3=io
PT3.address=0xf036
PT3.comment=PWM Module Up/Down Counter 3
PW0=io
PW0.address=0xfe30
PW0.comment=PWM Module Pulse Width Register 0
PW1=io
PW1.address=0xfe32
PW1.comment=PWM Module Pulse Width Register 1
PW2=io
PW2.address=0xfe34
PW2.comment=PWM Module Pulse Width Register 2
PW3=io
PW3.address=0xfe36
PW3.comment=PWM Module Pulse Width Register 3
PWMCON0=io
PWMCON0.address=0xff30
PWMCON0.comment=PWM Module Control Register 0
PWMCON1=io
PWMCON1.address=0xff32
PWMCON1.comment=PWM Module Control Register 1
PWMIC=io
PWMIC.address=0xf17e
PWMIC.comment=PWM Module Interrupt Control Register
RP0H=io
RP0H.address=0xf108
RP0H.comment=System Start-up Config. Reg. (Rd. only)
S0BG=io
S0BG.address=0xfeb4
S0BG.comment=Serial Channel 0 Baudrate Generator Reload Register
S0CON=io
S0CON.address=0xffb0
S0CON.comment=Serial Channel 0 Control Register
S0EIC=io
S0EIC.address=0xff70
S0EIC.comment=Serial Chan. 0 Error Interrupt Ctrl. Reg.
S0RBUF=io
S0RBUF.address=0xfeb2
S0RBUF.comment=Serial Channel 0 Receive Buffer Reg. (read only)
S0RIC=io
S0RIC.address=0xff6e
S0RIC.comment=Serial Channel 0 Receive Interrupt Control Register
S0TBIC=io
S0TBIC.address=0xf19c
S0TBIC.comment=Serial Channel 0 Transmit Buffer Interrupt Control Register
S0TBUF=io
S0TBUF.address=0xfeb0
S0TBUF.comment=Serial Channel 0 Transmit Buffer Reg. (write only)
S0TIC=io
S0TIC.address=0xff6c
S0TIC.comment=Serial Channel 0 Transmit Interrupt Control Register
S0RIC=io
S0RIC.address=0xff6e
S0RIC.comment=Serial Channel 0 Receive Interrupt Control Register
SP=io
SP.address=0xfe12
SP.comment=CPU System Stack Pointer Register
SSCBR=io
SSCBR.address=0xf0b4
SSCBR.comment=SSC Baudrate Register
SSCCON=io
SSCCON.address=0xffb2
SSCCON.comment=SSC Control Register
SSCEIC=io
SSCEIC.address=0xff76
SSCEIC.comment=SSC Error Interrupt Control Register
SSCRB=io
SSCRB.address=0xf0b2
SSCRB.comment=SSC Receive Buffer
SSCRIC=io
SSCRIC.address=0xff74
SSCRIC.comment=SSC Receive Interrupt Control Register
SSCTB=io
SSCTB.address=0xf0b0
SSCTB.comment=SSC Transmit Buffer
SSCTIC=io
SSCTIC.address=0xff72
SSCTIC.comment=SSC Transmit Interrupt Control Register
STKOV=io
STKOV.address=0xfe14
STKOV.comment=CPU Stack Overflow Pointer Register
STKUN=io
STKUN.address=0xfe16
STKUN.comment=CPU Stack Underflow Pointer Register
SYSCON=io
SYSCON.address=0xff12
SYSCON.comment=CPU System Configuration Register
T0=io
T0.address=0xfe50
T0.comment=CAPCOM Timer 0 Register
T01CON=io
T01CON.address=0xff50
T01CON.comment=CAPCOM Timer 0 and Timer 1 Ctrl. Reg.
T0IC=io
T0IC.address=0xff9c
T0IC.comment=CAPCOM Timer 0 Interrupt Ctrl. Reg.
T0REL=io
T0REL.address=0xfe54
T0REL.comment=CAPCOM Timer 0 Reload Register
T1=io
T1.address=0xfe52
T1.comment=CAPCOM Timer 1 Register
T1IC=io
T1IC.address=0xff9e
T1IC.comment=CAPCOM Timer 1 Interrupt Ctrl. Reg.
T1REL=io
T1REL.address=0xfe56
T1REL.comment=CAPCOM Timer 1 Reload Register
T2=io
T2.address=0xfe40
T2.comment=GPT1 Timer 2 Register
T2CON=io
T2CON.address=0xff40
T2CON.comment=GPT1 Timer 2 Control Register
T2IC=io
T2IC.address=0xff60
T2IC.comment=GPT1 Timer 2 Interrupt Control Register
T3=io
T3.address=0xfe42
T3.comment=GPT1 Timer 3 Register
T3CON=io
T3CON.address=0xff42
T3CON.comment=GPT1 Timer 3 Control Register
T3IC=io
T3IC.address=0xff62
T3IC.comment=GPT1 Timer 3 Interrupt Control Register
T4=io
T4.address=0xfe44
T4.comment=GPT1 Timer 4 Register
T4CON=io
T4CON.address=0xff44
T4CON.comment=GPT1 Timer 4 Control Register
T4IC=io
T4IC.address=0xff64
T4IC.comment=GPT1 Timer 4 Interrupt Control Register
T5=io
T5.address=0xfe46
T5.comment=GPT2 Timer 5 Register
T5CON=io
T5CON.address=0xff46
T5CON.comment=GPT2 Timer 5 Control Register
T5IC=io
T5IC.address=0xff66
T5IC.comment=GPT2 Timer 5 Interrupt Control Register
T6=io
T6.address=0xfe48
T6.comment=GPT2 Timer 6 Register
T6CON=io
T6CON.address=0xff48
T6CON.comment=GPT2 Timer 6 Control Register
T6IC=io
T6IC.address=0xff68
T6IC.comment=GPT2 Timer 6 Interrupt Control Register
T7=io
T7.address=0xf050
T7.comment=CAPCOM Timer 7 Register
T78CON=io
T78CON.address=0xff20
T78CON.comment=CAPCOM Timer 7 and 8 Ctrl. Reg.
T7IC=io
T7IC.address=0xf17a
T7IC.comment=CAPCOM Timer 7 Interrupt Ctrl. Reg.
T7REL=io
T7REL.address=0xf054
T7REL.comment=CAPCOM Timer 7 Reload Register
T8=io
T8.address=0xf052
T8.comment=CAPCOM Timer 8 Register
T8IC=io
T8IC.address=0xf17c
T8IC.comment=CAPCOM Timer 8 Interrupt Ctrl. Reg.
T8REL=io
T8REL.address=0xf056
T8REL.comment=CAPCOM Timer 8 Reload Register
ALTSEL0P3=io
ALTSEL0P3.address=0xf126
ALTSEL0P3.comment=Alternate I/O Source Port 3 Selection

TFR=io
TFR.address=0xffac
TFR.comment=Trap Flag Register
WDT=io
WDT.address=0xfeae
WDT.comment=Watchdog Timer Register (read only)
WDTCON=io
WDTCON.address=0xffae
WDTCON.comment=Watchdog Timer Control Register
XP0IC=io
XP0IC.address=0xf186
XP0IC.comment=CAN1 Module Interrupt Control Register
XP1IC=io
XP1IC.address=0xf18e
XP1IC.comment=Unassigned Interrupt Control Register
XP2IC=io
XP2IC.address=0xf196
XP2IC.comment=Unassigned Interrupt Control Register
XP3IC=io
XP3IC.address=0xf19e
XP3IC.comment=PLL/OWD Interrupt Control Register
ZEROS=io
ZEROS.address=0xff1c
ZEROS.comment=Constant Value 0’s Register (read only)
SYSCON1=io
SYSCON1.address=0xf1dc
SYSCON1.comment=Constant Value 0’s Register (read only)
SYSCON3=io
SYSCON3.address=0xf1d4
SYSCON3.comment=Constant Value 0’s Register (read only)
FOCON=io
FOCON.address=0xffaa
FOCON.comment=Frequency Output Control Register
PLLCON=io
PLLCON.address=0xf1d0
PLLCON.comment=PLL Control Register
