-:2: 16-bit addresses not supported in 64-bit mode
-:4: 16-bit addresses not supported in 64-bit mode
-:5: invalid effective address
-:6: invalid effective address
-:7: cannot use A/B/C/DH with instruction needing REX
