d "aaa" 37
d "aas" 3F
d "adc [eax], al" 1000
d "adc [eax], eax" 1100
d "adc al, 0x0" 1400
d "adc al, [eax]" 1200
d "adc eax, [eax]" 1300
d "add [eax], al" 0000
d "add [eax], eax" 0100
d "add al, 0x0" 0400
d "add al, [eax]" 0200
d "add byte [eax], 0x0" 800000
d "add byte [eax], 0x0" 820000
d "add dword [eax], 0x0" 810000000000
d "add dword [eax], 0x0" 830000
d "add eax, [eax]" 0300
d "and [eax], al" 2000
d "and [eax], eax" 2100
d "and al, 0x0" 2400
d "and al, [eax]" 2200
d "and eax, [eax]" 2300
d "arpl [eax], ax" 6300
d "bound eax, [eax]" 6200
d "bsf eax, [eax]" 0fbc00
d "bsr eax, [eax]" 0fbd00
d "bswap eax" 0fc8
d "bswap ebp" 0fcd
d "bswap ebx" 0fcb
d "bswap ecx" 0fc9
d "bswap edi" 0fcf
d "bswap edx" 0fca
d "bswap esi" 0fce
d "bswap esp" 0fcc
d "bt [eax], eax" 0fa300
d "btc [eax], eax" 0fbb00
d "btr [eax], eax" 0fb300
d "bts [eax], eax" 0fab00
d "cbw" 6698
d "cdq" 99
d "clc" F8
d "cld" FC
d "clflush [eax]" 0fae38
d "clgi" 0f01dd
d "cli" FA
d "clts" 0f06
d "cmc" F5
d "cmova eax, [eax]" 0f4700
d "cmovae eax, [eax]" 0f4300
d "cmovb eax, [eax]" 0f4200
d "cmovbe eax, [eax]" 0f4600
d "cmove eax, [eax]" 0f4400
d "cmovg eax, [eax]" 0f4f00
d "cmovge eax, [eax]" 0f4d00
d "cmovl eax, [eax]" 0f4c00
d "cmovle eax, [eax]" 0f4e00
d "cmovne eax, [eax]" 0f4500
d "cmovno eax, [eax]" 0f4100
d "cmovnp eax, [eax]" 0f4b00
d "cmovns eax, [eax]" 0f4900
d "cmovo eax, [eax]" 0f4000
d "cmovp eax, [eax]" 0f4a00
d "cmovs eax, [eax]" 0f4800
d "cmp [eax], al" 3800
d "cmp [eax], eax" 3900
d "cmp al, 0x0" 3c00
d "cmp al, [eax]" 3a00
d "cmp eax, [eax]" 3b00
d "cmpsb" a6
d "cmpsd" a7
d "cmpxchg [eax], al" 0fb000
d "cmpxchg [eax], eax" 0fb100
d "cpuid" 0fa2
d "crc32 eax, [eax]" f20f38f100
d "crc32 eax, byte [eax]" f20f38f000
d "cwd" 6699
d "cwde" 98
d "daa" 27
d "das" 2F
d "dec byte [eax]" fe08
d "dec dword [eax]" ff08
d "dec eax" 48
d "dec ebp" 4d
d "dec ebx" 4b
d "dec ecx" 49
d "dec edi" 4f
d "dec edx" 4a
d "dec esi" 4e
d "dec esp" 4c
d "div byte [eax]" f630
d "emms" 0f77
d "femms" 0f0e
d "fxrstor [eax]" 0fae08
d "fxsave [eax]" 0fae00
d "getsec" 0f37
d "hlt" F4
d "idiv byte [eax]" f638
d "imul byte [eax]" f628
d "in al, 0x0" E400
d "in al, dx" ec
d "in eax, 0x0" E500
d "in eax, dx" ed
d "inc byte [eax]" fe00
d "inc dword [eax]" ff00
d "inc eax" 40
d "inc ebp" 45
d "inc ebx" 43
d "inc ecx" 41
d "inc edi" 47
d "inc edx" 42
d "inc esi" 46
d "inc esp" 44
d "insb" 6c
d "insd" 6d
d "int 0x1" CD01
d "int 0x3" CD03
d "int1" F1
d "int3" CC
d "into" CE
d "invd" 0f08
d "invlpg [eax]" 0f0138
d "invlpga" 0f01df
d "iretd" CF
d "iretw" 66CF
d "ja 0x2" 7700
d "ja 0x6" 0f8700000000
d "jae 0x2" 7300
d "jae 0x6" 0f8300000000
d "jb 0x2" 7200
d "jb 0x6" 0f8200000000
d "jbe 0x2" 7600
d "jbe 0x6" 0f8600000000
d "je 0x2" 7400
d "je 0x6" 0f8400000000
d "jg 0x2" 7f00
d "jg 0x6" 0f8f00000000
d "jge 0x2" 7d00
d "jge 0x6" 0f8d00000000
d "jl 0x2" 7c00
d "jl 0x6" 0f8c00000000
d "jle 0x2" 7e00
d "jle 0x6" 0f8e00000000
d "jne 0x2" 7500
d "jne 0x6" 0f8500000000
d "jno 0x2" 7100
d "jno 0x6" 0f8100000000
d "jnp 0x2" 7b00
d "jnp 0x6" 0f8b00000000
d "jns 0x2" 7900
d "jns 0x6" 0f8900000000
d "jo 0x2" 7000
d "jo 0x6" 0f8000000000
d "jp 0x2" 7a00
d "jp 0x6" 0f8a00000000
d "js 0x2" 7800
d "js 0x6" 0f8800000000
d "lahf" 9F
d "lar eax, word [eax]" 0f0200
d "ldmxcsr dword [eax]" 0fae10
d "lds eax, [eax]" c500
d "lea eax, [eax]" 8d00
d "leave" C9
d "les eax, [eax]" c400
d "lfence" 0faee8
d "lgdt [eax]" 0f0110
d "lidt [eax]" 0f0118
d "lldt ax" 0f00d0
d "lldt word [eax]" 0f0010
d "lmsw ax" 0f01f0
d "lmsw word [eax]" 0f0130
d "lodsb" ac
d "lodsd" ad
d "lsl eax, word [eax]" 0f0300
d "ltr ax" 0f00d8
d "ltr word [eax]" 0f0018
d "mfence" 0faef0
d "monitor" 0f01c8
d "mov [0x0], al" a200000000
d "mov [0x0], eax" a300000000
d "mov [cs:eax], eax" 2e8900
d "mov [ds:eax], eax" 3e8900
d "mov [eax], al" 8800
d "mov [eax], eax" 8900
d "mov [eax], es" 8c00
d "mov [es:eax], eax" 268900
d "mov [fs:eax], eax" 648900
d "mov [gs:eax], eax" 658900
d "mov [ss:eax], eax" 368900
d "mov ah, 0x0" B400
d "mov ah, 0x0" b400
d "mov al, 0x0" B000
d "mov al, 0x0" b000
d "mov al, [0x0]" a000000000
d "mov al, [eax]" 8a00
d "mov bh, 0x0" B700
d "mov bh, 0x0" b700
d "mov bl, 0x0" B300
d "mov bl, 0x0" b300
d "mov byte [eax], 0x0" c60000
d "mov ch, 0x0" B500
d "mov ch, 0x0" b500
d "mov cl, 0x0" B100
d "mov cl, 0x0" b100
d "mov dh, 0x0" B600
d "mov dh, 0x0" b600
d "mov dl, 0x0" B200
d "mov dl, 0x0" b200
d "mov dword [eax], 0x0" c70000000000
d "mov eax, 0x0" b800000000
d "mov eax, [0x0]" a100000000
d "mov eax, [eax]" 8b00
d "mov ebp, 0x0" bd00000000
d "mov ebx, 0x0" bb00000000
d "mov ecx, 0x0" b900000000
d "mov edi, 0x0" bf00000000
d "mov edx, 0x0" ba00000000
d "mov es, [eax]" 8e00
d "mov esi, 0x0" be00000000
d "mov esp, 0x0" bc00000000
d "movntdq [eax], xmm0" 660fe700
d "movntq [eax], mm0" 0fe700
d "movsb" a4
d "movsd" a5
d "mul byte [eax]" f620
d "mwait" 0f01c9
d "neg byte [eax]" f618
d "nop" 90
d "not byte [eax]" f610
d "o16 seta byte [eax]" 660f9700
d "o16 setae byte [eax]" 660f9300
d "o16 setb byte [eax]" 660f9200
d "o16 setbe byte [eax]" 660f9600
d "o16 sete byte [eax]" 660f9400
d "o16 setg byte [eax]" 660f9f00
d "o16 setge byte [eax]" 660f9d00
d "o16 setl byte [eax]" 660f9c00
d "o16 setle byte [eax]" 660f9e00
d "o16 setne byte [eax]" 660f9500
d "o16 setno byte [eax]" 660f9100
d "o16 setnp byte [eax]" 660f9b00
d "o16 setns byte [eax]" 660f9900
d "o16 seto byte [eax]" 660f9000
d "o16 setp byte [eax]" 660f9a00
d "o16 sets byte [eax]" 660f9800
d "or [eax], al" 0800
d "or [eax], eax" 0900
d "or al, 0x0" 0c00
d "or eax, [eax]" 0b00
d "out 0x0, al" E600
d "out 0x0, eax" E700
d "out dx, al" ee
d "out dx, eax" ef
d "outsb" 6e
d "outsd" 6f
d "paddsb mm0, [eax]" 0fec00
d "paddsw mm0, [eax]" 0fed00
d "paddusb mm0, [eax]" 0fdc00
d "paddusw mm0, [eax]" 0fdd00
d "pand mm0, [eax]" 0fdb00
d "pandn mm0, [eax]" 0fdf00
d "pause" f390
d "pavgb mm0, [eax]" 0fe000
d "pavgw mm0, [eax]" 0fe300
d "pmaxsw mm0, [eax]" 0fee00
d "pmaxub mm0, [eax]" 0fde00
d "pminsw mm0, [eax]" 0fea00
d "pminub mm0, [eax]" 0fda00
d "pop ds" 1F
d "pop dword [eax]" 8f00
d "pop eax" 58
d "pop ebp" 5D
d "pop ebx" 5B
d "pop ecx" 59
d "pop edi" 5F
d "pop edx" 5A
d "pop es" 07
d "pop esi" 5E
d "pop esp" 5C
d "pop fs" 0fa1
d "pop gs" 0fa9
d "pop ss" 17
d "popa" 6661
d "popad" 61
d "popfd" 9D
d "por mm0, [eax]" 0feb00
d "prefetch [eax]" 0f0d00
d "prefetchnta [eax]" 0f1800
d "prefetcht0 [eax]" 0f1808
d "prefetcht1 [eax]" 0f1810
d "prefetcht2 [eax]" 0f1818
d "psrad mm0, [eax]" 0fe200
d "psrad xmm0, [eax]" 660fe200
d "psraw mm0, [eax]" 0fe100
d "psraw xmm0, [eax]" 660fe100
d "psubsb mm0, [eax]" 0fe800
d "psubsw mm0, [eax]" 0fe900
d "psubusb mm0, [eax]" 0fd800
d "psubusw mm0, [eax]" 0fd900
d "push 0x0" 6a00
d "push cs" 0E
d "push ds" 1E
d "push dword [eax]" ff30
d "push eax" 50
d "push ebp" 55
d "push ebx" 53
d "push ecx" 51
d "push edi" 57
d "push edx" 52
d "push es" 06
d "push esi" 56
d "push esp" 54
d "push fs" 0fa0
d "push gs" 0fa8
d "push ss" 16
d "pushad" 60
d "pushfd" 9C
d "pxor mm0, [eax]" 0fef00
d "rdmsr" 0f32
d "rdpmc" 0f33
d "rdtsc" 0f31
d "rdtscp" 0f01f9
d "ret" C3
d "retf 0x0" CA0000
d "retf" CB
d "rol byte [eax], 0x0" c00000
d "rol byte [eax], cl" d200
d "rol dword [eax], 0x0" c10000
d "rol dword [eax], cl" d300
d "rsm" 0faa
d "sahf" 9E
d "salc" D6
d "sbb [eax], al" 1800
d "sbb [eax], eax" 1900
d "sbb al, 0x0" 1c00
d "sbb al, [eax]" 1a00
d "sbb eax, [eax]" 1b00
d "scasb" ae
d "scasd" af
d "sfence" 0faef8
d "sgdt [eax]" 0f0100
d "shld [eax], eax, 0x0" 0fa40000
d "shld [eax], eax, cl" 0fa500
d "shrd [eax], eax, 0x0" 0fac0000
d "shrd [eax], eax, cl" 0fad00
d "shufps xmm0, [eax], 0x0" 0fc60000
d "sidt [eax]" 0f0108
d "skinit" 0f01de
d "sldt word [eax]" 0f0000
d "smsw ax" 660f01e0
d "smsw eax" 0f01e0
d "smsw word [eax]" 0f0120
d "stc" F9
d "std" FD
d "stgi" 0f01dc
d "sti" FB
d "stmxcsr dword [eax]" 0fae18
d "stosb" aa
d "stosd" ab
d "str word [eax]" 0f0008
d "sub [eax], al" 2800
d "sub [eax], eax" 2900
d "sub al, 0x0" 2c00
d "sub al, [eax]" 2a00
d "sub eax, [eax]" 2b00
d "syscall" 0f05
d "sysenter" 0f34
d "sysexit" 0f35
d "sysret" 0f07
d "test [eax], al" 8400
d "test [eax], eax" 8500
d "test al, 0x0" A800
d "test al, 0x0" a800
d "test byte [eax], 0x0" f60000
d "test byte [eax], 0x0" f60800
d "test dword [eax], 0x0" f70000000000
d "test dword [eax], 0x0" f70000000000
d "test dword [eax], 0x0" f70800000000
d "test eax, 0x0" a900000000
d "ud2" 0f0b
d "verr ax" 0f00e0
d "verr word [eax]" 0f0020
d "verw ax" 0f00e8
d "verw word [eax]" 0f0028
d "vmload" 0f01da
d "vmmcall" 0f01d9
d "vmrun" 0f01d8
d "vmsave" 0f01db
d "vzeroall" c5fc77
d "vzeroupper" c5f877
d "wbinvd" 0f09
d "wrmsr" 0f30
d "xchg [eax], al" 8600
d "xchg [eax], eax" 8700
d "xchg ebp, eax" 95
d "xchg ebx, eax" 93
d "xchg ecx, eax" 91
d "xchg edi, eax" 97
d "xchg edx, eax" 92
d "xchg esi, eax" 96
d "xchg esp, eax" 94
d "xgetbv" 0f01d0
d "xlatb" D7
d "xor [eax], al" 3000
d "xor [eax], eax" 3100
d "xor al, 0x0" 3400
d "xor al, [eax]" 3200
d "xor eax, [eax]" 3300
d "xrstor [eax]" 0fae28
d "xsave [eax]" 0fae20
d "xsetbv" 0f01d1
dB "cmpxchg8b [eax]" 0fc7c0
dB "lock cmpxchg8b [eax]" f00fc7c0
dB "mov cr0, eax" 0f22
dB "mov dr0, eax" 0f23
dB "mov eax, cr0" 0f20
dB "mov eax, dr0" 0f21
dB "vmcall" 0f01c1
dB "vmclear [eax]" 660fc730
dB "vmlaunch" 0f01c2
dB "vmptrld [eax]" 0fc730
dB "vmptrst [eax]" 0fc738
dB "vmresume" 0f01c3
dB "vmxoff" 0f01c4
dB "vmxon [eax]" f30fc730
d "vaddpd ymm0, ymm0, ymm0" c5fd58c0
d "aesdec xmm0, xmm0" 660f38dec0
d "aesdeclast xmm0, xmm0" 660f38dfc0
d "aesenc xmm0, xmm0" 660f38dcc0
d "aesenclast xmm0, xmm0" 660f38ddc0
d "aesimc xmm0, xmm0" 660f38dbc0
d "aeskeygenassist xmm0, xmm0, 0x0" 660f3adfc000
d "vaesdec xmm0, xmm0, xmm0" c4e279dec0
d "vaesdeclast xmm0, xmm0" c4e279dfc0
d "vaesenc xmm0, xmm0" c4e279dcc0
d "vaesenclast xmm0, xmm0, xmm0" c4e279ddc0
d "vaesimc xmm0, xmm0" c4e279dbc0
d "vaeskeygenassist xmm0, xmm0, 0x0" c4e379dfc000
d "vextractf128 xmm0, ymm0, 0x0" c4e37d19c000
dB "vbroadcastf128 ymm0, [0x0]" c4e27d1a0500000000
d "vbroadcastsd ymm0, qword [0x0]" c4e27d190500000000
d "vinsertf128 ymm0, ymm0, xmm0, 0x0" c4e37d18c000
d "vperm2f128 ymm0, ymm0, ymm0, 0x0" c4e37d06c000
d "vpermilpd ymm0, ymm0, [0x0]" c4e27d0d0500000000
d "vpermilps ymm0, ymm0, [0x0]" c4e27d0c0500000000
dB "vfmadd132pd xmm0, xmm0, xmm0" c4e2f998c0
dB "vfmadd213pd xmm0, xmm0, xmm0" c4e2f9a8c0
dB "vfmadd231pd xmm0, xmm0, xmm0" c4e2f9b8c0
d "o16 mulsd xmm7, xmm7" 66f3f20f59ff
dB "mulss xmm7, xmm7" 66f2f0f59ff0
d "mulpd xmm7, xmm7" 660f59ff
d "o16 mulsd xmm7, xmm7" f2660f59ff
d "mulps xmm7, xmm7" 0f59ff
d "mpsadbw xmm0, xmm0, 0x0" 660f3a42c000
d "pcmpestrm xmm0, xmm0, 0x0" 660f3a60c000
d "pcmpestri xmm0, xmm0, 0x0" 660f3a61c000
d "pcmpistrm xmm0, xmm0, 0x0" 660f3a62c000
d "pcmpistri xmm0, xmm0, 0x0" 660f3a63c000
d "roundps xmm0, xmm0, 0x0" 660f3a08c000
d "roundpd xmm0, xmm0, 0x0" 660f3a09c000
d "roundss xmm0, xmm0, 0x0" 660f3a0ac000
d "roundsd xmm0, xmm0, 0x0" 660f3a0bc000
d "blendps xmm0, xmm0, 0x0" 660f3a0cc000
d "blendpd xmm0, xmm0, 0x0" 660f3a0dc000
d "pblendw xmm0, xmm0, 0x0" 660f3a0ec000
d "palignr xmm0, xmm0, 0x0" 660f3a0fc000
d "palignr mm0, mm0, 0x0" 0f3a0fc000
d "psrlw mm0, 0x0" 0f71d000
d "psrld mm0, 0x0" 0f72d000
d "psrlq mm0, 0x0" 0f73d000
d "psllw mm0, 0x0" 0f71f000
d "psllq mm0, 0x0" 0f73f000
d "psrlw xmm0, 0x0" 660f71d000
d "psrld xmm0, 0x0" 660f72d000
d "psrlq xmm0, 0x0" 660f73d000
d "psllw xmm0, 0x0" 660f71f000
d "pslld xmm0, 0x0" 660f72f000
d "psllq xmm0, 0x0" 660f73f000
d "psrldq xmm0, 0x0" 660f73d800
d "pslldq xmm0, 0x0" 660f73f800
d "sqrtps xmm0, [eax]" 0f5100
d "sqrtpd xmm0, [eax]" 660f5100
d "sqrtsd xmm0, [eax]" f20f5100
d "sqrtss xmm0, [eax]" f30f5100
d "rsqrtps xmm0, [eax]" 0f5200
d "rsqrtss xmm0, [eax]" f30f5200
d "rcpps xmm0, [eax]" 0f5300
d "rcpss xmm0, [eax]" f30f5300
d "andps xmm0, [eax]" 0f5400
d "andnps xmm0, [eax]" 0f5500
d "andpd xmm0, [eax]" 660f5400
d "andnpd xmm0, [eax]" 660f5500
d "orps xmm0, [eax]" 0f5600
d "xorps xmm0, [eax]" 0f5700
d "orpd xmm0, [eax]" 660f5600
d "xorpd xmm0, [eax]" 660f5700
d "addps xmm0, [eax]" 0f5800
d "subps xmm0, [eax]" 0f5c00
d "mulps xmm0, [eax]" 0f5900
d "divps xmm0, [eax]" 0f5e00
d "addpd xmm0, [eax]" 660f5800
d "subpd xmm0, [eax]" 660f5c00
d "mulpd xmm0, [eax]" 660f5900
d "divpd xmm0, [eax]" 660f5e00
d "minps xmm0, [eax]" 0f5d00
d "maxps xmm0, [eax]" 0f5f00
d "minpd xmm0, [eax]" 660f5d00
d "maxpd xmm0, [eax]" 660f5f00
d "minsd xmm0, qword [eax]" f20f5d00
d "maxsd xmm0, [eax]" f20f5f00
d "minss xmm0, dword [eax]" f30f5d00
d "maxss xmm0, [eax]" f30f5f00
d "punpcklbw mm0, [eax]" 0f6000
d "punpcklwd mm0, [eax]" 0f6100
d "punpckldq mm0, [eax]" 0f6200
d "punpcklbw xmm0, [eax]" 660f6000
d "punpcklwd xmm0, [eax]" 660f6100
d "punpckldq xmm0, [eax]" 660f6200
d "packsswb mm0, [eax]" 0f6300
d "packuswb mm0, [eax]" 0f6700
d "packsswb xmm0, [eax]" 660f6300
d "packuswb xmm0, [eax]" 660f6700
d "pcmpgtb mm0, [eax]" 0f6400
d "pcmpgtw mm0, [eax]" 0f6500
d "pcmpgtd mm0, [eax]" 0f6600
d "pcmpgtb xmm0, [eax]" 660f6400
d "pcmpgtw xmm0, [eax]" 660f6500
d "pcmpgtd xmm0, [eax]" 660f6600
d "punpckhbw mm0, [eax]" 0f6800
d "punpckhwd mm0, [eax]" 0f6900
d "punpckhdq mm0, [eax]" 0f6a00
d "punpckhbw xmm0, [eax]" 660f6800
d "punpckhwd xmm0, [eax]" 660f6900
d "punpckhdq xmm0, [eax]" 660f6a00
d "packssdw mm0, [eax]" 0f6b00
d "packssdw xmm0, [eax]" 660f6b00
d "pshufb mm0, [eax]" 0f380000
d "pshufw mm0, [eax], 0x0" 0f700000
d "pshufb xmm0, [eax]" 660f380000
d "pshufd xmm0, [eax], 0x0" 660f700000
d "pshuflw xmm0, [eax], 0x0" f20f700000
d "pshufhw xmm0, [eax], 0x0" f30f700000
d "pcmpeqb mm0, [eax]" 0f7400
d "pcmpeqw mm0, [eax]" 0f7500
d "pcmpeqd mm0, [eax]" 0f7600
d "pcmpeqb xmm0, [eax]" 660f7400
d "pcmpeqw xmm0, [eax]" 660f7500
d "pcmpeqd xmm0, [eax]" 660f7600
d "movd mm0, dword [eax]" 0f6e00
d "movq mm0, [eax]" 0f6f00
d "movd dword [eax], mm0" 0f7e00
d "movq [eax], mm0" 0f7f00
d "movd xmm0, dword [eax]" 660f6e00
d "movdqa xmm0, [eax]" 660f6f00
d "movd dword [eax], xmm0" 660f7e00
d "movdqa [eax], xmm0" 660f7f00
d "movdqu xmm0, [eax]" f30f6f00
d "movq xmm0, [eax]" f30f7e00
d "movdqu [eax], xmm0" f30f7f00
d "pmovsxbw xmm0, xmm0" 660f3820c0
d "pmovsxbd xmm0, xmm0" 660f3821c0
d "pmovsxbq xmm0, xmm0" 660f3822c0
d "pmovsxwd xmm0, xmm0" 660f3823c0
d "pmovsxwq xmm0, xmm0" 660f3824c0
d "pmovsxdq xmm0, xmm0" 660f3825c0
d "pmovzxbw xmm0, xmm0" 660f3830c0
d "pmovzxbd xmm0, xmm0" 660f3831c0
d "pmovzxbq xmm0, xmm0" 660f3832c0
d "pmovzxwd xmm0, xmm0" 660f3833c0
d "pmovzxwq xmm0, xmm0" 660f3834c0
d "pmovzxdq xmm0, xmm0" 660f3835c0
d "pminsb xmm0, xmm0" 660f3838c0
d "pminsd xmm0, xmm0" 660f3839c0
d "pminuw xmm0, xmm0" 660f383ac0
d "pminud xmm0, xmm0" 660f383bc0
d "pmaxsb xmm0, xmm0" 660f383cc0
d "pmaxsd xmm0, xmm0" 660f383dc0
d "pmaxuw xmm0, xmm0" 660f383ec0
d "pmaxud xmm0, xmm0" 660f383fc0
d "psignb xmm0, xmm0" 660f3808c0
d "psignw xmm0, xmm0" 660f3809c0
d "psignd xmm0, xmm0" 660f380ac0
d "pmulhrsw xmm0, xmm0" 660f380bc0
d "pabsb xmm0, xmm0" 660f381cc0
d "pabsw xmm0, xmm0" 660f381dc0
d "pabsd xmm0, xmm0" 660f381ec0
d "pmuldq xmm0, xmm0" 660f3828c0
d "pcmpeqq xmm0, xmm0" 660f3829c0
d "movntdqa xmm0, [eax]" 660f382a00
d "packusdw xmm0, xmm0" 660f382bc0
d "extractps eax, xmm0, 0x0" 660f3a17c000
d "pinsrb xmm0, eax, 0x0" 660f3a20c000
dB "insertps xmm0, xmm0, 0x0" 660f3a21c000
d "dpps xmm0, xmm0, 0x0" 660f3a40c000
d "dppd xmm0, xmm0, 0x0" 660f3a41c000
d "pslld mm0, 0x0" 0f72f000
d "movups xmm0, [eax]" 0f1000
d "movups [eax], xmm0" 0f1100
d "unpcklps xmm0, [eax]" 0f1400
d "unpckhps xmm0, [eax]" 0f1500
d "movlps xmm0, [eax]" 0f1200
d "movlps [eax], xmm0" 0f1300
dB "movhlps xmm0, xmm0" 0f1200
dB "movlhps xmm0, xmm0" 0f1600
d "movhps xmm0, [eax]" 0f1600
d "movhps [eax], xmm0" 0f1700
d "movmskps eax, xmm0" 0f50c0
d "movmskpd eax, xmm0" 660f50c0
dB "vfmsubpd xmm0, xmm0, xmm0, xmm0" c4e3796dc000
dB "vfmsubps xmm0, xmm0, xmm0, xmm0" c4e3796cc000
dB "vfmsubsd xmm0, xmm0, xmm0, xmm0" c4e3796fc000
dB "vfmsubss xmm0, xmm0, xmm0, xmm0" c4e3796ec000
dB "vfnmaddpd xmm0, xmm0, xmm0, xmm0" c4e37979c000
dB "vfnmaddps xmm0, xmm0, xmm0, xmm0" c4e37978c000
dB "vfnmaddsd xmm0, xmm0, xmm0, xmm0" c4e3797bc000
dB "vfnmaddss xmm0, xmm0, xmm0, xmm0" c4e3797ac000
dB "vfnmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d79c000
dB "vfnmaddps ymm0, ymm0, ymm0, ymm0" c4e37d78c000
dB "vfnmsubpd xmm0, xmm0, xmm0, xmm0" c4e3797dc000
dB "vfnmsubps xmm0, xmm0, xmm0, xmm0" c4e3797cc000
dB "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000
dB "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000
dB "vfnmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d7dc000
dB "vfnmsubps ymm0, ymm0, ymm0, ymm0" c4e37d7cc000
dB "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000
dB "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000
d "movsd xmm0, qword [eax]" f20f1000
d "movsd [eax], xmm0" f20f1100
d "movddup xmm0, [eax]" f20f1200
d "cvtps2pd xmm0, [eax]" 0f5a00
d "cvtpd2ps xmm0, [eax]" 660f5a00
d "cvtsd2ss xmm0, [eax]" f20f5a00
d "cvtss2sd xmm0, [eax]" f30f5a00
d "cvtdq2ps xmm0, [eax]" 0f5b00
d "cvtps2dq xmm0, [eax]" 660f5b00
d "cvttps2dq xmm0, [eax]" f30f5b00
d "cvttpd2dq xmm0, [eax]" 660fe600
d "cvtpd2dq xmm0, [eax]" f20fe600
d "cvtdq2pd xmm0, [eax]" f30fe600
d "cvttps2pi mm0, oword [eax]" 0f2c00
d "cvttpd2pi mm0, oword [eax]" 660f2c00
d "cvttsd2si eax, qword [eax]" f20f2c00
d "cvttss2si eax, [eax]" f30f2c00
d "cvtpi2ps xmm0, qword [eax]" 0f2a00
d "cvtpi2pd xmm0, qword [eax]" 660f2a00
d "cvtsi2sd xmm0, dword [eax]" f20f2a00
d "cvtsi2ss xmm0, dword [eax]" f30f2a00
d "cvtps2pi mm0, [eax]" 0f2d00
d "cvtsd2si eax, qword [eax]" f20f2d00
d "cvtss2si eax, [eax]" f30f2d00
d "cvtpd2pi mm0, oword [eax]" 660f2d00
d "movaps xmm0, [eax]" 0f2800
d "movaps [eax], xmm0" 0f2900
d "movntps [eax], xmm0" 0f2b00
d "movntpd [eax], xmm0" 660f2b00
d "ucomiss xmm0, [eax]" 0f2e00
d "comiss xmm0, [eax]" 0f2f00
d "ucomisd xmm0, [eax]" 660f2e00
d "comisd xmm0, [eax]" 660f2f00
d "psubb mm0, [eax]" 0ff800
d "psubw mm0, [eax]" 0ff900
d "psubd mm0, [eax]" 0ffa00
d "psubq mm0, [eax]" 0ffb00
d "paddb mm0, [eax]" 0ffc00
d "paddw mm0, [eax]" 0ffd00
d "paddd mm0, [eax]" 0ffe00
d "psrlw mm0, [eax]" 0fd100
d "psrld mm0, [eax]" 0fd200
d "psrlq mm0, [eax]" 0fd300
d "psrlw xmm0, [eax]" 660fd100
d "psrld xmm0, [eax]" 660fd200
d "psrlq xmm0, [eax]" 660fd300
d "psllw mm0, [eax]" 0ff100
d "pslld mm0, [eax]" 0ff200
d "psllq mm0, [eax]" 0ff300
d "psllw xmm0, [eax]" 660ff100
d "pslld xmm0, [eax]" 660ff200
d "psllq xmm0, [eax]" 660ff300
d "pmullw mm0, [eax]" 0fd500
d "pmullw xmm0, [eax]" 660fd500
d "pmulhuw mm0, [eax]" 0fe400
d "pmulhuw xmm0, [eax]" 660fe400
d "pmulhw mm0, [eax]" 0fe500
d "pmulhw xmm0, [eax]" 660fe500
d "pmuludq mm0, [eax]" 0ff400
d "pmuludq xmm0, [eax]" 660ff400
d "pmaddwd mm0, [eax]" 0ff500
d "pmaddwd xmm0, [eax]" 660ff500
d "psadbw mm0, [eax]" 0ff600
d "psadbw xmm0, [eax]" 660ff600
d "psubusb xmm0, [eax]" 660fd800
d "psubusw xmm0, [eax]" 660fd900
d "pminub xmm0, [eax]" 660fda00
d "pmaxub xmm0, [eax]" 660fde00
d "pand xmm0, [eax]" 660fdb00
d "pandn xmm0, [eax]" 660fdf00
d "paddusb xmm0, [eax]" 660fdc00
d "paddusw xmm0, [eax]" 660fdd00
d "pavgb xmm0, [eax]" 660fe000
d "pavgw xmm0, [eax]" 660fe300
d "psubsb xmm0, [eax]" 660fe800
d "psubsw xmm0, [eax]" 660fe900
d "pminsw xmm0, [eax]" 660fea00
d "pmaxsw xmm0, [eax]" 660fee00
d "por xmm0, [eax]" 660feb00
d "paddsb xmm0, [eax]" 660fec00
d "paddsw xmm0, [eax]" 660fed00
d "pxor xmm0, [eax]" 660fef00
d "psubb xmm0, [eax]" 660ff800
d "psubw xmm0, [eax]" 660ff900
d "psubd xmm0, [eax]" 660ffa00
d "psubq xmm0, [eax]" 660ffb00
d "paddb xmm0, [eax]" 660ffc00
d "paddw xmm0, [eax]" 660ffd00
d "paddd xmm0, [eax]" 660ffe00
d "f2xm1" d9f0
d "fabs" d9e1
d "fadd dword [eax]" d800
d "fadd qword [eax]" dc00
d "fadd st0, st0" d8c0
d "faddp st0, st0" dec0
d "fbld tword [eax]" df20
d "fbstp tword [eax]" df30
d "fchs" d9e0
dB "fnclex" dbe2
d "fcmovb st0, st0" dac0
d "fcmovbe st0, st0" dad0
d "fcmove st0, st0" dac8
d "fcmovnb st0, st0" dbc0
d "fcmovnbe st0, st0" dbd0
d "fcmovne st0, st0" dbc8
d "fcmovnu st0, st0" dbd8
d "fcmovu st0, st0" dad8
d "fcom dword [eax]" d810
d "fcom qword [eax]" dc10
d "fcom st0, st0" d8d0
d "fcomi st0, st0" dbf0
d "fcomip st0, st0" dff0
d "fcomp dword [eax]" d818
d "fcomp qword [eax]" dc18
d "fcomp st0, st0" d8d8
d "fcompp" ded9
d "fcos" d9ff
d "fdecstp" d9f6
d "fdiv dword [eax]" d830
d "fdiv qword [eax]" dc30
d "fdiv st0, st0" d8f0
d "fdiv st0, st0" dcf8
d "fdivp st0, st0" def8
d "fdivr dword [eax]" d838
d "fdivr qword [eax]" dc38
d "fdivr st0, st0" d8f8
d "fdivr st0, st0" dcf0
d "fdivrp st0, st0" def0
d "fneni" dbe0
d "ffree st0" ddc0
d "ffreep st0" dfc0
d "fiadd dword [eax]" da00
d "fiadd word [eax]" de00
d "ficom dword [eax]" da10
d "ficom word [eax]" de10
d "ficomp dword [eax]" da18
d "ficomp word [eax]" de18
d "fidiv dword [eax]" da30
d "fidiv word [eax]" de30
d "fidivr dword [eax]" da38
d "fidivr word [eax]" de38
d "fild dword [eax]" db00
d "fild qword [eax]" df28
d "fild word [eax]" df00
d "fimul dword [eax]" da08
d "fimul word [eax]" de08
d "fincstp" d9f7
d "fninit" dbe3
d "fist dword [eax]" db10
d "fist word [eax]" df10
d "fistp dword [eax]" db18
d "fistp qword [eax]" df38
d "fistp word [eax]" df18
d "fisttp word [eax]" df08
d "fisub dword [eax]" da20
d "fisub word [eax]" de20
d "fisubr dword [eax]" da28
d "fisubr word [eax]" de28
d "fld dword [eax]" d900
d "fld qword [eax]" dd00
d "fld st0" d9c0
d "fld tword [eax]" db28
d "fld1" d9e8
d "fldcw word [eax]" d928
d "fldenv [eax]" d920
d "fldl2e" d9ea
d "fldl2t" d9e9
d "fldlg2" d9ec
d "fldln2" d9ed
d "fldpi" d9eb
d "fldz" d9ee
d "fmul dword [eax]" d808
d "fmul qword [eax]" dc08
d "fmul st0, st0" d8c8
d "fmul st0, st0" dcc8
d "fmulp st0, st0" dec8
d "fclex" dbe2
d "fndisi" dbe1
d "fnop" d9d0
d "fpatan" d9f3
d "fprem" d9f8
d "fprem1" d9f5
d "fptan" d9f2
d "frndint" d9fc
d "frstor [eax]" dd20
d "fnsave [eax]" dd30
d "fscale" d9fd
d "fnsetpm" dbe4
d "fsin" d9fe
d "fsincos" d9fb
d "fsqrt" d9fa
d "fst dword [eax]" d910
d "fst qword [eax]" dd10
d "fst st0" ddd0
d "fnstcw word [eax]" d938
d "fnstenv [eax]" d930
d "fstp dword [eax]" d918
d "fstp qword [eax]" dd18
d "fstp st0" ddd8
d "fstp tword [eax]" db38
d "fsub dword [eax]" d820
d "fsub qword [eax]" dc20
d "fsub st0, st0" d8e0
d "fsubp st0, st0" dee8
d "fsubr dword [eax]" d828
d "fsubr qword [eax]" dc28
d "fsubr st0, st0" d8e8
d "fsubrp st0, st0" dee0
d "ftst" d9e4
d "fucom st0" dde0
d "fucomi st0, st0" dbe8
d "fucomip st0, st0" dfe8
d "fucomp st0" dde8
d "fucompp" dae9
d "fxam" d9e5
d "fxch st0, st0" d9c8
d "fxtract" d9f4
d "fyl2x" d9f1
d "fyl2xp1" d9f9
d "wait" 9b
d "fstp1 st0" d9d8
d "fcom2 st0" dcd0
d "fcomp3 st0" dcd8
d "fxch4 st0" ddc8
d "fcomp5 st0" ded0
d "fxch7 st0" dfc8
d "fstp8 st0" dfd0
d "fstp9 st0" dfd8
d "not dword [eax]" f710
d "neg dword [eax]" f718
d "mul dword [eax]" f720
d "imul dword [eax]" f728
d "div dword [eax]" f730
d "idiv dword [eax]" f738
d "rol byte [eax], 0x0" c00000
d "ror byte [eax], 0x0" c00800
d "rcl byte [eax], 0x0" c01000
d "rcr byte [eax], 0x0" c01800
d "shl byte [eax], 0x0" c02000
d "shr byte [eax], 0x0" c02800
d "shl byte [eax], 0x0" c03000
d "sar byte [eax], 0x0" c03800
d "rol dword [eax], 0x0" c10000
d "ror dword [eax], 0x0" c10800
d "rcl dword [eax], 0x0" c11000
d "rcr dword [eax], 0x0" c11800
d "shl dword [eax], 0x0" c12000
d "shr dword [eax], 0x0" c12800
d "shl dword [eax], 0x0" c13000
d "sar dword [eax], 0x0" c13800
d "nop [eax]" 0f1f00
d "nop [ecx]" 0f1f01
