ad "lea edx, [0x2c4b]" 8d154b2c0000
d "aaa" 37
d "aad" d50a
d "aam" d40a
d "aas" 3F
d "adc al, 0" 1400
d "adc al, byte [eax]" 1200
d "adc byte [eax], al" 1000
d "adc dword [eax], eax" 1100
d "adc eax, dword [eax]" 1300
d "add al, 0" 0400
d "add al, byte [eax]" 0200
d "add byte [bx + si], al" 670000
d "add byte [eax], 0" 800000
d "add byte [eax], 0" 820000
d "add byte [eax], al" 0000
d "add byte [eax], al" 0000
d "add dword [eax], 0" 810000000000
d "add dword [eax], 0" 830000
d "add dword [eax], eax" 0100
d "add eax, dword [eax]" 0300
d "addsd xmm0, qword [eax]" f20f5800
d "addss xmm0, dword [eax]" f30f5800
d "addsubpd xmm0, xmmword [eax]" 660fd000
d "addsubps xmm0, xmmword [eax]" f20fd000
d "and al, 0" 2400
d "and al, byte [eax]" 2200
d "and byte [eax], al" 2000
d "and dword [eax], eax" 2100
d "and eax, dword [eax]" 2300
d "arpl word [eax], ax" 6300
d "bound eax, qword [eax]" 6200
d "bsf eax, dword [eax]" 0fbc00
d "bsr eax, dword [eax]" 0fbd00
d "bswap eax" 0fc8
d "bswap ebp" 0fcd
d "bswap ebx" 0fcb
d "bswap ecx" 0fc9
d "bswap edi" 0fcf
d "bswap edx" 0fca
d "bswap esi" 0fce
d "bswap esp" 0fcc
d "bt dword [eax], eax" 0fa300
d "btc dword [eax], eax" 0fbb00
d "btr dword [eax], eax" 0fb300
d "bts dword [eax], eax" 0fab00
d "call 4" 66e80000
d "call 5" e800000000
d "call dword [eax]" ff10
d "cbw" 6698
d "cdq" 99
d "clc" F8
d "cld" FC
d "clflush byte [eax]" 0fae38
d "clgi" 0f01dd
d "cli" FA
d "clts" 0f06
d "cmc" F5
d "cmova eax, dword [eax]" 0f4700
d "cmovae eax, dword [eax]" 0f4300
d "cmovb eax, dword [eax]" 0f4200
d "cmovbe eax, dword [eax]" 0f4600
d "cmove eax, dword [eax]" 0f4400
d "cmovg eax, dword [eax]" 0f4f00
d "cmovge eax, dword [eax]" 0f4d00
d "cmovl eax, dword [eax]" 0f4c00
d "cmovle eax, dword [eax]" 0f4e00
d "cmovne eax, dword [eax]" 0f4500
d "cmovno eax, dword [eax]" 0f4100
d "cmovnp eax, dword [eax]" 0f4b00
d "cmovns eax, dword [eax]" 0f4900
d "cmovo eax, dword [eax]" 0f4000
d "cmovp eax, dword [eax]" 0f4a00
d "cmovs eax, dword [eax]" 0f4800
d "cmp al, 0" 3c00
d "cmp al, byte [eax]" 3a00
d "cmp byte [eax], al" 3800
d "cmp dword [eax], eax" 3900
d "cmp eax, dword [eax]" 3b00
d "cmpeqpd xmm0, xmmword [eax]" 660fc20000
d "cmpeqps xmm0, xmmword [eax]" 0fc20000
d "cmpeqsd xmm0, qword [eax]" f20fc20000
d "cmpeqss xmm0, dword [eax]" f30fc20000
d "cmplepd xmm0, xmmword [eax]" 660fc20002
d "cmpleps xmm0, xmmword [eax]" 0fc20002
d "cmplesd xmm0, qword [eax]" f20fc20002
d "cmpless xmm0, dword [eax]" f30fc20002
d "cmpltpd xmm0, xmmword [eax]" 660fc20001
d "cmpltps xmm0, xmmword [eax]" 0fc20001
d "cmpltsd xmm0, qword [eax]" f20fc20001
d "cmpltss xmm0, dword [eax]" f30fc20001
d "cmpneqpd xmm0, xmmword [eax]" 660fc20004
d "cmpneqps xmm0, xmmword [eax]" 0fc20004
d "cmpneqsd xmm0, qword [eax]" f20fc20004
d "cmpneqss xmm0, dword [eax]" f30fc20004
d "cmpnlepd xmm0, xmmword [eax]" 660fc20006
d "cmpnleps xmm0, xmmword [eax]" 0fc20006
d "cmpnlesd xmm0, qword [eax]" f20fc20006
d "cmpnless xmm0, dword [eax]" f30fc20006
d "cmpnltpd xmm0, xmmword [eax]" 660fc20005
d "cmpnltps xmm0, xmmword [eax]" 0fc20005
d "cmpnltsd xmm0, qword [eax]" f20fc20005
d "cmpnltss xmm0, dword [eax]" f30fc20005
d "cmpordpd xmm0, xmmword [eax]" 660fc20007
d "cmpordps xmm0, xmmword [eax]" 0fc20007
d "cmpordsd xmm0, qword [eax]" f20fc20007
d "cmpordss xmm0, dword [eax]" f30fc20007
d "cmpsb byte [esi], byte ptr es:[edi]" a6
d "cmpsd dword [esi], dword ptr es:[edi]" a7
d "cmpunordpd xmm0, xmmword [eax]" 660fc20003
d "cmpunordps xmm0, xmmword [eax]" 0fc20003
d "cmpunordsd xmm0, qword [eax]" f20fc20003
d "cmpunordss xmm0, dword [eax]" f30fc20003
d "cmpxchg byte [eax], al" 0fb000
d "cmpxchg dword [eax], eax" 0fb100
d "cpuid" 0fa2
d "crc32 eax, byte [eax]" f20f38f000
d "crc32 eax, dword [eax]" f20f38f100
d "cwd" 6699
d "cwde" 98
d "daa" 27
d "das" 2F
d "dec byte [eax]" fe08
d "dec dword [eax]" ff08
d "dec eax" 48
d "dec ebp" 4d
d "dec ebx" 4b
d "dec ecx" 49
d "dec edi" 4f
d "dec edx" 4a
d "dec esi" 4e
d "dec esp" 4c
d "div byte [eax]" f630
d "divsd xmm0, qword [eax]" f20f5e00
d "divss xmm0, dword [eax]" f30f5e00
d "emms" 0f77
ad "endbr32" f30f1efb
d "femms" 0f0e
d "fxrstor [eax]" 0fae08
d "fxsave [eax]" 0fae00
d "getsec" 0f37
d "haddpd xmm0, xmmword [eax]" 660f7c00
d "haddps xmm0, xmmword [eax]" f20f7c00
d "hlt" F4
d "hsubpd xmm0, xmmword [eax]" 660f7d00
d "hsubps xmm0, xmmword [eax]" f20f7d00
d "idiv byte [eax]" f638
d "imul byte [eax]" f628
d "imul eax, dword [eax]" 0faf00
d "imul eax, dword [eax], 0" 690000000000
d "imul eax, dword [eax], 0" 6b0000
d "in al, 0" E400
d "in al, dx" ec
d "in eax, 0" E500
d "in eax, 0x8c" e58c
d "in eax, dx" ed
d "inc byte [eax]" fe00
d "inc dword [eax]" ff00
d "inc eax" 40
d "inc ebp" 45
d "inc ebx" 43
d "inc ecx" 41
d "inc edi" 47
d "inc edx" 42
d "inc esi" 46
d "inc esp" 44
d "insb byte es:[edi], dx" 6c
d "insd dword es:[edi], dx" 6d
d "int 1" CD01
d "int 3" CD03
d "int1" F1
d "int3" CC
d "into" CE
d "invd" 0f08
d "invlpg byte [eax]" 0f0138
d "iret" 66CF
d "iretd" CF
d "ja 2" 7700
d "ja 6" 0f8700000000
d "jae 2" 7300
d "jae 6" 0f8300000000
d "jb 2" 7200
d "jb 6" 0f8200000000
d "jbe 2" 7600
d "jbe 6" 0f8600000000
d "je 2" 7400
d "je 6" 0f8400000000
d "jg 2" 7f00
d "jg 6" 0f8f00000000
d "jge 2" 7d00
d "jge 6" 0f8d00000000
d "jl 2" 7c00
d "jl 6" 0f8c00000000
d "jle 2" 7e00
d "jle 6" 0f8e00000000
d "jmp 3" 66EB00
d "jne 2" 7500
d "jne 6" 0f8500000000
d "jno 2" 7100
d "jno 6" 0f8100000000
d "jnp 2" 7b00
d "jnp 6" 0f8b00000000
d "jns 2" 7900
d "jns 6" 0f8900000000
d "jo 2" 7000
d "jo 6" 0f8000000000
d "jp 2" 7a00
d "jp 6" 0f8a00000000
d "js 2" 7800
d "js 6" 0f8800000000
d "lahf" 9F
d "lar eax, word [eax]" 0f0200
d "lcall [0]" ff1c2500000000
d "lcall [eax]" ff18
d "lddqu xmm0, xmmword [eax]" f20ff000
d "ldmxcsr dword [eax]" 0fae10
d "lds eax, [eax]" c500
d "lea eax, [eax]" 8d00
d "leave" C9
d "les eax, [eax]" c400
d "lfence" 0faee8
d "lgdt [eax]" 0f0110
d "lidt [eax]" 0f0118
d "lldt ax" 0f00d0
d "lldt word [eax]" 0f0010
d "lmsw ax" 0f01f0
d "lmsw word [eax]" 0f0130
d "lock and word fs:[bx + si], si" 646766f02130
d "lodsb al, byte [esi]" ac
d "lodsd eax, dword [esi]" ad
d "loop 3" 66e200
d "lsl eax, dword [eax]" 0f0300
d "ltr ax" 0f00d8
d "ltr word [eax]" 0f0018
d "lzcnt eax, dword [eax]" f30fbd00
d "mfence" 0faef0
d "monitor" 0f01c8
d "mov ah, 0" B400
d "mov ah, 0" b400
d "mov al, 0" B000
d "mov al, 0" b000
d "mov al, byte [0]" a000000000
d "mov al, byte [eax]" 8a00
d "mov bh, 0" B700
d "mov bh, 0" b700
d "mov bl, 0" B300
d "mov bl, 0" b300
d "mov byte [0], al" a200000000
d "mov byte [eax], 0" c60000
d "mov byte [eax], al" 8800
d "mov ch, 0" B500
d "mov ch, 0" b500
d "mov cl, 0" B100
d "mov cl, 0" b100
d "mov dh, 0" B600
d "mov dh, 0" b600
d "mov dl, 0" B200
d "mov dl, 0" b200
d "mov dr0, eax" 0f2300
d "mov dword [0], eax" a300000000
d "mov dword [eax], 0" c70000000000
d "mov dword [eax], eax" 8900
d "mov dword cs:[eax], eax" 2e8900
d "mov dword ds:[eax], eax" 3e8900
d "mov dword es:[eax], eax" 268900
d "mov dword fs:[eax], eax" 648900
d "mov dword gs:[eax], eax" 658900
d "mov dword ss:[eax], eax" 368900
d "mov eax, 0" b800000000
d "mov eax, cr0" 0f2000
d "mov eax, dr0" 0f2100
d "mov cr0, eax" 0f2200
d "mov eax, dword [0]" a100000000
d "mov eax, dword [eax]" 8b00
d "mov eax, dword [ebp]" 8b4500
d "mov eax, dword [esp]" 8b0424
d "mov eax, dword fs:[ebp]" 648b4500
d "mov ebp, 0" bd00000000
d "mov ebx, 0" bb00000000
d "mov ecx, 0" b900000000
d "mov edi, 0" bf00000000
d "mov edx, 0" ba00000000
d "mov es, word [eax]" 8e00
d "mov esi, 0" be00000000
d "mov esp, 0" bc00000000
d "mov word [eax], es" 8c00
a "mov al, [0xbeef]" a0efbe0000
a "mov ax, [0xbeef]" 66a1efbe0000
a "mov eax, [0xbeef]" a1efbe0000
a "mov eax, [0x12345678]" a178563412
d "movapd xmm0, xmmword [eax]" 660f2800
d "movapd xmmword [eax], xmm0" 660f2900
d "movhpd qword [eax], xmm0" 660f1700
d "movhpd xmm0, qword [eax]" 660f1600
d "movlpd qword [eax], xmm0" 660f1300
d "movlpd xmm0, qword [eax]" 660f1200
d "movntdq xmmword [eax], xmm0" 660fe700
d "movnti dword [eax], eax" 0fc300
d "movntq qword [eax], mm0" 0fe700
d "movq qword [eax], xmm0" 660fd600
d "movsb byte es:[edi], byte ptr [esi]" a4
d "movsd dword es:[edi], dword ptr [esi]" a5
d "movsd dword es:[edi], dword ptr fs:[esi]" 64a5
d "movshdup xmm0, xmmword [eax]" f30f1600
d "movsldup xmm0, xmmword [eax]" f30f1200
d "movss dword [eax], xmm0" f30f1100
d "movss xmm0, dword [eax]" f30f1000
d "movsx eax, byte [eax]" 0fbe00
d "movsx eax, word [eax]" 0fbf00
d "movupd xmm0, xmmword [eax]" 660f1000
d "movupd xmmword [eax], xmm0" 660f1100
d "movzx eax, byte [eax]" 0fb600
d "movzx eax, word [eax]" 0fb700
ad "mov byte [esp + eax + 0xf], 0" c644040f00
ad "mov byte [eax + ecx + 0xf], 0" c644080f00
ad "mov byte [edx + ecx + 2], 4" c6440a0204
d "mul byte [eax]" f620
d "mulsd xmm0, qword [eax]" f20f5900
d "mulss xmm0, dword [eax]" f30f5900
d "mwait" 0f01c9
d "neg byte [eax]" f618
d "neg eax" f7d8
a "neg eax" f7d8
d "nop" 90
d "not byte [eax]" f610
d "not al" f6d0
d "or al, 0" 0c00
d "or byte [eax], al" 0800
d "or dword [eax], eax" 0900
d "or eax, dword [eax]" 0b00
d "out 0, al" E600
d "out 0, eax" E700
d "out 0x84, eax" e784
ad "out dx, al" ee
ad "out dx, eax" ef
d "outsb dx, byte [esi]" 6e
d "outsd dx, dword [esi]" 6f
d "paddq xmm0, xmmword [eax]" 660fd400
d "paddsb mm0, qword [eax]" 0fec00
d "paddsw mm0, qword [eax]" 0fed00
d "paddusb mm0, qword [eax]" 0fdc00
d "paddusw mm0, qword [eax]" 0fdd00
d "pand mm0, qword [eax]" 0fdb00
d "pandn mm0, qword [eax]" 0fdf00
d "pause" f390
d "pavgb mm0, qword [eax]" 0fe000
d "pavgb mm0, qword [eax]" 0fe000
d "pavgw mm0, qword [eax]" 0fe300
d "pextrb eax, xmm0, 0" 660f3a14c000
d "pextrd eax, xmm0, 0" 660f3a16c000
d "pextrw eax, mm0, 0" 0fc5c000
d "pextrw eax, xmm0, 0" 660fc5c000
d "pinsrd xmm0, dword [eax], 0" 660f3a220000
d "pinsrw mm0, word [eax], 0" 0fc40000
d "pinsrw xmm0, word [eax], 0" 660fc40000
d "pmaxsw mm0, qword [eax]" 0fee00
d "pmaxub mm0, qword [eax]" 0fde00
d "pminsw mm0, qword [eax]" 0fea00
d "pminub mm0, qword [eax]" 0fda00
d "pop ds" 1F
d "pop dword [eax]" 8f00
d "pop eax" 58
d "pop ebp" 5D
d "pop ebx" 5B
d "pop ecx" 59
d "pop edi" 5F
d "pop edx" 5A
d "pop es" 07
d "pop esi" 5E
d "pop esp" 5C
d "pop fs" 0fa1
d "pop gs" 0fa9
d "pop ss" 17
d "popal" 61
d "popaw" 6661
d "popfd" 9D
d "por mm0, qword [eax]" 0feb00
d "prefetchnta byte [eax]" 0f1800
d "prefetcht0 byte [eax]" 0f1808
d "prefetcht1 byte [eax]" 0f1810
d "prefetcht2 byte [eax]" 0f1818
d "psrad mm0, 0" 0f72e000
d "psrad mm0, qword [eax]" 0fe200
d "psrad xmm0, 0" 660f72e000
d "psrad xmm0, xmmword [eax]" 660fe200
d "psraw mm0, 0" 0f71e000
d "psraw mm0, qword [eax]" 0fe100
d "psraw xmm0, 0" 660f71e000
d "psraw xmm0, xmmword [eax]" 660fe100
d "psubsb mm0, qword [eax]" 0fe800
d "psubsw mm0, qword [eax]" 0fe900
d "psubusb mm0, qword [eax]" 0fd800
d "psubusw mm0, qword [eax]" 0fd900
d "punpckhqdq xmm0, xmmword [eax]" 660f6d00
d "punpcklqdq xmm0, xmmword [eax]" 660f6c00
d "push 0" 6a00
d "push cs" 0E
d "push ds" 1E
d "push dword [eax]" ff30
d "push eax" 50
d "push ebp" 55
d "push ebx" 53
d "push ecx" 51
d "push edi" 57
d "push edx" 52
d "push es" 06
d "push esi" 56
d "push esp" 54
d "push fs" 0fa0
d "push gs" 0fa8
d "push ss" 16
d "pushal" 60
d "pushfd" 9C
d "pxor mm0, qword [eax]" 0fef00
d "rdmsr" 0f32
d "rdpmc" 0f33
d "rdtsc" 0f31
d "rdtscp" 0f01f9
d "repne movsb byte es:[edi], byte ptr [esi]" f2a4
d "ret" C3
d "retf 0" CA0000
d "retf" CB
d "rol byte [eax], 0" c00000
d "rol byte [eax], 1" d000
d "rol byte [eax], cl" d200
d "rol dword [eax], 0" c10000
d "rol dword [eax], 1" d100
d "rol dword [eax], cl" d300
d "rsm" 0faa
d "sahf" 9E
d "salc" D6
d "sbb al, 0" 1c00
d "sbb al, byte [eax]" 1a00
d "sbb byte [eax], al" 1800
d "sbb dword [eax], eax" 1900
d "sbb eax, dword [eax]" 1b00
d "scasb al, byte es:[edi]" ae
d "scasd eax, dword es:[edi]" af
d "seta byte [eax]" 660f9700
d "setae byte [eax]" 660f9300
d "setb byte [eax]" 660f9200
d "setbe byte [eax]" 660f9600
d "sete byte [eax]" 660f9400
d "setg byte [eax]" 660f9f00
d "setge byte [eax]" 660f9d00
d "setl byte [eax]" 660f9c00
d "setle byte [eax]" 660f9e00
d "setne byte [eax]" 660f9500
d "setno byte [eax]" 660f9100
d "setnp byte [eax]" 660f9b00
d "setns byte [eax]" 660f9900
d "seto byte [eax]" 660f9000
d "setp byte [eax]" 660f9a00
d "sets byte [eax]" 660f9800
d "sfence" 0faef8
d "sgdt [eax]" 0f0100
d "shld dword [eax], eax, 0" 0fa40000
d "shld dword [eax], eax, cl" 0fa500
d "shrd dword [eax], eax, 0" 0fac0000
d "shrd dword [eax], eax, cl" 0fad00
d "shufpd xmm0, xmmword [eax], 0" 660fc60000
d "shufps xmm0, xmmword [eax], 0" 0fc60000
d "sidt [eax]" 0f0108
d "sldt word [eax]" 0f0000
d "smsw ax" 660f01e0
d "smsw eax" 0f01e0
d "smsw word [eax]" 0f0120
d "stc" F9
d "std" FD
d "stgi" 0f01dc
d "sti" FB
d "stmxcsr dword [eax]" 0fae18
d "stosb byte es:[edi], al" aa
d "stosd dword es:[edi], eax" ab
d "str word [eax]" 0f0008
d "sub al, 0" 2c00
d "sub al, byte [eax]" 2a00
d "sub byte [eax], al" 2800
d "sub dword [eax], eax" 2900
d "sub eax, dword [eax]" 2b00
d "subsd xmm0, qword [eax]" f20f5c00
d "subss xmm0, dword [eax]" f30f5c00
d "syscall" 0f05
d "sysenter" 0f34
d "sysexit" 0f35
d "sysret" 0f07
d "test al, 0" a800
d "test byte [eax], 0" f60000
d "test byte [eax], 0" f60800
d "test byte [eax], al" 8400
d "test dword [eax], 0" f70000000000
d "test dword [eax], 0" f70000000000
d "test dword [eax], 0" f70800000000
d "test dword [eax], eax" 8500
d "test eax, 0" a900000000
d "ud2" 0f0b
d "unpckhpd xmm0, xmmword [eax]" 660f1500
d "unpcklpd xmm0, xmmword [eax]" 660f1400
d "verr ax" 0f00e0
d "verr word [eax]" 0f0020
d "verw ax" 0f00e8
d "verw word [eax]" 0f0028
d "vmcall" 0f01c1
d "vmclear qword [eax]" 660fc730
d "vmlaunch" 0f01c2
d "vmmcall" 0f01d9
d "vmptrld qword [eax]" 0fc730
d "vmptrst qword [eax]" 0fc738
d "vmresume" 0f01c3
d "vmxoff" 0f01c4
d "vmxon qword [eax]" f30fc730
d "vzeroall" c5fc77
d "vzeroupper" c5f877
d "wbinvd" 0f09
d "wrmsr" 0f30
d "xadd byte [eax], al" 0fc000
d "xadd dword [eax], eax" 0fc100
d "xchg byte [eax], al" 8600
d "xchg dword [eax], eax" 8700
d "xchg eax, ebp" 95
d "xchg eax, ebx" 93
d "xchg eax, ecx" 91
d "xchg eax, edi" 97
d "xchg eax, edx" 92
d "xchg eax, esi" 96
d "xchg eax, esp" 94
d "xgetbv" 0f01d0
d "xlatb" D7
d "xor al, 0" 3400
d "xor al, byte [eax]" 3200
d "xor byte [eax], al" 3000
d "xor byte [eax], 0xff" 8030FF
d "xor dword [eax], eax" 3100
d "xor eax, dword [eax]" 3300
d "xrstor [eax]" 0fae28
d "xsave [eax]" 0fae20
d "xsetbv" 0f01d1
d "xsaves [ecx]" 0fc729
d "xsaveopt [ecx]" 0fae31
d "xrstors [ecx]" 0fc719
dB "adx" d4
dB "amx" d5
d "cwde" 98
dB "cmpxchg16b [eax]" 67480f0c70
dB "cmpxchg8b dword [eax]" 0fc7c0
dB "extrq xmm0, 0, 0" 660f78000000
dB "extrq xmm0, xmm0" 660f7900
dB "invlpga" 0f01df
dB "lcall 0, 0" 9a
dB "lfs eax, dword [eax]" 0fb400
dB "lgs eax, dword [eax]" 0fb500
dB "lock mov dword [eax], eax" f08900
dB "lock mov eax, eax" f089c0
dB "lock" f00fc7c0
dB "lss eax, dword [eax]" 0fb200
dB "maskmovdqu xmm0, xmm0" 660ff7
dB "maskmovq mm0, mm0" 0ff7
dB "movdq2q mm0, xmm0" f20fd6
dB "movq2dq xmm0, mm0" f30fd6
dB "pextrq dword [eax], xmm0, 0" 660f3a16
dB "pinsrq xmm0, dword [eax], 0" 660f3a22
dB "pmovmskb eax, mm0" 0fd7
dB "popcnt eax, qword [eax]" f30fb8
dB "prefetch byte [eax]" 0f0d00
d "rep movsb byte es:[edi], byte ptr [esi]" f3a4
dB "retw" 66c3
dB "skinit" 0f01de
dB "swapgs" 0f1ff8
dB "vmload" 0f01da
dB "vmrun" 0f01d8
dB "vmsave" 0f01db
d "vaddpd ymm0, ymm0, ymm0" c5fd58c0
d "aesdec xmm0, xmm0" 660f38dec0
d "aesdeclast xmm0, xmm0" 660f38dfc0
d "aesenc xmm0, xmm0" 660f38dcc0
d "aesenclast xmm0, xmm0" 660f38ddc0
d "aesimc xmm0, xmm0" 660f38dbc0
d "aeskeygenassist xmm0, xmm0, 0" 660f3adfc000
d "vaesdec xmm0, xmm0, xmm0" c4e279dec0
d "vaesdeclast xmm0, xmm0, xmm0" c4e279dfc0
d "vaesenc xmm0, xmm0, xmm0" c4e279dcc0
d "vaesenclast xmm0, xmm0, xmm0" c4e279ddc0
d "vaesimc xmm0, xmm0" c4e279dbc0
d "vaeskeygenassist xmm0, xmm0, 0" c4e379dfc000
d "vextractf128 xmm0, ymm0, 0" c4e37d19c000
d "vbroadcastf128 ymm0, xmmword [0]" c4e27d1a0500000000
d "vbroadcastsd ymm0, qword [0]" c4e27d190500000000
d "vinsertf128 ymm0, ymm0, xmm0, 0" c4e37d18c000
d "vperm2f128 ymm0, ymm0, ymm0, 0" c4e37d06c000
d "vpermilpd ymm0, ymm0, ymmword [0]" c4e27d0d0500000000
d "vpermilps ymm0, ymm0, ymmword [0]" c4e27d0c0500000000
d "vfmadd132pd xmm0, xmm0, xmm0" c4e2f998c0
d "vfmadd213pd xmm0, xmm0, xmm0" c4e2f9a8c0
d "vfmadd231pd xmm0, xmm0, xmm0" c4e2f9b8c0
d "addpd xmm0, xmmword [eax]" 660f5800
d "vaeskeygenassist xmm0, xmm0, 0" c4e379dfc000
d "vextractf128 xmm0, ymm0, 0" c4e37d19c000
d "vbroadcastf128 ymm0, xmmword [0]" c4e27d1a0500000000
d "vbroadcastsd ymm0, qword [0]" c4e27d190500000000
d "vbroadcastss ymm0, dword [eax]" c4e27d1800
d "vinsertf128 ymm0, ymm0, xmm0, 0" c4e37d18c000
d "vperm2f128 ymm0, ymm0, ymm0, 0" c4e37d06c000
d "vmaskmovps ymm0, ymm0, ymmword [0]" c4e27d2c0500000000
d "vmaskmovpd ymm0, ymm0, ymmword [0]" c4e27d2d0500000000
d "vpermilpd ymm0, ymm0, ymmword [0]" c4e27d0d0500000000
d "vpermilps ymm0, ymm0, ymmword [0]" c4e27d0c0500000000
d "pclmulqdq xmm0, xmm0, 0" 660f3a44c000
d "vtestps ymm0, ymm0" c4e27d0ec0
d "vtestpd ymm0, ymm0" c4e27d0fc0
d "pshufb xmm0, xmmword [eax]" 660f380000
d "phaddw xmm0, xmmword [eax]" 660f380100
d "phaddd xmm0, xmmword [eax]" 660f380200
d "phaddsw xmm0, xmmword [eax]" 660f380300
d "pmaddubsw xmm0, xmmword [eax]" 660f380400
d "phsubw xmm0, xmmword [eax]" 660f380500
d "phsubd xmm0, xmmword [eax]" 660f380600
d "phsubsw xmm0, xmmword [eax]" 660f380700
d "pblendvb xmm0, xmm0" 660f3810c0
d "blendvps xmm0, xmm0" 660f3814c0
d "blendvpd xmm0, xmm0" 660f3815c0
d "ptest xmm0, xmm0" 660f3817c0
d "pcmpgtq xmm0, xmm0" 660f3837c0
d "pmulld xmm0, xmm0" 660f3840c0
d "phminposuw xmm0, xmm0" 660f3841c0
d "movbe dword [eax], eax" 0f38f100
d "movbe eax, dword [eax]" 0f38f000
d "mulsd xmm7, xmm7" 66f3f20f59ff
dB "mulss xmm7, xmm7" 66f2f0f59ff0
d "mulpd xmm7, xmm7" 660f59ff
dB "mulsd xmm7, xmm7" f2660f59ff
d "mulps xmm7, xmm7" 0f59ff
d "mpsadbw xmm0, xmm0, 0" 660f3a42c000
d "pcmpestrm xmm0, xmm0, 0" 660f3a60c000
d "pcmpestri xmm0, xmm0, 0" 660f3a61c000
d "pcmpistrm xmm0, xmm0, 0" 660f3a62c000
d "pcmpistri xmm0, xmm0, 0" 660f3a63c000
d "roundps xmm0, xmm0, 0" 660f3a08c000
d "roundpd xmm0, xmm0, 0" 660f3a09c000
d "roundss xmm0, xmm0, 0" 660f3a0ac000
d "roundsd xmm0, xmm0, 0" 660f3a0bc000
d "blendps xmm0, xmm0, 0" 660f3a0cc000
d "blendpd xmm0, xmm0, 0" 660f3a0dc000
d "pblendw xmm0, xmm0, 0" 660f3a0ec000
d "palignr xmm0, xmm0, 0" 660f3a0fc000
d "palignr mm0, mm0, 0" 0f3a0fc000
d "psrlw mm0, 0" 0f71d000
d "psrld mm0, 0" 0f72d000
d "psrlq mm0, 0" 0f73d000
d "psllw mm0, 0" 0f71f000
d "psllq mm0, 0" 0f73f000
d "psrlw xmm0, 0" 660f71d000
d "psrld xmm0, 0" 660f72d000
d "psrlq xmm0, 0" 660f73d000
d "psllw xmm0, 0" 660f71f000
d "pslld xmm0, 0" 660f72f000
d "psllq xmm0, 0" 660f73f000
d "psrldq xmm0, 0" 660f73d800
d "pslldq xmm0, 0" 660f73f800
d "sqrtps xmm0, xmmword [eax]" 0f5100
d "sqrtpd xmm0, xmmword [eax]" 660f5100
d "sqrtsd xmm0, qword [eax]" f20f5100
d "sqrtss xmm0, dword [eax]" f30f5100
d "rsqrtps xmm0, xmmword [eax]" 0f5200
d "rsqrtss xmm0, dword [eax]" f30f5200
d "rcpps xmm0, xmmword [eax]" 0f5300
d "rcpss xmm0, dword [eax]" f30f5300
d "andps xmm0, xmmword [eax]" 0f5400
d "andnps xmm0, xmmword [eax]" 0f5500
d "andpd xmm0, xmmword [eax]" 660f5400
d "andnpd xmm0, xmmword [eax]" 660f5500
d "orps xmm0, xmmword [eax]" 0f5600
d "xorps xmm0, xmmword [eax]" 0f5700
d "orpd xmm0, xmmword [eax]" 660f5600
d "xorpd xmm0, xmmword [eax]" 660f5700
d "addps xmm0, xmmword [eax]" 0f5800
d "subps xmm0, xmmword [eax]" 0f5c00
d "mulps xmm0, xmmword [eax]" 0f5900
d "divps xmm0, xmmword [eax]" 0f5e00
d "addpd xmm0, xmmword [eax]" 660f5800
d "subpd xmm0, xmmword [eax]" 660f5c00
d "mulpd xmm0, xmmword [eax]" 660f5900
d "divpd xmm0, xmmword [eax]" 660f5e00
d "minps xmm0, xmmword [eax]" 0f5d00
d "maxps xmm0, xmmword [eax]" 0f5f00
d "minpd xmm0, xmmword [eax]" 660f5d00
d "maxpd xmm0, xmmword [eax]" 660f5f00
d "minsd xmm0, qword [eax]" f20f5d00
d "maxsd xmm0, qword [eax]" f20f5f00
d "minss xmm0, dword [eax]" f30f5d00
d "maxss xmm0, dword [eax]" f30f5f00
d "punpcklbw mm0, qword [eax]" 0f6000
d "punpcklwd mm0, qword [eax]" 0f6100
d "punpckldq mm0, qword [eax]" 0f6200
d "punpcklbw xmm0, xmmword [eax]" 660f6000
d "punpcklwd xmm0, xmmword [eax]" 660f6100
d "punpckldq xmm0, xmmword [eax]" 660f6200
d "packsswb mm0, qword [eax]" 0f6300
d "packuswb mm0, qword [eax]" 0f6700
d "packsswb xmm0, xmmword [eax]" 660f6300
d "packuswb xmm0, xmmword [eax]" 660f6700
d "pcmpgtb mm0, qword [eax]" 0f6400
d "pcmpgtw mm0, qword [eax]" 0f6500
d "pcmpgtd mm0, qword [eax]" 0f6600
d "pcmpgtb xmm0, xmmword [eax]" 660f6400
d "pcmpgtw xmm0, xmmword [eax]" 660f6500
d "pcmpgtd xmm0, xmmword [eax]" 660f6600
d "punpckhbw mm0, qword [eax]" 0f6800
d "punpckhwd mm0, qword [eax]" 0f6900
d "punpckhdq mm0, qword [eax]" 0f6a00
d "punpckhbw xmm0, xmmword [eax]" 660f6800
d "punpckhwd xmm0, xmmword [eax]" 660f6900
d "punpckhdq xmm0, xmmword [eax]" 660f6a00
d "packssdw mm0, qword [eax]" 0f6b00
d "packssdw xmm0, xmmword [eax]" 660f6b00
d "pshufb mm0, qword [eax]" 0f380000
d "pshufw mm0, qword [eax], 0" 0f700000
d "pshufb xmm0, xmmword [eax]" 660f380000
d "pshufd xmm0, xmmword [eax], 0" 660f700000
d "pshuflw xmm0, xmmword [eax], 0" f20f700000
d "pshufhw xmm0, xmmword [eax], 0" f30f700000
d "pcmpeqb mm0, qword [eax]" 0f7400
d "pcmpeqw mm0, qword [eax]" 0f7500
d "pcmpeqd mm0, qword [eax]" 0f7600
d "pcmpeqb xmm0, xmmword [eax]" 660f7400
d "pcmpeqw xmm0, xmmword [eax]" 660f7500
d "pcmpeqd xmm0, xmmword [eax]" 660f7600
d "movd mm0, dword [eax]" 0f6e00
d "movq mm0, qword [eax]" 0f6f00
d "movd dword [eax], mm0" 0f7e00
d "movq qword [eax], mm0" 0f7f00
d "movd xmm0, dword [eax]" 660f6e00
d "movdqa xmm0, xmmword [eax]" 660f6f00
d "movd dword [eax], xmm0" 660f7e00
d "movdqa xmmword [eax], xmm0" 660f7f00
d "movdqu xmm0, xmmword [eax]" f30f6f00
d "movq xmm0, qword [eax]" f30f7e00
d "movdqu xmmword [eax], xmm0" f30f7f00
d "pmovsxbw xmm0, xmm0" 660f3820c0
d "pmovsxbd xmm0, xmm0" 660f3821c0
d "pmovsxbq xmm0, xmm0" 660f3822c0
d "pmovsxwd xmm0, xmm0" 660f3823c0
d "pmovsxwq xmm0, xmm0" 660f3824c0
d "pmovsxdq xmm0, xmm0" 660f3825c0
d "pmovzxbw xmm0, xmm0" 660f3830c0
d "pmovzxbd xmm0, xmm0" 660f3831c0
d "pmovzxbq xmm0, xmm0" 660f3832c0
d "pmovzxwd xmm0, xmm0" 660f3833c0
d "pmovzxwq xmm0, xmm0" 660f3834c0
d "pmovzxdq xmm0, xmm0" 660f3835c0
d "pminsb xmm0, xmm0" 660f3838c0
d "pminsd xmm0, xmm0" 660f3839c0
d "pminuw xmm0, xmm0" 660f383ac0
d "pminud xmm0, xmm0" 660f383bc0
d "pmaxsb xmm0, xmm0" 660f383cc0
d "pmaxsd xmm0, xmm0" 660f383dc0
d "pmaxuw xmm0, xmm0" 660f383ec0
d "pmaxud xmm0, xmm0" 660f383fc0
d "psignb xmm0, xmm0" 660f3808c0
d "psignw xmm0, xmm0" 660f3809c0
d "psignd xmm0, xmm0" 660f380ac0
d "pmulhrsw xmm0, xmm0" 660f380bc0
d "pabsb xmm0, xmm0" 660f381cc0
d "pabsw xmm0, xmm0" 660f381dc0
d "pabsd xmm0, xmm0" 660f381ec0
d "pmuldq xmm0, xmm0" 660f3828c0
d "pcmpeqq xmm0, xmm0" 660f3829c0
d "movntdqa xmm0, xmmword [eax]" 660f382a00
d "packusdw xmm0, xmm0" 660f382bc0
d "extractps eax, xmm0, 0" 660f3a17c000
d "pinsrb xmm0, eax, 0" 660f3a20c000
d "insertps xmm0, xmm0, 0" 660f3a21c000
d "dpps xmm0, xmm0, 0" 660f3a40c000
d "dppd xmm0, xmm0, 0" 660f3a41c000
d "pslld mm0, 0" 0f72f000
d "movups xmm0, xmmword [eax]" 0f1000
d "movups xmmword [eax], xmm0" 0f1100
d "unpcklps xmm0, xmmword [eax]" 0f1400
d "unpckhps xmm0, xmmword [eax]" 0f1500
d "movlps xmm0, qword [eax]" 0f1200
d "movlps qword [eax], xmm0" 0f1300
dB "movhlps xmm0, xmm0" 0f1200
dB "movlhps xmm0, xmm0" 0f1600
d "movhps xmm0, qword [eax]" 0f1600
d "movhps qword [eax], xmm0" 0f1700
d "movmskps eax, xmm0" 0f50c0
d "movmskpd eax, xmm0" 660f50c0
d "vfmsubpd xmm0, xmm0, xmm0, xmm0" c4e3796dc000
d "vfmsubps xmm0, xmm0, xmm0, xmm0" c4e3796cc000
d "vfmsubsd xmm0, xmm0, xmm0, xmm0" c4e3796fc000
d "vfmsubss xmm0, xmm0, xmm0, xmm0" c4e3796ec000
d "vfnmaddpd xmm0, xmm0, xmm0, xmm0" c4e37979c000
d "vfnmaddps xmm0, xmm0, xmm0, xmm0" c4e37978c000
d "vfnmaddsd xmm0, xmm0, xmm0, xmm0" c4e3797bc000
d "vfnmaddss xmm0, xmm0, xmm0, xmm0" c4e3797ac000
d "vfnmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d79c000
d "vfnmaddps ymm0, ymm0, ymm0, ymm0" c4e37d78c000
d "vfnmsubpd xmm0, xmm0, xmm0, xmm0" c4e3797dc000
d "vfnmsubps xmm0, xmm0, xmm0, xmm0" c4e3797cc000
d "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000
d "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000
d "vfnmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d7dc000
d "vfnmsubps ymm0, ymm0, ymm0, ymm0" c4e37d7cc000
d "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000
d "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000
d "movsd xmm0, qword [eax]" f20f1000
d "movsd qword [eax], xmm0" f20f1100
d "movddup xmm0, qword [eax]" f20f1200
d "cvtps2pd xmm0, qword [eax]" 0f5a00
d "cvtpd2ps xmm0, xmmword [eax]" 660f5a00
d "cvtsd2ss xmm0, qword [eax]" f20f5a00
d "cvtss2sd xmm0, dword [eax]" f30f5a00
d "cvtdq2ps xmm0, xmmword [eax]" 0f5b00
d "cvtps2dq xmm0, xmmword [eax]" 660f5b00
d "cvttps2dq xmm0, xmmword [eax]" f30f5b00
d "cvttpd2dq xmm0, xmmword [eax]" 660fe600
d "cvtpd2dq xmm0, xmmword [eax]" f20fe600
d "cvtdq2pd xmm0, qword [eax]" f30fe600
d "cvttps2pi mm0, qword [eax]" 0f2c00
d "cvttpd2pi mm0, xmmword [eax]" 660f2c00
d "cvttsd2si eax, qword [eax]" f20f2c00
d "cvttss2si eax, dword [eax]" f30f2c00
d "cvtpi2ps xmm0, qword [eax]" 0f2a00
d "cvtpi2pd xmm0, qword [eax]" 660f2a00
d "cvtsi2sd xmm0, dword [eax]" f20f2a00
d "cvtsi2ss xmm0, dword [eax]" f30f2a00
d "cvtps2pi mm0, qword [eax]" 0f2d00
d "cvtsd2si eax, qword [eax]" f20f2d00
d "cvtss2si eax, dword [eax]" f30f2d00
d "cvtpd2pi mm0, xmmword [eax]" 660f2d00
d "movaps xmm0, xmmword [eax]" 0f2800
d "movaps xmmword [eax], xmm0" 0f2900
d "movntps xmmword [eax], xmm0" 0f2b00
d "movntpd xmmword [eax], xmm0" 660f2b00
d "ucomiss xmm0, dword [eax]" 0f2e00
d "comiss xmm0, xmmword [eax]" 0f2f00
d "ucomisd xmm0, qword [eax]" 660f2e00
d "comisd xmm0, xmmword [eax]" 660f2f00
d "psubb mm0, qword [eax]" 0ff800
d "psubw mm0, qword [eax]" 0ff900
d "psubd mm0, qword [eax]" 0ffa00
d "psubq mm0, qword [eax]" 0ffb00
d "paddb mm0, qword [eax]" 0ffc00
d "paddw mm0, qword [eax]" 0ffd00
d "paddd mm0, qword [eax]" 0ffe00
d "psrlw mm0, qword [eax]" 0fd100
d "psrld mm0, qword [eax]" 0fd200
d "psrlq mm0, qword [eax]" 0fd300
d "psrlw xmm0, xmmword [eax]" 660fd100
d "psrld xmm0, xmmword [eax]" 660fd200
d "psrlq xmm0, xmmword [eax]" 660fd300
d "psllw mm0, qword [eax]" 0ff100
d "pslld mm0, qword [eax]" 0ff200
d "psllq mm0, qword [eax]" 0ff300
d "psllw xmm0, xmmword [eax]" 660ff100
d "pslld xmm0, xmmword [eax]" 660ff200
d "psllq xmm0, xmmword [eax]" 660ff300
d "pmullw mm0, qword [eax]" 0fd500
d "pmullw xmm0, xmmword [eax]" 660fd500
d "pmulhuw mm0, qword [eax]" 0fe400
d "pmulhuw xmm0, xmmword [eax]" 660fe400
d "pmulhw mm0, qword [eax]" 0fe500
d "pmulhw xmm0, xmmword [eax]" 660fe500
d "pmuludq mm0, qword [eax]" 0ff400
d "pmuludq xmm0, xmmword [eax]" 660ff400
d "pmaddwd mm0, qword [eax]" 0ff500
d "pmaddwd xmm0, xmmword [eax]" 660ff500
d "psadbw mm0, qword [eax]" 0ff600
d "psadbw xmm0, xmmword [eax]" 660ff600
d "psubusb xmm0, xmmword [eax]" 660fd800
d "psubusw xmm0, xmmword [eax]" 660fd900
d "pminub xmm0, xmmword [eax]" 660fda00
d "pmaxub xmm0, xmmword [eax]" 660fde00
d "pand xmm0, xmmword [eax]" 660fdb00
d "pandn xmm0, xmmword [eax]" 660fdf00
d "paddusb xmm0, xmmword [eax]" 660fdc00
d "paddusw xmm0, xmmword [eax]" 660fdd00
d "pavgb xmm0, xmmword [eax]" 660fe000
d "pavgw xmm0, xmmword [eax]" 660fe300
d "psubsb xmm0, xmmword [eax]" 660fe800
d "psubsw xmm0, xmmword [eax]" 660fe900
d "pminsw xmm0, xmmword [eax]" 660fea00
d "pmaxsw xmm0, xmmword [eax]" 660fee00
d "por xmm0, xmmword [eax]" 660feb00
d "paddsb xmm0, xmmword [eax]" 660fec00
d "paddsw xmm0, xmmword [eax]" 660fed00
d "pxor xmm0, xmmword [eax]" 660fef00
d "psubb xmm0, xmmword [eax]" 660ff800
d "psubw xmm0, xmmword [eax]" 660ff900
d "psubd xmm0, xmmword [eax]" 660ffa00
d "psubq xmm0, xmmword [eax]" 660ffb00
d "paddb xmm0, xmmword [eax]" 660ffc00
d "paddw xmm0, xmmword [eax]" 660ffd00
d "paddd xmm0, xmmword [eax]" 660ffe00
d "vpmadcsswd xmm0, xmm0, xmm0, xmm0" 8fe878a6c000
d "vfrczpd xmm0, xmm0" 8fe97881c0
dB "vcvtph2ps xmm0, xmm0, 0" 8fe878a0c000
dB "vcvtps2ph xmm0, xmm0, 0" 8fe878a1c000
d "vfrczps xmm0, xmm0" 8fe97880c0
d "vfrczsd xmm0, xmm0" 8fe97883c0
d "vfrczss xmm0, xmm0" 8fe97882c0
d "vphaddbd xmm0, xmm0" 8fe978c2c0
d "vphaddbq xmm0, xmm0" 8fe978c3c0
d "vphaddbw xmm0, xmm0" 8fe978c1c0
d "vphadddq xmm0, xmm0" 8fe978cbc0
d "vphaddwd xmm0, xmm0" 8fe978c6c0
d "vphaddwq xmm0, xmm0" 8fe978c7c0
d "vphsubbw xmm0, xmm0" 8fe978e1c0
d "vphsubdq xmm0, xmm0" 8fe978e3c0
d "vphsubwd xmm0, xmm0" 8fe978e2c0
d "vfmaddpd xmm0, xmm0, xmm0, xmm0" c4e37969c000
d "vfmaddps xmm0, xmm0, xmm0, xmm0" c4e37968c000
d "vfmaddsd xmm0, xmm0, xmm0, xmm0" c4e3796bc000
d "vfmaddss xmm0, xmm0, xmm0, xmm0" c4e3796ac000
d "vfmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d69c000
d "vfmaddps ymm0, ymm0, ymm0, ymm0" c4e37d68c000
d "vfmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d6dc000
d "vfmsubps ymm0, ymm0, ymm0, ymm0" c4e37d6cc000
d "vfmaddsubpd xmm0, xmm0, xmm0, xmm0" c4e3795dc000
d "vfmaddsubps xmm0, xmm0, xmm0, xmm0" c4e3795cc000
d "vfmsubaddpd xmm0, xmm0, xmm0, xmm0" c4e3795fc000
d "vfmsubaddps xmm0, xmm0, xmm0, xmm0" c4e3795ec000
d "vfmaddsubpd ymm0, ymm0, ymm0, ymm0" c4e37d5dc000
d "vfmaddsubps ymm0, ymm0, ymm0, ymm0" c4e37d5cc000
d "vfmsubaddps ymm0, ymm0, ymm0, ymm0" c4e37d5ec000
d "vfmsubaddpd ymm0, ymm0, ymm0, ymm0" c4e37d5fc000
d "vpcmov xmm0, xmm0, xmm0, xmm0" 8fe878a2c000
dB "vpcomb xmm0, xmm0, xmm0, 0" 8fe878ccc000
dB "vpcomd xmm0, xmm0, xmm0, 0" 8fe878cec000
dB "vpcomq xmm0, xmm0, xmm0, 0" 8fe878cfc000
dB "vpcomub xmm0, xmm0, xmm0, 0" 8fe878ecc000
dB "vpcomud xmm0, xmm0, xmm0, 0" 8fe878eec000
dB "vpcomuq xmm0, xmm0, xmm0, 0" 8fe878efc000
dB "vpcomuw xmm0, xmm0, xmm0, 0" 8fe878edc000
dB "vpcomw xmm0, xmm0, xmm0, 0" 8fe878cdc000
d "vpmacsdd xmm0, xmm0, xmm0, xmm0" 8fe8789ec000
d "vpmacsdqh xmm0, xmm0, xmm0, xmm0" 8fe8789fc000
d "vpmacsdql xmm0, xmm0, xmm0, xmm0" 8fe87897c000
d "vpmacssdd xmm0, xmm0, xmm0, xmm0" 8fe8788ec000
d "vpmacssdqh xmm0, xmm0, xmm0, xmm0" 8fe8788fc000
d "vpmacssdql xmm0, xmm0, xmm0, xmm0" 8fe87887c000
d "vpmacsswd xmm0, xmm0, xmm0, xmm0" 8fe87886c000
d "vpmacssww xmm0, xmm0, xmm0, xmm0" 8fe87885c000
d "vpmacswd xmm0, xmm0, xmm0, xmm0" 8fe87896c000
d "vpmacsww xmm0, xmm0, xmm0, xmm0" 8fe87895c000
d "vpmadcswd xmm0, xmm0, xmm0, xmm0" 8fe878b6c000
d "vpperm xmm0, xmm0, xmm0, xmm0" 8fe878a3c000
d "vprotb xmm0, xmm0, xmm0" 8fe97890c0
d "vprotd xmm0, xmm0, xmm0" 8fe97892c0
d "vprotq xmm0, xmm0, xmm0" 8fe97893c0
d "vprotw xmm0, xmm0, xmm0" 8fe97891c0
d "vpshab xmm0, xmm0, xmm0" 8fe97898c0
d "vpshad xmm0, xmm0, xmm0" 8fe9789ac0
d "vpshaq xmm0, xmm0, xmm0" 8fe9789bc0
d "vpshaw xmm0, xmm0, xmm0" 8fe97899c0
d "vpshlb xmm0, xmm0, xmm0" 8fe97894c0
d "vpshld xmm0, xmm0, xmm0" 8fe97896c0
d "vpshlq xmm0, xmm0, xmm0" 8fe97897c0
d "vpshlw xmm0, xmm0, xmm0" 8fe97895c0
d "vphaddubd xmm0, xmm0" 8fe978d2c0
d "vphaddubq xmm0, xmm0" 8fe978d3c0
d "vphaddubw xmm0, xmm0" 8fe978d1c0
d "vphaddudq xmm0, xmm0" 8fe978dbc0
d "vphadduwd xmm0, xmm0" 8fe978d6c0
d "vphadduwq xmm0, xmm0" 8fe978d7c0
d "vpmadcsswd xmm0, xmm0, xmm0, xmm0" 8fe878a6c000
a "aaa" 37
a "aad" d50a
a "aam" d40a
a "aam 12" d40c
a "aas" 3f
a "adc al, 0" 1400
a "adc al, byte [eax]" 1200
a "adc byte [eax], al" 1000
a "adc dword [eax], eax" 1100
a "adc eax, dword [eax]" 1300
a "add al, 0" 0400
a "add ax, 0x4" 6683c004
a "add ax, 0x96" 66059600
a "add cx, 0x4" 6683c104
a "add al, byte [eax]" 0200
aB "add byte [bx + si], al" 670001
a "add byte [eax], 0" 800000
a "add byte [eax], al" 0000
a "add dword [eax], 1" 830001
a "add dword [eax+8], 1" 83400801
a "add dword [eax], eax" 0100
a "add dword [ebp+4], 1" 83450401
a "add dword [ebp+8], 1" 83450801
a "add dword [ebx], 1" 830301
a "add dword [ebx+8], 1" 83430801
a "add dword [esp+8], 1" 8344240801
a "add eax, 1" 83c001
a "add eax, 3" 83c003
a "add eax, dword [eax]" 0300
a "add [eax], eax" 0100
a "add esi,-334" 81c6b2feffff
a "add byte [0x45342], al" 000542530400
a "add byte [0x45a42], 0x24" 8005425a040024
a "add byte [eax + eax], bl" 001c
aB "addpd xmm0, xmmword [eax]" 660f5800
aB "addps xmm0, xmmword [eax]" 0f5800
aB "addsd xmm0, qword [eax]" F20F5800
aB "addss xmm0, dword [eax]" F30F5800
aB "addsubpd xmm0, xmmword [eax]" 660fd000
aB "addsubps xmm0, xmmword [eax]" f20fd000
a "adx" d4
aB "aesdeclast xmm0, xmm0" 660f38dfc0
aB "aesdec xmm0, xmm0" 660f38dec0
aB "aesenclast xmm0, xmm0" 660f38ddc0
aB "aesenc xmm0, xmm0" 660f38dcc0
aB "aesimc xmm0, xmm0" 660f38dbc0
aB "aeskeygenassist xmm0, xmm0, 0x0" 660f3adfc000
a "amx" d5
a "and al, 0" 2400
a "and ax, 0x6" 6683e006
a "and ax, 0x97" 66259700
a "and bx, 0x7" 6683e307
a "and bx, 0x97" 6681e39700
a "and al, byte [eax]" 2200
a "and byte [eax], al" 2000
a "and dword [eax], eax" 2100
a "and eax, dword [eax]" 2300
aB "andnpd xmm0, xmmword [eax]" 660f55
aB "andnps xmm0, xmmword [eax]" 0f5500
aB "andpd xmm0, xmmword [eax]" 660f54
aB "andps xmm0, xmmword [eax]" 0f5400
aB "arpl word [eax], ax" 6300
aB "blendpd xmm0, xmm0, 0" 660f3a0dc000
aB "blendps xmm0, xmm0, 0" 660f3a0cc000
aB "blendvpd xmm0, xmm0" 660f3815c0
aB "blendvps xmm0, xmm0" 660f3814c0
aB "bound eax, qword [eax]" 6200
a "bsf eax, dword [eax]" 0fbc00
a "bsr eax, dword [eax]" 0fbd00
a "bswap eax" 0fc8
a "bswap ebp" 0fcd
a "bswap ebx" 0fcb
a "bswap ecx" 0fc9
a "bswap edi" 0fcf
a "bswap edx" 0fca
a "bswap esi" 0fce
a "bswap esp" 0fcc
aB "btc dword [eax], eax" 0fbb00
aB "bt dword [eax], eax" 0fa300
aB "bt ecx, esp" 0fa3e1
aB "bt edx, 59" 0fbae23b
aB "bt ebp, -20" 0fbae5e0
aB "btr dword [eax], eax" 0fb300
aB "bts dword [eax], eax" 0fab00
a "call 0x8049100" e8fb900408
a "call 4" e8ffffffff
a "call 5" e800000000
a "call dword [eax]" ff10
a "call ebx" ffd3
a "bnd call ebx" f2ffd3
a "cbw" 6698
a "cdq" 99
a "cdqe" 98
a "clc" f8
a "cld" fc
a "clflush byte [eax]" 0fae38
a "clgi" 0f01dd
a "cli" fa
a "clts" 0f06
a "cmc" f5
a "cmova eax, dword [eax]" 0f4700
a "cmovae eax, dword [eax]" 0f4300
a "cmovb eax, dword [eax]" 0f4200
a "cmovbe eax, dword [eax]" 0f4600
a "cmove eax, dword [eax]" 0f4400
a "cmovg eax, [eax]" 0f4f00
a "cmovge eax, dword [eax]" 0f4d00
a "cmovl eax, dword [eax]" 0f4c00
a "cmovle eax, dword [eax]" 0f4e00
a "cmovne eax, dword [eax]" 0f4500
a "cmovno eax, dword [eax]" 0f4100
a "cmovnp eax, dword [eax]" 0f4b00
a "cmovns eax, dword [eax]" 0f4900
a "cmovo eax, dword [eax]" 0f4000
a "cmovp eax, dword [eax]" 0f4a00
a "cmovs eax, dword [eax]" 0f4800
a "cmova eax, dword eax" 0f47c0
a "cmovae eax, dword eax" 0f43c0
a "cmovb eax, dword eax" 0f42c0
a "cmovbe eax, dword eax" 0f46c0
a "cmove eax, dword eax" 0f44c0
a "cmovg eax, eax" 0f4fc0
a "cmovge eax, dword eax" 0f4dc0
a "cmovl eax, dword eax" 0f4cc0
a "cmovle eax, dword eax" 0f4ec0
a "cmovne eax, dword eax" 0f45c0
a "cmovno eax, dword eax" 0f41c0
a "cmovnp eax, dword eax" 0f4bc0
a "cmovns eax, dword eax" 0f49c0
a "cmovo eax, dword eax" 0f40c0
a "cmovp eax, dword eax" 0f4ac0
a "cmovs eax, dword eax" 0f48c0
a "cmova eax, [eax*2]" 0f470400
a "cmovae eax, [ecx+4]" 0f434104
a "cmovb eax, [edx*4+edx]" 0f420492
a "cmovbe eax, [ecx*8]" 0f4604cd
a "cmove eax, [ebx*2+44]" 0f44441b2c
a "cmovg ecx, [eax*4+656]" 0f4f0c8590020000
a "cmovge edx, [ebp]" 0f4d5500
a "cmovl eax, [ebp*2+88]" 0f4c442d58
a "cmp al, 0" 3c00
a "cmp al, byte [eax]" 3a00
a "cmp byte [eax], al" 3800
a "cmp dword [eax], eax" 3900
a "cmp eax, 33" 83f821
a "cmp eax, dword [eax]" 3b00
a "cmp eax, ebx" 39d8
a "cmp ebx, eax" 39c3
a "cmp edx, esi" 39f2
aB "cmpeqpd xmm0, xmmword [eax]" 660fc20000
aB "cmpeqps xmm0, xmmword [eax]" 0fc20000
aB "cmpeqss xmm0, dword [eax]" f30fc20000
aB "cmplepd xmm0, xmmword [eax]" 660fc20002
aB "cmpleps xmm0, xmmword [eax]" 0fc20002
aB "cmplesd xmm0, qword [eax]" f20fc20002
aB "cmpless xmm0, dword [eax]" f30fc20002
aB "cmpltpd xmm0, xmmword [eax]" 660fc20001
aB "cmpltps xmm0, xmmword [eax]" 0fc20001
aB "cmpltsd xmm0, qword [eax]" f20fc20001
aB "cmpltss xmm0, dword [eax]" f30fc20001
aB "cmpneqpd xmm0, xmmword [eax]" 660fc20004
aB "cmpneqps xmm0, xmmword [eax]" 0fc20004
aB "cmpneqsd xmm0, qword [eax]" f20fc20004
aB "cmpneqss xmm0, dword [eax]" f30fc20004
aB "cmpnlepd xmm0, xmmword [eax]" 660fc20006
aB "cmpnleps xmm0, xmmword [eax]" 0fc20006
aB "cmpnlesd xmm0, qword [eax]" f20fc20006
aB "cmpnless xmm0, dword [eax]" f30fc20006
aB "cmpnltpd xmm0, xmmword [eax]" 660fc20005
aB "cmpnltps xmm0, xmmword [eax]" 0fc20005
aB "cmpnltsd xmm0, qword [eax]" f20fc20005
aB "cmpnltss xmm0, dword [eax]" f30fc20005
aB "cmpordpd xmm0, xmmword [eax]" 660fc20007
aB "cmpordps xmm0, xmmword [eax]" 0fc20007
aB "cmpordsd xmm0, qword [eax]" f20fc20007
aB "cmpordss xmm0, dword [eax]" f30fc20007
a "cmpsb byte [esi], byte ptr es:[edi]" a6
a "cmpsd dword [esi], dword ptr es:[edi]" a7
aB "cmpsd xmm0, qword [eax]" f20fc20000
aB "cmpunordpd xmm0, xmmword [eax]" 660fc20003
aB "cmpunordps xmm0, xmmword [eax]" 0fc20003
aB "cmpunordsd xmm0, qword [eax]" f20fc20003
aB "cmpunordss xmm0, dword [eax]" f30fc20003
aB "cmpxchg16b [eax]" 67480f0c70
aB "cmpxchg8b dword [eax]" 0fc7c0
aB "cmpxchg byte [eax], al" 0fb000
aB "cmpxchg dword [eax], eax" 0fb100
aB "comisd xmm0, xmmword [eax]" 660f2f00
aB "comiss xmm0, xmmword [eax]" 0f2f00
a "cpuid" 0fa2
aB "crc32 eax, byte [eax]" f20f38f0
aB "crc32 eax, dword [eax]" f20f38f1
aB "cvtdq2pd xmm0, qword [eax]" f30fe600
aB "cvtdq2ps xmm0, xmmword [eax]" 0f5b00
aB "cvtpd2dq xmm0, xmmword [eax]" f20fe600
aB "cvtpd2pi mm0, xmmword [eax]" 660f2d00
aB "cvtpd2ps xmm0, xmmword [eax]" 660f5a00
aB "cvtpi2pd xmm0, qword [eax]" 660f2a00
aB "cvtpi2ps xmm0, qword [eax]" 0f2a00
aB "cvtps2dq xmm0, xmmword [eax]" 660f5b00
aB "cvtps2pd xmm0, qword [eax]" 0f5a00
aB "cvtps2pi mm0, qword [eax]" 0f2d00
aB "cvtsd2si eax, qword [eax]" f20f2d00
aB "cvtsd2ss xmm0, qword [eax]" f20f5a00
aB "cvtsi2sd xmm0, dword [eax]" f20f2a00
aB "cvtsi2ss xmm0, dword [eax]" f30f2a00
aB "cvtss2sd xmm0, dword [eax]" f30f5a00
aB "cvtss2si eax, dword [eax]" f30f2d00
aB "cvttpd2dq xmm0, xmmword [eax]" 660fe600
aB "cvttpd2pi mm0, xmmword [eax]" 660f2c00
aB "cvttps2dq xmm0, xmmword [eax]" f30f5b00
aB "cvttps2pi mm0, qword [eax]" 0f2c00
aB "cvttsd2si eax, qword [eax]" f20f2c00
aB "cvttss2si eax, dword [eax]" f30f2c00
a "cwd" 6699
a "cwde" 98
a "daa" 27
a "das" 2f
a "dec byte [eax]" fe08
a "dec dword [eax]" ff08
a "dec eax" 48
a "dec ebp" 4d
a "dec ebx" 4b
a "dec ecx" 49
a "dec edi" 4f
a "dec edx" 4a
a "dec esi" 4e
a "dec esp" 4c
a "div byte [eax]" f630
aB "divpd xmm0, xmmword [eax]" 660f5e00
aB "divps xmm0, xmmword [eax]" 0f5e00
aB "divsd xmm0, qword [eax]" f20f5e00
aB "divss xmm0, dword [eax]" f30f5e00
aB "dppd xmm0, xmm0, 0" 660f3a41c000
aB "dpps xmm0, xmm0, 0" 660f3a40c000
a "emms" 0f77
aB "extractps eax, xmm0, 0" 660f3a17c000
aB "extrq xmm0, 0x0, 0x0" 660f78c00000
aB "extrq xmm0, xmm0" 660f7900
a "femms" 0f0e
a "fsincos" d9fb
a "fxrstor [eax]" 0fae08
a "fxsave [eax]" 0fae00
a "getsec" 0f37
aB "haddpd xmm0, xmmword [eax]" 660f7c00
aB "haddps xmm0, xmmword [eax]" f20f7c00
a "hlt" f4
aB "hsubpd xmm0, xmmword [eax]" 660f7d00
aB "hsubps xmm0, xmmword [eax]" f20f7d00
a "idiv byte [eax]" f638
a "imul eax" f7e8
a "imul edx" f7ea
a "imul edx, eax" 0fafd0
a "imul ecx, 23" 6bc917
a "imul edx, ecx, 34" 6bd122
a "imul byte [eax]" f628
a "imul dword [eax]" f728
a "imul ebx, [edx + ecx]" 0faf1c0a
a "imul ebx, dword [edx], 0" 6b1a00
a "imul ebx, edx, 4" 6bda04
a "imul eax, dword [eax]" 0faf00
a "imul eax, [eax], 0" 6b0000
a "in al,0" e400
a "in al,dx" ec
a "inc byte [eax]" fe00
a "inc dword [eax]" ff00
a "inc eax" 40
a "inc ebp" 45
a "inc ebx" 43
a "inc ecx" 41
a "inc edi" 47
a "inc edx" 42
a "inc esi" 46
a "inc esp" 44
a "in eax, 0" e500
a "in eax, 0x8c" e58c
a "in eax, dx" ed
a "insb byte es:[edi], dx" 6c
a "insd dword es:[edi], dx" 6d
aB "insertps xmm0, xmm0, 0" 660f3a21c000
a "int 0x21" cd21
a "int 1" cd01
a "int1" f1
a "int3" cc
a "int 3" cd03
a "into" ce
a "invd" 0f08
aB "invlpga" 0f01df
aB "invlpg byte [eax]" 0f0138
a "iret" 66cf
a "iretd" cf
a "ja 0x8049300" 0f87fa920408
a "ja 2" 7700
a "ja 6" 7704
a "jae 2" 7300
a "jae 6" 7304
a "jb 0x8049300" 0f82fa920408
a "jb 2" 7200
a "jb 6" 7204
a "jbe 2" 7600
a "jbe 6" 7604
a "je 2" 7400
a "je 6" 7404
a "jg 0x8049300" 0f8ffa920408
a "jg 2" 7f00
a "jg 6" 7f04
a "jge 0x8048010" 0f8d0a800408
a "jge 0x8049300" 0f8dfa920408
a "jge 2" 7d00
a "jge 6" 7d04
a "jl 0x8048010" 0f8c0a800408
a "jl 0x8049300" 0f8cfa920408
a "jl 2" 7c00
a "jl 6" 7c04
a "jle 0x8048010" 0f8e0a800408
a "jle 0x8049300" 0f8efa920408
a "jle 2" 7e00
a "jle 6" 7e04
a "jmp 0" ebfe
a "jmp 0x42" eb40
a "jmp -0x7e" eb80
a "jmp -0x7f" e97cffffff
a "jmp 0x8049200" e9fb910408
a "jmp 0x81" eb7f
a "jmp 0x82" e97d000000
a "jmp 2" eb00
a "jmp 3" eb01
a "jmp ecx" ffe1
a "jmp [ecx]" ff21
a "jmp [ebx+43]" ff632b
a "jmp [ecx+200]" ffa1c8000000
a "jmp [edx-10]" ff62f6
a "jmp [eax-140]" ffa074ffffff
a "bnd jmp 0x82" f2e97d000000
a "jne 6" 7504
a "jno 2" 7100
a "jno 6" 7104
a "jnp 2" 7b00
a "jnp 6" 7b04
a "jns 2" 7900
a "jns 6" 7904
a "jnz 2" 7500
a "jo 2" 7000
a "jo 6" 7004
a "jp 2" 7a00
a "jp 6" 7a04
a "jpo 599" 0f8b51020000
a "js 2" 7800
a "js 6" 7804
a "jz 6" 7404
a "jz short 2" 7400
a "jnz short 6" 7504
a "jz short 5" 7403
a "jnz short -2" 75fc
a "jz short -52" 74ca
a "jnz short 23" 7515
a "jo short 32" 701e
a "jo short -62" 70c0
a "jno short 52" 7132
a "jno short -33" 71dd
a "js short 43" 7829
a "js short -73" 78b5
a "jns short -41" 79d5
a "jns short 63" 793d
a "je short 24" 7416
a "jne SHORT 84" 7552
a "jb short 23" 7215
a "jnae short 65" 723f
a "jc SHORT 37" 7223
a "jnb short 97" 735f
a "jae short 10" 7308
a "jnc short 0" 73fe
a "jbe short -12" 76f2
a "jna short 24" 7616
a "ja short 86" 7754
a "jnbe short 31" 771d
a "jl short 16" 7c0e
a "jnge short -40" 7cd6
a "jge short 52" 7d32
a "jnl short 76" 7d4a
a "jle short 54" 7e34
a "jng short -80" 7eae
a "jg short 56" 7f36
a "jnle short 2" 7f00
a "jp short -7" 7af7
a "jpe short 22" 7a14
a "jnp short 64" 7b3e
a "jpo short 88" 7b56
aB "lahf" 9e
aB "lar eax, word [eax]" 0f02
aB "lcall 0, 0" 9a
aB "lcall [0]" ff1c2500000000
aB "lcall [eax]" ff18
aB "lddqu xmm0, xmmword [eax]" f20ff000
aB "ldmxcsr [eax]" 0fae10
aB "lds eax, [eax]" c500
a "lea eax, [4]" 8d0504000000
a "lea eax, [eax+4]" 8d4004
a "lea eax, [eax]" 8d00
a "lea eax, [ebp+24]" 8d4518
a "lea eax, [ebx+24]" 8d4318
a "lea eax, [ebx+4]" 8d4304
a "lea eax, [ecx]" 8d01
a "lea eax, [esp]" 8d0424
a "lea ebx, [4]" 8d1d04000000
a "lea ebx, [eax+24]" 8d5818
a "lea ebx, [eax+4]" 8d5804
a "lea ebx, [ebp+324]" 8d9d44010000
a "lea ebx, [ebp]" 8d5d00
a "lea edx, [0x4422221d]" 8d151d222244
a "lea edx, 0x2c4b" 8d154b2c0000
a "leave" c9
a "les eax, [eax]" c400
a "les eax, [eax+12]" c4400c
a "les eax, [eax-233]" c48017ffffff
a "lfence" 0faee8
aB "lfs eax, dword [eax]" 0fb400
a "lgdt [eax]" 0f0110
aB "lgs eax, dword [eax]" 0fb500
a "lidt [eax]" 0f0118
a "lldt ax" 0f00d0
a "lldt word [eax]" 0f0010
a "lmsw ax" 0f01f0
a "lmsw word [eax]" 0f0130
aB "lock and word [fs:bx + si], si" 646766f02130
aB "lock cmpxchg8b" f00fc7c0
aB "lock mov dword [eax], eax" f08900
aB "lock mov eax, eax" f089c0
a "lodsb al, byte [esi]" ac
a "lodsd eax, dword [esi]" ad
aB "loop 3" 66e200
aB "lsl eax, dword [eax]" 0f03
aB "lss eax, dword [eax]" 0fb200
aB "ltr ax" 0f00d8
aB "ltr word [eax]" 0f0018
aB "lzcnt eax, dword [eax]" f30fbd00
aB "maskmovdqu xmm0, xmm0" 660ff7
aB "maskmovq mm0, mm0" 0ff7
aB "maxpd xmm0, xmmword [eax]" 660f5f00
aB "maxps xmm0, xmmword [eax]" 0f5f00
aB "maxsd xmm0, qword [eax]" f20f5f00
aB "maxss xmm0, dword [eax]" f30f5f00
a "mfence" 0faef0
aB "minpd xmm0, xmmword [eax]" 660f5d00
aB "minps xmm0, xmmword [eax]" 0f5d00
aB "minsd xmm0, qword [eax]" f20f5d00
aB "minss xmm0, dword [eax]" f30f5d00
a "monitor" 0f01c8
a "mov [33], ebp" 892d21000000
a "mov [33], ebx" 891d21000000
a "mov [33], ecx" 890d21000000
a "mov [33], edi" 893d21000000
a "mov [33], edx" 891521000000
a "mov [33], esi" 893521000000
a "mov [33], esp" 892521000000
a "mov ah, 0" b400
a "mov al, 0" b000
a "mov al, byte [0]" a000000000
a "mov al, byte [eax]" 8a00
a "mov al, [eax]" 8a00
aB "movapd xmm0, xmmword [eax]" 660f2800
aB "movapd xmmword [eax], xmm0" 660f2900
aB "movaps xmm0, xmmword [eax]" 0f2800
aB "movaps xmmword [eax], xmm0" 0f2900
aB "movbe dword [eax], eax" 0f38f100
aB "movbe eax, dword [eax]" 0f38f000
a "mov bh, 0" b700
a "mov bl, 0" b300
a "mov byte [0], al" 880500000000
a "mov ch, 0" b500
a "mov cl, 0" b100
a "mov cr0, eax" 0f22c0
aB "movddup xmm0, qword [eax]" f20f1200
aB "movd dword [eax], mm0" 0f7e00
aB "movd dword [eax], xmm0" 660f7e00
a "mov dh, 0" b600
a "mov dl, 0" b200
aB "movd mm0, dword [eax]" 0f6e00
aB "movdq2q mm0, xmm0" f20fd6
aB "movdqa xmm0, xmmword [eax]" 660f6f00
aB "movdqa xmmword [eax], xmm0" 660f7f00
aB "movdqu xmm0, xmmword [eax]" f30f6f00
aB "movdqu xmmword [eax], xmm0" f30f7f00
a "mov dr0, eax" 0f23c0
a "mov dword [0], eax" 890500000000
aB "mov dword cs:[eax], eax" 2e8900
aB "mov dword ds:[eax], eax" 3e8900
a "mov dword [eax], 0" c70000000000
a "mov dword [eax], 0x6f77206f" c7006f20776f
a "mov dword [eax+16], 0x6f77206f" c740106f20776f
a "mov dword [eax], 3" c70003000000
a "mov dword [eax+4], 1" c7400401000000
a "mov dword [eax+4], 3" c7400403000000
a "mov dword [eax+450], 0x6f77206f" c780c20100006f20776f
a "mov dword [eax+4], 666" c740049a020000
a "mov dword [eax-512], 421" c78000feffffa5010000
a "mov dword [eax], 666" c7009a020000
a "mov dword [eax], eax" 8900
a "mov dword [ebp-12], 1" c745f401000000
a "mov dword [ebp+16], 0x6f77206f" c745106f20776f
a "mov dword [ebp-312], 3" c785c8feffff03000000
a "mov dword [ebp+4], 1" c7450401000000
a "mov dword [ebp+450], 0x6f77206f" c785c20100006f20776f
aB "mov dword es:[eax], eax" 268900
a "mov dword [esi+4], 33" c7460421000000
a "mov dword [esp-312], 321" c78424c8feffff41010000
a "mov dword [esp], 3" c7042403000000
a "mov dword [esp+4], 1" c744240401000000
aB "mov dword fs:[eax], eax" 648900
aB "mov dword gs:[eax], eax" 658900
aB "mov dword ss:[eax], eax" 368900
aB "mov eax, dword fs:[1]" 648b042501000000
aB "movd xmm0, dword [eax]" 660f6e00
a "mov eax, 0" b800000000
a "mov [eax], 0" c70000000000
a "mov eax, 0x8049000" b800900408
a "mov eax, 1" b801000000
a "mov [eax+2], ebx" 895802
a "mov [eax+345], ebx" 899859010000
a "mov eax, 300" b82c010000
a "mov eax, 3" b803000000
a "mov [eax+4], eax" 894004
a "mov [eax+4], ecx" 894804
a "mov eax, cr0" 0f20c0
a "mov eax, dr0" 0f21c0
a "mov eax, dword [0]" a100000000
a "mov ecx, dword [0]" 8b0d00000000
a "mov ecx, dword [1]" 8b0d01000000
a "mov eax, dword [eax]" 8b00
a "mov eax, dword [ebp]" 8b4500
a "mov eax, dword [esp]" 8b0424
aB "mov eax, dword fs:[ebp]" 648b4500
a "mov eax, [eax+1337]" 8b8039050000
a "mov ecx, [eip+1337]" 8b0d39050000
a "mov ecx, [eip+13]" 8b0d0d000000
a "mov eax, [eax-1337]" 8b80c7faffff
a "mov eax,[eax*4+32]" 8b048520000000
a "mov eax,[eax*4-32]" 8b0485e0ffffff
a "mov eax,[eax*4+332]" 8b04854c010000
a "mov eax,[eax*4-332]" 8b0485b4feffff
a "mov eax, [eax+4]" 8b4004
a "mov eax, [eax-4]" 8b40fc
a "mov [eax], eax" 8900
a "mov byte [eax], al" 8800
a "mov eax, eax" 89c0
a "mov eax, [eax]" 8b00
a "mov [eax+eax], eax" 890400
aB "mov eax,[eax+ebx*4+32]" 8b449820
a "mov [eax+eax], ebx" 891c00
a "mov [eax+eax], ecx" 890c00
a "mov eax, [ebp]" 8b4500
a "mov [eax], ebx" 8918
a "mov eax, ebx" 89d8
a "mov eax, [ebx]" 8b03
a "mov eax,[ecx*8+64]" 8b04cd40000000
aB "mov [ecx*8+64], eax" 8904CD40000000
a "mov [eax+ecx], eax" 890408
a "mov eax, [esi]" 8b06
a "mov eax, [esp+4]" 8b442404
a "mov eax, esp" 89e0
a "mov eax, [esp]" 8b0424
a "mov ebp, 0" bd00000000
a "mov [ebp+4], eax" 898504000000
a "mov [ebp+4], ebx" 899d04000000
a "mov [ebp+4], ecx" 898d04000000
a "mov ebx, 0" bb00000000
a "mov [ebx+2], ebx" 895b02
a "mov [ebx-2], ecx" 894bfe
a "mov ebx, -3" bbfdffffff
a "mov [ebx+454], ebx" 899bc6010000
a "mov [ebx-552], edx" 8993d8fdffff
a "mov [ebx], eax" 8903
a "mov ebx, eax" 89c3
a "mov ebx, [eax]" 8b18
a "mov [ebx+eax], eax" 890403
a "mov ebx, [ecx + edx]" 8b1c11
a "mov ecx, 0" b900000000
a "mov ecx, -432" b950feffff
a "mov ecx, [eax]" 8b08
a "mov edi, 0" bf00000000
a "mov edx, 0" ba00000000
a "mov esi, 0" be00000000
a "mov esi, [esi + 8]" 8b7608
a "mov esp, 0" bc00000000
a "mov [esp-12], eax" 894424f4
a "mov [esp+2], ebx" 895c2402
a "mov [esp-2], ebx" 895c24fe
a "mov [esp-233], ebx" 899c2417ffffff
a "mov [esp+454], ebx" 899c24c6010000
aB "mov es, word [eax]" 8e00
aB "movhlps xmm0, xmm0" 0f12
aB "movhpd qword [eax], xmm0" 660f1700
aB "movhpd xmm0, qword [eax]" 660f1600
aB "movhps qword [eax], xmm0" 0f17
aB "movhps xmm0, qword [eax]" 0f16
aB "movlhps xmm0, xmm0" 0f16
aB "movlpd qword [eax], xmm0" 660f1300
aB "movlpd xmm0, qword [eax]" 660f1200
aB "movlps qword [eax], xmm0" 0f13
aB "movlps xmm0, qword [eax]" 0f12
aB "movmskpd eax, xmm0" 660f50c0
aB "movmskps eax, xmm0" 0f50c0
aB "movntdqa xmm0, xmmword [eax]" 660f382a00
aB "movntdq xmmword [eax], xmm0" 660fe700
aB "movnti dword [eax], eax" 0fc300
aB "movntpd xmmword [eax], xmm0" 660f2b00
aB "movntps xmmword [eax], xmm0" 0f2b00
aB "movntq qword [eax], mm0" 0fe700
aB "movq2dq xmm0, mm0" f30fd6
aB "movq mm0, qword [eax]" 0f6f00
aB "movq qword [eax], mm0" 0f7f00
aB "movq qword [eax], xmm0" 660fd600
aB "movq xmm0, qword [eax]" f30f7e00
a "movsb byte es:[edi], byte ptr [esi]" a4
a "movsd dword es:[edi], dword ptr [esi]" a5
aB "movsd dword es:[edi], dword ptr fs:[esi]" 64a5
aB "movsd qword [eax], xmm0" f20f1100
aB "movsd xmm0, qword [eax]" f20f1000
aB "movshdup xmm0, xmmword [eax]" f30f1600
aB "movsldup xmm0, xmmword [eax]" f30f1200
aB "movss dword [eax], xmm0" f30f1100
aB "movss xmm0, dword [eax]" f30f1000
a "movsx eax, byte [eax]" 0fbe00
a "movsx eax, word [eax]" 0fbf00
aB "movupd xmm0, xmmword [eax]" 660f1000
aB "movupd xmmword [eax], xmm0" 660f1100
aB "movups xmm0, xmmword [eax]" 0f10
aB "movups xmmword [eax], xmm0" 0f11
a "mov word [eax], es" 8c00
a "movzx eax, byte [eax]" 0fb600
a "movzx ecx, byte [esp]" 0fb60c24
a "movzx eax, word [eax]" 0fb700
a "movzx edx, word [esp]" 0fb71424
aB "mpsadbw xmm0, xmm0, 0" 660f3a42c000
a "mul byte [eax]" f620
aB "mulpd xmm0, xmmword [eax]" 660f5900
aB "mulpd xmm7, xmm7" 660f59ff
aB "mulps xmm0, xmmword [eax]" 0f5900
aB "mulps xmm7, xmm7" 0f59ff
aB "mulsd xmm0, qword [eax]" f20f5900
aB "mulsd xmm7, xmm7" 66f3f20f59ff
aB "mulsd xmm7, xmm7" f2660f59ff
aB "mulss xmm0, dword [eax]" f30f5900
aB "mulss xmm7, xmm7" 66f2f0f59ff0
a "mwait" 0f01c9
aB "neg byte [eax]" f618
a "nop" 90
aB "not byte [eax]" f610
aB "not al" f6d0
a "or al, 0" 0c00
a "or byte [eax], al" 0800
a "or dword [eax], eax" 0900
a "or eax, dword [eax]" 0b00
aB "orpd xmm0, xmmword [eax]" 660f5600
aB "orps xmm0, xmmword [eax]" 0f5600
a "out 0, al" e600
a "out 0, eax" e700
a "out 0x84, eax" e784
a "outsb dx, byte [esi]" 6e
a "outsd dx, dword [esi]" 6f
aB "pabsb xmm0, xmm0" 660f381cc0
aB "pabsd xmm0, xmm0" 660f381ec0
aB "pabsw xmm0, xmm0" 660f381dc0
aB "packssdw mm0, qword [eax]" 0f6b00
aB "packssdw xmm0, xmmword [eax]" 660f6b00
aB "packsswb mm0, qword [eax]" 0f6300
aB "packsswb xmm0, xmmword [eax]" 660f6300
aB "packusdw xmm0, xmm0" 660f382bc0
aB "packuswb mm0, qword [eax]" 0f6700
aB "packuswb xmm0, xmmword [eax]" 660f6700
aB "paddb mm0, qword [eax]" 0ffc00
aB "paddb xmm0, xmmword [eax]" 660ffc00
aB "paddd mm0, qword [eax]" 0ffe00
aB "paddd xmm0, xmmword [eax]" 660ffe00
aB "paddq xmm0, xmmword [eax]" 660fd400
aB "paddsb mm0, qword [eax]" 0fec00
aB "paddsb xmm0, xmmword [eax]" 660fec00
aB "paddsw mm0, qword [eax]" 0fed00
aB "paddsw xmm0, xmmword [eax]" 660fed00
aB "paddusb mm0, qword [eax]" 0fdc00
aB "paddusb xmm0, xmmword [eax]" 660fdc00
aB "paddusw mm0, qword [eax]" 0fdd00
aB "paddusw xmm0, xmmword [eax]" 660fdd00
aB "paddw mm0, qword [eax]" 0ffd00
aB "paddw xmm0, xmmword [eax]" 660ffd00
aB "palignr mm0, mm0, 0" 0f3a0fc000
aB "palignr xmm0, xmm0, 0" 660f3a0fc000
aB "pand mm0, qword [eax]" 0fdb00
aB "pandn mm0, qword [eax]" 0fdf00
aB "pandn xmm0, xmmword [eax]" 660fdf00
aB "pand xmm0, xmmword [eax]" 660fdb00
aB "pause" f390
aB "pavgb mm0, qword [eax]" 0fe000
aB "pavgb mm0, qword [eax]" 0fe0
aB "pavgb xmm0, xmmword [eax]" 660fe000
aB "pavgw mm0, qword [eax]" 0fe300
aB "pavgw xmm0, xmmword [eax]" 660fe300
aB "pblendvb xmm0, xmm0" 660f3810c0
aB "pblendw xmm0, xmm0, 0" 660f3a0ec000
aB "pclmulqdq xmm0, xmm0, 0" 660f3a44c000
aB "pcmpeqb mm0, qword [eax]" 0f7400
aB "pcmpeqb xmm0, xmmword [eax]" 660f7400
aB "pcmpeqd mm0, qword [eax]" 0f7600
aB "pcmpeqd xmm0, xmmword [eax]" 660f7600
aB "pcmpeqq xmm0, xmm0" 660f3829c0
aB "pcmpeqw mm0, qword [eax]" 0f7500
aB "pcmpeqw xmm0, xmmword [eax]" 660f7500
aB "pcmpestri xmm0, xmm0, 0" 660f3a61c000
aB "pcmpestrm xmm0, xmm0, 0" 660f3a60c000
aB "pcmpgtb mm0, qword [eax]" 0f6400
aB "pcmpgtb xmm0, xmmword [eax]" 660f6400
aB "pcmpgtd mm0, qword [eax]" 0f6600
aB "pcmpgtd xmm0, xmmword [eax]" 660f6600
aB "pcmpgtq xmm0, xmm0" 660f3837c0
aB "pcmpgtw mm0, qword [eax]" 0f6500
aB "pcmpgtw xmm0, xmmword [eax]" 660f6500
aB "pcmpistri xmm0, xmm0, 0" 660f3a63c000
aB "pcmpistrm xmm0, xmm0, 0" 660f3a62c000
aB "pextrb eax, xmm0, 0" 660f3a14c000
aB "pextrd eax, xmm0, 0" 660f3a16c000
aB "pextrq dword [eax], xmm0, 0" 660f3a16
aB "pextrw eax, mm0, 0" 0fc5c000
aB "pextrw eax, xmm0, 0" 660fc5c000
aB "phaddd xmm0, xmmword [eax]" 660f380200
aB "phaddsw xmm0, xmmword [eax]" 660f380300
aB "phaddw xmm0, xmmword [eax]" 660f380100
aB "phminposuw xmm0, xmm0" 660f3841c0
aB "phsubd xmm0, xmmword [eax]" 660f380600
aB "phsubsw xmm0, xmmword [eax]" 660f380700
aB "phsubw xmm0, xmmword [eax]" 660f380500
aB "pinsrb xmm0, eax, 0" 660f3a20c000
aB "pinsrd xmm0, dword [eax], 0" 660f3a22
aB "pinsrq xmm0, dword [eax], 0" 660f3a22
aB "pinsrw mm0, word [eax], 0x0" 0fc40000
aB "pinsrw xmm0, word [eax], 0x0" 660fc40000
aB "pmaddubsw xmm0, xmmword [eax]" 660f380400
aB "pmaddwd mm0, qword [eax]" 0ff500
aB "pmaddwd xmm0, xmmword [eax]" 660ff500
aB "pmaxsb xmm0, xmm0" 660f383cc0
aB "pmaxsd xmm0, xmm0" 660f383dc0
aB "pmaxsw mm0, qword [eax]" 0fee00
aB "pmaxsw xmm0, xmmword [eax]" 660fee00
aB "pmaxub mm0, qword [eax]" 0fde00
aB "pmaxub xmm0, xmmword [eax]" 660fde00
aB "pmaxud xmm0, xmm0" 660f383fc0
aB "pmaxuw xmm0, xmm0" 660f383ec0
aB "pminsb xmm0, xmm0" 660f3838c0
aB "pminsd xmm0, xmm0" 660f3839c0
aB "pminsw mm0, qword [eax]" 0fea00
aB "pminsw xmm0, xmmword [eax]" 660fea00
aB "pminub mm0, qword [eax]" 0fda00
aB "pminub xmm0, xmmword [eax]" 660fda00
aB "pminud xmm0, xmm0" 660f383bc0
aB "pminuw xmm0, xmm0" 660f383ac0
aB "pmovmskb eax, mm0" 0fd7
aB "pmovsxbd xmm0, xmm0" 660f3821c0
aB "pmovsxbq xmm0, xmm0" 660f3822c0
aB "pmovsxbw xmm0, xmm0" 660f3820c0
aB "pmovsxdq xmm0, xmm0" 660f3825c0
aB "pmovsxwd xmm0, xmm0" 660f3823c0
aB "pmovsxwq xmm0, xmm0" 660f3824c0
aB "pmovzxbd xmm0, xmm0" 660f3831c0
aB "pmovzxbq xmm0, xmm0" 660f3832c0
aB "pmovzxbw xmm0, xmm0" 660f3830c0
aB "pmovzxdq xmm0, xmm0" 660f3835c0
aB "pmovzxwd xmm0, xmm0" 660f3833c0
aB "pmovzxwq xmm0, xmm0" 660f3834c0
aB "pmuldq xmm0, xmm0" 660f3828c0
aB "pmulhrsw xmm0, xmm0" 660f380bc0
aB "pmulhuw mm0, qword [eax]" 0fe400
aB "pmulhuw xmm0, xmmword [eax]" 660fe400
aB "pmulhw mm0, qword [eax]" 0fe500
aB "pmulhw xmm0, xmmword [eax]" 660fe500
aB "pmulld xmm0, xmm0" 660f3840c0
aB "pmullw mm0, qword [eax]" 0fd500
aB "pmullw xmm0, xmmword [eax]" 660fd500
aB "pmuludq mm0, qword [eax]" 0ff400
aB "pmuludq xmm0, xmmword [eax]" 660ff400
a "popal" 61
a "popaw" 6661
aB "popcnt eax, qword [eax]" f30fb8
a "pop ds" 1f
a "pop dword [eax+4]" 8f4004
a "pop dword [eax]" 8f00
a "pop dword [ebp+4]" 8f4504
a "pop dword [ebp]" 8f4500
a "pop dword [ecx]" 8f01
a "pop dword [edi]" 8f07
a "pop dword [esi]" 8f06
a "pop dword [esp]" 8f0424
a "pop eax" 58
a "pop ebp" 5d
a "pop ebx" 5b
a "pop ecx" 59
a "pop edi" 5f
a "pop edx" 5a
a "pop es" 07
a "pop esi" 5e
a "pop esp" 5c
a "popfd" 9d
a "pop fs" 0fa1
a "pop gs" 0fa9
a "pop ss" 17
aB "por mm0, qword [eax]" 0feb00
aB "por xmm0, xmmword [eax]" 660feb00
aB "prefetch byte [eax]" 0f0d00
aB "prefetchnta byte [eax]" 0f1800
aB "prefetcht0 byte [eax]" 0f1808
aB "prefetcht1 byte [eax]" 0f1810
aB "prefetcht2 byte [eax]" 0f1818
aB "psadbw mm0, qword [eax]" 0ff600
aB "psadbw xmm0, xmmword [eax]" 660ff600
aB "pshufb mm0, qword [eax]" 0f380000
aB "pshufb xmm0, xmmword [eax]" 660f380000
aB "pshufd xmm0, xmmword [eax], 0" 660f700000
aB "pshufhw xmm0, xmmword [eax], 0" f30f700000
aB "pshuflw xmm0, xmmword [eax], 0" f20f700000
aB "pshufw mm0, qword [eax], 0" 0f700000
aB "psignb xmm0, xmm0" 660f3808c0
aB "psignd xmm0, xmm0" 660f380ac0
aB "psignw xmm0, xmm0" 660f3809c0
aB "pslld mm0, 0" 0f72f000
aB "pslld mm0, qword [eax]" 0ff200
aB "pslldq xmm0, 0" 660f73f800
aB "pslld xmm0, 0" 660f72f000
aB "pslld xmm0, xmmword [eax]" 660ff200
aB "psllq mm0, 0" 0f73f000
aB "psllq mm0, qword [eax]" 0ff300
aB "psllq xmm0, 0" 660f73f000
aB "psllq xmm0, xmmword [eax]" 660ff300
aB "psllw mm0, 0" 0f71f000
aB "psllw mm0, qword [eax]" 0ff100
aB "psllw xmm0, 0" 660f71f000
aB "psllw xmm0, xmmword [eax]" 660ff100
aB "psrad mm0, 0" 0f72e000
aB "psrad mm0, qword [eax]" 0fe200
aB "psrad xmm0, 0" 660f72e000
aB "psrad xmm0, xmmword [eax]" 660fe200
aB "psraw mm0, 0" 0f71e000
aB "psraw mm0, qword [eax]" 0fe100
aB "psraw xmm0, 0" 660f71e000
aB "psraw xmm0, xmmword [eax]" 660fe100
aB "psrld mm0, 0" 0f72d000
aB "psrld mm0, qword [eax]" 0fd200
aB "psrldq xmm0, 0" 660f73d800
aB "psrld xmm0, 0" 660f72d000
aB "psrld xmm0, xmmword [eax]" 660fd200
aB "psrlq mm0, 0" 0f73d000
aB "psrlq mm0, qword [eax]" 0fd300
aB "psrlq xmm0, 0" 660f73d000
aB "psrlq xmm0, xmmword [eax]" 660fd300
aB "psrlw mm0, 0" 0f71d000
aB "psrlw mm0, qword [eax]" 0fd100
aB "psrlw xmm0, 0" 660f71d000
aB "psrlw xmm0, xmmword [eax]" 660fd100
aB "psubb mm0, qword [eax]" 0ff800
aB "psubb xmm0, xmmword [eax]" 660ff800
aB "psubd mm0, qword [eax]" 0ffa00
aB "psubd xmm0, xmmword [eax]" 660ffa00
aB "psubq mm0, qword [eax]" 0ffb00
aB "psubq xmm0, xmmword [eax]" 660ffb00
aB "psubsb mm0, xmmword [eax]" 0fe800
aB "psubsb xmm0, xmmword [eax]" 660fe800
aB "psubsw mm0, xmmword [eax]" 0fe900
aB "psubsw xmm0, xmmword [eax]" 660fe900
aB "psubusb mm0, qword [eax]" 0fd800
aB "psubusb xmm0, xmmword [eax]" 660fd800
aB "psubusw mm0, qword [eax]" 0fd900
aB "psubusw xmm0, xmmword [eax]" 660fd900
aB "psubw mm0, qword [eax]" 0ff900
aB "psubw xmm0, xmmword [eax]" 660ff900
aB "ptest xmm0, xmm0" 660f3817c0
aB "punpckhbw mm0, qword [eax]" 0f6800
aB "punpckhbw xmm0, xmmword [eax]" 660f6800
aB "punpckhdq mm0, qword [eax]" 0f6a00
aB "punpckhdq xmm0, xmmword [eax]" 660f6a00
aB "punpckhqdq xmm0, xmmword [eax]" 660f6d00
aB "punpckhwd mm0, qword [eax]" 0f6900
aB "punpckhwd xmm0, xmmword [eax]" 660f6900
aB "punpcklbw mm0, qword [eax]" 0f6000
aB "punpcklbw xmm0, xmmword [eax]" 660f6000
aB "punpckldq mm0, qword [eax]" 0f6200
aB "punpckldq xmm0, xmmword [eax]" 660f6200
aB "punpcklqdq xmm0, xmmword [eax]" 660f6c00
aB "punpcklwd mm0, qword [eax]" 0f6100
aB "punpcklwd xmm0, xmmword [eax]" 660f6100
a "push 0" 6a00
a "pushal" 60
a "push cs" 0e
a "push ds" 1e
a "push dword [eax+8]" ff7008
a "push dword [eax]" ff30
a "push dword [ebp+4]" ff7504
a "push dword [ebp]" ff7500
a "push dword [ebx+4]" ff7304
a "push dword [ecx]" ff31
a "push dword [edi]" ff37
a "push dword [esi+4]" ff7604
a "push dword [esi]" ff36
a "push dword [esp+4]" ff742404
a "push dword [esp]" ff3424
a "push [esp+4]" ff742404
a "push [esp]" ff3424
a "push eax" 50
a "push ebp" 55
a "push ebx" 53
a "push ecx" 51
a "push edi" 57
a "push edx" 52
a "push es" 06
a "push esi" 56
a "push esp" 54
a "pushfd" 9c
a "push fs" 0fa0
a "push gs" 0fa8
a "push ss" 16
aB "pxor mm0, qword [eax]" 0fef00
aB "pxor xmm0, xmmword [eax]" 660fef00
aB "rcpps xmm0, xmmword [eax]" 0f5300
aB "rcpss xmm0, dword [eax]" f30f5300
a "rdmsr" 0f32
a "rdpmc" 0f33
a "rdtsc" 0f31
a "rdtscp" 0f01f9
a "repne movsb byte es:[edi], byte ptr [esi]" f2a4
a "repz movsb" f3a4
a "ret" c3
a "bnd ret" f2c3
a "retf 0" ca0000
a "retf" cb
a "retw" 66c3
a "rol byte [eax], 0" c00000
a "rol byte [eax], 1" d000
a "rol byte [eax], cl" d200
a "rol dword [eax], 0" c10000
a "rol dword [eax], 1" d100
a "rol dword [eax], cl" d300
aB "roundpd xmm0, xmm0, 0" 660f3a09c000
aB "roundps xmm0, xmm0, 0" 660f3a08c000
aB "roundsd xmm0, xmm0, 0" 660f3a0bc000
aB "roundss xmm0, xmm0, 0" 660f3a0ac000
a "rsm" 0faa
aB "rsqrtps xmm0, xmmword [eax]" 0f5200
aB "rsqrtss xmm0, dword [eax]" f30f5200
a "sahf" 9e
a "salc" d6
a "sbb al, 0" 1c00
a "sbb al, byte [eax]" 1a00
a "sbb byte [eax], al" 1800
a "sbb dword [eax], eAX" 1900
a "sbb eax, dword [eax]" 1b00
a "scasb al, byte es:[edi]" ae
a "scasd eax, dword es:[edi]" af
a "seta byte [eax]" 0f9700
a "setae byte [eax]" 0f9300
a "setb byte [eax]" 0f9200
a "setbe byte [eax]" 0f9600
a "sete byte [eax]" 0f9400
a "setg byte [eax]" 0f9f00
a "setge byte [eax]" 0f9d00
a "setl byte [eax]" 0f9c00
a "setle byte [eax]" 0f9e00
a "setne byte [eax]" 0f9500
a "setno byte [eax]" 0f9100
a "setnp byte [eax]" 0f9b00
a "setns byte [eax]" 0f9900
a "seto byte [eax]" 0f9000
a "setp byte [eax]" 0f9a00
a "sets byte [eax]" 0f9800
a "sfence" 0faef8
a "sgdt [eax]" 0f0100
aB "shld dword [eax], eax, 0" 0fa40000
aB "shld dword [eax], eax, cl" 0fa500
a "shl edx, 5" c1e205
aB "shrd dword [eax], eax, 0" 0fac0000
aB "shrd dword [eax], eax, cl" 0fad00
aB "shufpd xmm0, xmmword [eax], 0x0" 660fc60000
aB "shufps xmm0, xmmword [eax], 0" 0fc60000
a "sidt [eax]" 0f0108
aB "skinit" 0f01de
a "sldt word [eax]" 0f0000
aB "smsw ax" 660f01e0
a "smsw eax" 0f01e0
a "smsw word [eax]" 0f0120
aB "sqrtpd xmm0, xmmword [eax]" 660f5100
aB "sqrtps xmm0, xmmword [eax]" 0f5100
aB "sqrtsd xmm0, qword [eax]" f20f5100
aB "sqrtss xmm0, dword [eax]" f30f5100
a "stc" f9
a "std" fd
a "stgi" 0f01dc
a "sti" fb
a "stmxcsr dword [eax]" 0fae18
a "stosb byte es:[edi], al" aa
a "stosd dword es:[edi], eax" ab
a "str word [eax]" 0f0008
a "sub al, 0" 2c00
a "sub al, byte [eax]" 2a00
a "sub byte [eax], al" 2800
a "sub dword [eax], 1" 832801
a "sub dword [eax+4], -666" 81680466fdffff
a "sub dword [eax+4], 666" 8168049a020000
a "sub dword [eax+666], 666" 81a89a0200009a020000
a "sub dword [eax], 666" 81289a020000
a "sub dword [eax], eax" 2900
a "sub dword [ebp+4], 1" 836d0401
a "sub dword [ebp+555], 1" 83ad2b02000001
a "sub dword [ebp+555], 7357" 81ad2b020000bd1c0000
a "sub dword [ebp-555], 7357" 81add5fdffffbd1c0000
a "sub dword [ebx], 1" 832b01
a "sub eax, 3" 83e803
a "sub eax, -666" 2d66fdffff
a "sub eax, 666" 2d9a020000
a "sub eax, dword [eax]" 2b00
a "sub eax, eax" 29c0
a "sub eax, ebx" 29d8
a "sub ebx, 3" 83eb03
a "sub ebx, -3" 83ebfd
a "sub ebx, 666" 81eb9a020000
a "sub [ebx], eax" 2903
a "sub ebx, eax" 29c3
a "sub ecx, 666" 81e99a020000
a "sub esi,-334" 81eeb2feffff
aB "subpd xmm0, xmmword [eax]" 660f5c00
aB "subps xmm0, xmmword [eax]" 0f5c00
aB "subsd xmm0, qword [eax]" f20f5c00
aB "subss xmm0, dword [eax]" f30f5c00
a "swapgs" 0f1ff8
a "syscall" 0f05
a "sysenter" 0f34
a "sysexit" 0f35
a "sysret" 0f07
a "test al, 0" f6c000
a "test byte [eax], 0" f60000
a "test byte [eax], al" 8400
a "test dword [eax], 0" f70000000000
a "test dword [eax], eax" 8500
a "test eax, 0" f7c000000000
a "test eax, ebx" 85d8
a "test edx, esi" 85f2
aB "ucomisd xmm0, qword [eax]" 660f2e00
aB "ucomiss xmm0, dword [eax]" 0f2e00
a "ud2" 0f0b
aB "unpckhpd xmm0, xmmword [eax]" 660f1500
aB "unpckhps xmm0, xmmword [eax]" 0f15
aB "unpcklpd xmm0, xmmword [eax]" 660f1400
aB "unpcklps xmm0, xmmword [eax]" 0f14
aB "vaddpd ymm0, ymm0, ymm0" c5fd58c0
aB "vaesdeclast xmm0, xmm0, xmm0" c4e279dfc0
aB "vaesdec xmm0, xmm0, xmm0" c4e279dec0
aB "vaesenclast xmm0, xmm0, xmm0" c4e279ddc0
aB "vaesenc xmm0, xmm0, xmm0" c4e279dcc0
aB "vaesimc xmm0, xmm0" c4e279dbc0
aB "vaeskeygenassist xmm0, xmm0, 0" c4e379dfc000
aB "vaeskeygenassist xmm0, xmm0, 0x0" c4e379dfc000
aB "vbroadcastf128 ymm0, xmmword [0]" c4e27d1a0500000000
aB "vbroadcastsd ymm0, qword [0]" c4e27d190500000000
aB "vbroadcastss ymm0, dword [eax]" c4e27d1800
aB "vcvtph2ps xmm0, xmm0, 0" 8fe878a0c000
aB "vcvtps2ph xmm0, xmm0, 0" 8fe878a1c000
a "verr ax" 0f00e0
aB "verr [eax]" 0f0020
a "verw ax" 0f00e8
a "verw word [eax]" 0f0028
aB "vextractf128 xmm0, ymm0, 0" c4e37d19c000
aB "vextractf128 xmm0, ymm0, 0x0" c4e37d19c000
aB "vfmadd132pd xmm0, xmm0, xmm0" c4e2f998c0
aB "vfmadd213pd xmm0, xmm0, xmm0" c4e2f9a8c0
aB "vfmadd231pd xmm0, xmm0, xmm0" c4e2f9b8c0
aB "vfmaddpd xmm0, xmm0, xmm0, xmm0" c4e37969c000
aB "vfmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d69c000
aB "vfmaddps xmm0, xmm0, xmm0, xmm0" c4e37968c000
aB "vfmaddps ymm0, ymm0, ymm0, ymm0" c4e37d68c000
aB "vfmaddsd xmm0, xmm0, xmm0, xmm0" c4e3796bc000
aB "vfmaddss xmm0, xmm0, xmm0, xmm0" c4e3796ac000
aB "vfmaddsubpd xmm0, xmm0, xmm0, xmm0" c4e3795dc000
aB "vfmaddsubpd ymm0, ymm0, ymm0, ymm0" c4e37d5dc000
aB "vfmaddsubps xmm0, xmm0, xmm0, xmm0" c4e3795cc000
aB "vfmaddsubps ymm0, ymm0, ymm0, ymm0" c4e37d5cc000
aB "vfmsubaddpd xmm0, xmm0, xmm0, xmm0" c4e3795fc000
aB "vfmsubaddpd ymm0, ymm0, ymm0, ymm0" c4e37d5fc000
aB "vfmsubaddps xmm0, xmm0, xmm0, xmm0" c4e3795ec000
aB "vfmsubaddps ymm0, ymm0, ymm0, ymm0" c4e37d5ec000
aB "vfmsubpd xmm0, xmm0, xmm0, xmm0" c4e3796dc000
aB "vfmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d6dc000
aB "vfmsubps xmm0, xmm0, xmm0, xmm0" c4e3796cc000
aB "vfmsubps ymm0, ymm0, ymm0, ymm0" c4e37d6cc000
aB "vfmsubsd xmm0, xmm0, xmm0, xmm0" c4e3796fc000
aB "vfmsubss xmm0, xmm0, xmm0, xmm0" c4e3796ec000
aB "vfnmaddpd xmm0, xmm0, xmm0, xmm0" c4e37979c000
aB "vfnmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d79c000
aB "vfnmaddps xmm0, xmm0, xmm0, xmm0" c4e37978c000
aB "vfnmaddps ymm0, ymm0, ymm0, ymm0" c4e37d78c000
aB "vfnmaddsd xmm0, xmm0, xmm0, xmm0" c4e3797bc000
aB "vfnmaddss xmm0, xmm0, xmm0, xmm0" c4e3797ac000
aB "vfnmsubpd xmm0, xmm0, xmm0, xmm0" c4e3797dc000
aB "vfnmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d7dc000
aB "vfnmsubps xmm0, xmm0, xmm0, xmm0" c4e3797cc000
aB "vfnmsubps ymm0, ymm0, ymm0, ymm0" c4e37d7cc000
aB "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000
aB "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000
aB "vfrczpd xmm0, xmm0" 8fe97881c0
aB "vfrczps xmm0, xmm0" 8fe97880c0
aB "vfrczsd xmm0, xmm0" 8fe97883c0
aB "vfrczss xmm0, xmm0" 8fe97882c0
aB "vinsertf128 ymm0, ymm0, xmm0, 0" c4e37d18c000
aB "vinsertf128 ymm0, ymm0, xmm0, 0x0" c4e37d18c000
aB "vmaskmovpd ymm0, ymm0, ymmword [0]" c4e27d2d0500000000
aB "vmaskmovps ymm0, ymm0, ymmword [0]" c4e27d2c0500000000
a "vmcall" 0f01c1
a "vmclear qword [eax]" 660fc730
a "vmlaunch" 0f01c2
a "vmload" 0f01da
a "vmmcall" 0f01d9
a "vmptrld qword [eax]" 0fc730
a "vmptrst qword [eax]" 0fc738
a "vmresume" 0f01c3
a "vmrun" 0f01d8
a "vmsave" 0f01db
a "vmxoff" 0f01c4
a "vmxon qword [eax]" f30fc730
aB "vpcmov xmm0, xmm0, xmm0, xmm0" 8fe878a2c000
aB "vpcomb xmm0, xmm0, xmm0, 0" 8fe878ccc000
aB "vpcomd xmm0, xmm0, xmm0, 0" 8fe878cec000
aB "vpcomq xmm0, xmm0, xmm0, 0" 8fe878cfc000
aB "vpcomub xmm0, xmm0, xmm0, 0" 8fe878ecc000
aB "vpcomud xmm0, xmm0, xmm0, 0" 8fe878eec000
aB "vpcomuq xmm0, xmm0, xmm0, 0" 8fe878efc000
aB "vpcomuw xmm0, xmm0, xmm0, 0" 8fe878edc000
aB "vpcomw xmm0, xmm0, xmm0, 0" 8fe878cdc000
aB "vperm2f128 ymm0, ymm0, ymm0, 0" c4e37d06c000
aB "vperm2f128 ymm0, ymm0, ymm0, 0x0" c4e37d06c000
aB "vpermilpd ymm0, ymm0, ymmword [0]" c4e27d0d0500000000
aB "vpermilps ymm0, ymm0, ymmword [0]" c4e27d0c0500000000
aB "vphaddbd xmm0, xmm0" 8fe978c2c0
aB "vphaddbq xmm0, xmm0" 8fe978c3c0
aB "vphaddbw xmm0, xmm0" 8fe978c1c0
aB "vphadddq xmm0, xmm0" 8fe978cbc0
aB "vphaddubd xmm0, xmm0" 8fe978d2c0
aB "vphaddubq xmm0, xmm0" 8fe978d3c0
aB "vphaddubw xmm0, xmm0" 8fe978d1c0
aB "vphaddudq xmm0, xmm0" 8fe978dbc0
aB "vphadduwd xmm0, xmm0" 8fe978d6c0
aB "VPHADDUWQ XMM0, XMM0" 8fe978d7c0
aB "vphaddwd xmm0, xmm0" 8fe978c6c0
aB "vphaddwq xmm0, xmm0" 8fe978c7c0
aB "vphsubbw xmm0, xmm0" 8fe978e1c0
aB "vphsubdq xmm0, xmm0" 8fe978e3c0
aB "vphsubwd xmm0, xmm0" 8fe978e2c0
aB "vpmacsddxmm0, xmm0, xmm0, xmm0" 8fe8789ec000
aB "vpmacsdqh xmm0, xmm0, xmm0, xmm0" 8fe8789fc000
aB "vpmacsdql xmm0, xmm0, xmm0, xmm0" 8fe87897c000
aB "vpmacssdd xmm0, xmm0, xmm0, xmm0" 8fe8788ec000
aB "vpmacssdqh xmm0, xmm0, xmm0, xmm0" 8fe8788fc000
aB "vpmacssdql xmm0, xmm0, xmm0, xmm0" 8fe87887c000
aB "vpmacsswd xmm0, xmm0, xmm0, xmm0" 8fe87886c000
aB "vpmacssww xmm0, xmm0, xmm0, xmm0" 8fe87885c000
aB "vpmacswd xmm0, xmm0, xmm0, xmm0" 8fe87896c000
aB "vpmacsww xmm0, xmm0, xmm0, xmm0" 8fe87895c000
aB "vpmadcsswd xmm0, xmm0, xmm0, xmm0" 8fe878a6c000
aB "VPMADCSSWD XMM0, XMM0, XMM0, XMM0" 8fe878a6c000
aB "vpmadcswd xmm0, xmm0, xmm0, xmm0" 8fe878b6c000
aB "vpperm xmm0, xmm0, xmm0, xmm0" 8fe878a3c000
aB "vprotb xmm0, xmm0, xmm0" 8fe97890c0
aB "vprotd xmm0, xmm0, xmm0" 8fe97892c0
aB "vprotq xmm0, xmm0, xmm0" 8fe97893c0
aB "vprotw xmm0, xmm0, xmm0" 8fe97891c0
aB "vpshab xmm0, xmm0, xmm0" 8fe97898c0
aB "vpshad xmm0, xmm0, xmm0" 8fe9789ac0
aB "vpshaq xmm0, xmm0, xmm0" 8fe9789bc0
aB "vpshaw xmm0, xmm0, xmm0" 8fe97899c0
aB "vpshlb xmm0, xmm0, xmm0" 8fe97894c0
aB "vpshld xmm0, xmm0, xmm0" 8fe97896c0
aB "vpshlq xmm0, xmm0, xmm0" 8fe97897c0
aB "vpshlw xmm0, xmm0, xmm0" 8fe97895c0
aB "vtestpd ymm0, ymm0" c4e27d0fc0
aB "vtestps ymm0, ymm0" c4e27d0ec0
a "vzeroall" c5fc77
a "vzeroupper" c5f877
a "wbinvd" 0f09
a "wrmsr" 0f30
aB "xadd byte [eax], al" 0fc000
aB "xadd dword [eax], eax" 0fc100
aB "xchg byte [eax], al" 8600
a "xchg dword [eax], eax" 8700
ad "xchg al, dl" 86d0
ad "xchg dl, al" 86c2
ad "xchg ax, dx" 6692
a "xchg dx, ax" 6692
ad "xchg ah, dh" 86f4
ad "xchg dh, ah" 86e6
a "xchg eax, eax" 90
ad "xchg eax, ebp" 95
ad "xchg eax, ebx" 93
ad "xchg eax, ebx" 93
ad "xchg eax, ecx" 91
ad "xchg eax, edi" 97
ad "xchg eax, edx" 92
ad "xchg eax, esi" 96
ad "xchg eax, esp" 94
ad "xchg ebx, ecx" 87cb
ad "xchg ecx, ebp" 87e9
ad "xchg ecx, ebx" 87d9
ad "xchg ecx, ecx" 87c9
a "xgetbv" 0f01d0
a "xlatb" d7
a "xor al, 0" 3400
a "xor al, 0x80" 3480
a "xor ax, 0x8080" 66358080
a "xor ax, 0x8" 6683f008
a "xor cx, 0x8080" 6681f18080
a "xor sp, 0x8080" 6681f48080
a "xor bp, 0x8080" 6681f58080
a "xor si, 0x8" 6683f608
a "xor al, byte [eax]" 3200
a "xor byte [eax], al" 3000
a "xor byte [eax], 0xff" 8030ff
a "xor dword [eax], eax" 3100
a "xor eax, dword [eax]" 3300
a "xor [eax], eax" 3100
a "xor eax, eax" 31c0
a "xor eax, ebx" 31d8
a "xor ebx, eax" 31c3
a "xor esi, ebp" 31ee
a "xor esp,esp" 31e4
aB "xorpd xmm0, xmmword [eax]" 660f5700
aB "xorps xmm0, xmmword [eax]" 0f5700
aB "xrstor [eax]" 0fae28
aB "xsave [eax]" 0fae20
a "xsetbv" 0f01d1
a "nop" 90
a "int 0x80" cd80
a "mov eax, 33" b821000000
a "mov rax, 33" 48c7c021000000
a "mov [ebp+4],0" c7450400000000
a "jmp 0x1b" eb05 0x14
ad "sete al" 0f94c0
a "mov byte ptr [bp+di],0x0" 67c60300
a "mov byte ptr [bp+di-0x1],0x20" 67c643ff20
a "mov byte ptr [bp+di],0x25" 67c60325
a "mov byte ptr [bp+di],0x30" 67c60330
a "mov byte ptr [bp+si-0x1],0x30" 67c642ff30
a "mov byte ptr [bx],0x0" 67c60700
a "mov byte ptr [bx+si+0x3e06],0x0" 67c680063e00
a "mov byte ptr [esi],0x7f" c6067f
a "mov byte ptr [esi],0x86" c60686
a "mov byte ptr [esp+0x25],0xc0" c6442425c0
a "mov byte ptr [si],0x11" 67c60411
a "mov byte ptr [si],0x13" 67c60413
a "mov byte ptr [si+0x24],0x14" 67c6442414
a "mov byte ptr [si+0x24],0x18" 67c6442418
a "mov byte ptr [si+0x24],0x1a" 67c644241a
a "mov byte ptr [si+0x24],0x25" 67c6442425
a "mov byte ptr [si+0x24],0x2e" 67c644242e
a "mov byte ptr [si+0x24],0x44" 67c6442444
a "mov byte ptr [si],0x24" 67c60424
a "mov dword ptr [bx+si+0x6],0x8b640000" 67c740060000648b
a "mov dword ptr [eax+eax*1],0xa740000" c704000000740a
a "mov dword ptr [ebp-0x44],0x31660305" c745bc05036631
a "mov dword ptr [ebp-0x4c],0x47534943" c745b443495347
a "mov dword ptr [edx],0x74000000" c70200000074
a "mov dword ptr [esi],0x15078" c70678500100
a "mov dword ptr [esi],0x404020" c70620404000
a "mov dword ptr [esi],0xb0003e04" c706043e00b0
a "mov dword ptr [esi],0xb8003e04" c706043e00b8
a "mov dword ptr [esp+0x1c],0x534d4150" c744241c50414d53
a "mov dword ptr [esp+0x1c],0xc6670001" c744241c010067c6
a "mov dword ptr [esp],0x1" c7042401000000
a "mov dword ptr [esp+0x20],0x66670014" c744242014006766
a "mov dword ptr [esp+0x24],0x66670f00" c7442424000f6766
a "mov dword ptr [esp+0x24],0x66671a00" c7442424001a6766
a "mov dword ptr [esp+0x4],0x0" c744240400000000
a "mov dword ptr [esp+0xc],0x1" c744240c01000000
a "mov dword ptr [esp+0xc],0x3" c744240c03000000
a "mov dword ptr [si+0x24],0x6606071c" 67c744241c070666
a "mov dword ptr [si+0x24],0x660b0c1c" 67c744241c0c0b66
a "mov dword ptr [si+0x24],0x66111120" 67c7442420111166
a "mov dword ptr [si+0x24],0x66111220" 67c7442420121166
a "mov dword ptr [si+0x24],0x66240120" 67c7442420012466
a "mov dword ptr [si+0x24],0x6700002a" 67c744242a000067
a "mov dword ptr [si+0x24],0x67000714" 67c7442414070067
a "mov dword ptr [si+0x24],0x674f0134" 67c7442434014f67
a "mov dword ptr [si+0x24],0x67e80124" 67c744242401e867
a "mov dword ptr [si+0x24],0x67e82024" 67c744242420e867
a "mov word ptr [bp+di+0x10],0x0" 6766c743100000
a "mov word ptr [bx+si],0x5" 6766c7000500
a "mov word ptr [esi],0x3d04" 66c706043d
a "mov word ptr [esi],0x4020" 66c7062040
a "mov word ptr [esi],0x5078" 66c7067850
a "mov word ptr [esi],0x5084" 66c7068450
a "mov word ptr [esp+0x10],0x0" 66c74424100000
a "mov word ptr [esp+0x14],0x0" 66c74424140000
a "mov word ptr [si+0x24],0x4" 6766c744240400
a "mov word ptr [si+0x24],0x8" 6766c744240800
a "mov word ptr [si+0x24],0xff04" 6766c7442404ff
a "mov word ptr [si],0x24" 6766c7042400
a "mov eax, [eax * 2 + 8]" 8b044508000000
a "inc al" fec0
a "inc ax" 6640
a "inc BYTE PTR [ebx+0x18]" fe4318
a "inc BYTE PTR [edi+0x18]" fe4718
a "inc BYTE PTR [esi+0x1a]" fe461a
a "inc cl" fec1
a "inc dl" fec2
a "inc DWORD PTR [eax]" ff00
a "inc DWORD PTR [eax+0x14c]" ff804c010000
a "inc DWORD PTR [ebp+0x10]" ff4510
a "inc DWORD PTR [ebx]" ff03
a "inc DWORD PTR [ebx+0x18]" ff4318
a "inc DWORD PTR [ebx+0x20]" ff4320
a "inc DWORD PTR [ecx]" ff01
a "inc DWORD PTR [ecx+0x4]" ff4104
a "inc DWORD PTR [edi]" ff07
a "inc DWORD PTR [edi+0x28]" ff4728
a "inc DWORD PTR [edx]" ff02
a "inc DWORD PTR [edx+0x10]" ff4210
a "inc DWORD PTR [esi+0x8]" ff4608
a "inc DWORD PTR [esp]" ff0424
a "inc DWORD PTR [esp+0x10]" ff442410
a "inc eax" 40
a "inc ebp" 45
a "inc ebx" 43
a "inc ecx" 41
a "inc edi" 47
a "inc edx" 42
a "dec al" fec8
a "dec ax" 6648
a "dec BYTE PTR [ebx+0x18]" fe4b18
a "dec BYTE PTR [edi+0x18]" fe4f18
a "dec BYTE PTR [esi+0x1a]" fe4e1a
a "dec cl" fec9
a "dec dl" feca
a "dec DWORD PTR [eax]" ff08
a "dec DWORD PTR [eax+0x14c]" ff884c010000
a "dec DWORD PTR [ebp+0x10]" ff4d10
a "dec DWORD PTR [ebx]" ff0b
a "dec DWORD PTR [ebx+0x18]" ff4b18
a "dec DWORD PTR [ebx+0x20]" ff4b20
a "dec DWORD PTR [ecx]" ff09
a "dec DWORD PTR [ecx+0x4]" ff4904
a "dec DWORD PTR [edi]" ff0f
a "dec DWORD PTR [edi+0x28]" ff4f28
a "dec DWORD PTR [edx]" ff0a
a "dec DWORD PTR [edx+0x10]" ff4a10
a "dec DWORD PTR [esi+0x8]" ff4e08
a "dec DWORD PTR [esp]" ff0c24
a "dec DWORD PTR [esp+0x10]" ff4c2410
a "dec eax" 48
a "dec ebp" 4d
a "dec ebx" 4b
a "dec ecx" 49
a "dec edi" 4f
a "dec edx" 4a
