a "aaa" 37 
a "aad" d50a 
a "aam" d40a 
a "aas" 3f 
a "adc al, 0" 1400 
a "adc al, byte [eax]" 1200 
a "adc byte [eax], al" 1000 
a "adc dword [eax], eax" 1100 
a "adc eax, dword [eax]" 1300 
a "add al, 0" 0400 
a "add al, byte [eax]" 0200 
a "add byte [bx + si], al" 670000 
a "add byte [eax], 0" 800000 
aB "add byte [eax], 0" 820000 
aB "add byte [eax], al" 00000000 
a "add byte [eax], al" 0000 
a "add dword [eax], 1" 830001
a "add dword [eax+8], 1" 83400801
a "add dword [eax], eax" 0100
a "add dword [ebp+4], 1" 83450401
a "add dword [ebp+8], 1" 83450801
a "add dword [ebx], 1" 830301
a "add dword [ebx+8], 1" 83430801
a "add dword [esp+8], 1" 8344240801
a "add eax, 1" 83c001
a "add eax, 3" 83c003
a "add eax, dword [eax]" 0300 
a "add [eax], eax" 0100
a "add esi,-334" 81c6b2feffff
a "addpd xmm0, xmmword [eax]" 660f5800 
a "addps xmm0, xmmword [eax]" 0f5800 
a "addsd xmm0, qword [eax]" f20f5800 
a "addss xmm0, dword [eax]" f30f5800 
a "addsubpd xmm0, xmmword [eax]" 660fd000 
a "addsubps xmm0, xmmword [eax]" f20fd000 
aB "adx" d4 
a "aesdeclast xmm0, xmm0" 660f38dfc0 
a "aesdec xmm0, xmm0" 660f38dec0 
a "aesenclast xmm0, xmm0" 660f38ddc0 
a "aesenc xmm0, xmm0" 660f38dcc0 
a "aesimc xmm0, xmm0" 660f38dbc0 
a "aeskeygenassist xmm0, xmm0, 0x0" 660f3adfc000 
aB "amx" d5 
a "and al, 0" 2400 
a "and al, byte [eax]" 2200 
a "and byte [eax], al" 2000 
a "and dword [eax], eax" 2100
a "and eax, dword [eax]" 2300 
aB "andnpd xmm0, xmmword [eax]" 660f55 
a "andnps xmm0, xmmword [eax]" 0f5500 
aB "andpd xmm0, xmmword [eax]" 660f54 
a "andps xmm0, xmmword [eax]" 0f5400 
a "arpl word [eax], ax" 6300 
a "blendpd xmm0, xmm0, 0" 660f3a0dc000 
a "blendps xmm0, xmm0, 0" 660f3a0cc000 
a "blendvpd xmm0, xmm0" 660f3815c0 
a "blendvps xmm0, xmm0" 660f3814c0 
a "bound eax, qword [eax]" 6200 
a "bsf eax, dword [eax]" 0fbc00 
a "bsr eax, dword [eax]" 0fbd00 
a "bswap eax" 0fc8 
a "bswap ebp" 0fcd 
a "bswap ebx" 0fcb 
a "bswap ecx" 0fc9 
a "bswap edi" 0fcf 
a "bswap edx" 0fca 
a "bswap esi" 0fce 
a "bswap esp" 0fcc 
a "btc dword [eax], eax" 0fbb00 
a "bt dword [eax], eax" 0fa300
a "bt ecx, esp" 0fa3e1
a "bt edx, 59" 0fbae23b
a "bt ebp, -21" 0fbae5eb
a "btr dword [eax], eax" 0fb300 
a "bts dword [eax], eax" 0fab00 
a "call 0x8049100" e8fb900408
a "call 4" e8ffffffff
a "call 5" e800000000
a "call dword [eax]" ff10 
a "call ebx" ffd3
a "cbw" 6698 
a "cdq" 99 
a "cdqe" 98 
a "clc" f8 
a "cld" fc 
a "clflush byte [eax]" 0fae38
a "clgi" 0f01dd 
a "cli" fa
a "clts" 0f06 
a "cmc" f5 
a "cmova eax, dword [eax]" 0f4700 
a "cmovae eax, dword [eax]" 0f4300 
a "cmovb eax, dword [eax]" 0f4200 
a "cmovbe eax, dword [eax]" 0f4600 
a "cmove eax, dword [eax]" 0f4400 
a "cmovg eax, [eax]" 0f4f00 
a "cmovge eax, dword [eax]" 0f4d00 
a "cmovl eax, dword [eax]" 0f4c00 
a "cmovle eax, dword [eax]" 0f4e00 
a "cmovne eax, dword [eax]" 0f4500 
a "cmovno eax, dword [eax]" 0f4100 
a "cmovnp eax, dword [eax]" 0f4b00 
a "cmovns eax, dword [eax]" 0f4900 
a "cmovo eax, dword [eax]" 0f4000 
a "cmovp eax, dword [eax]" 0f4a00 
a "cmovs eax, dword [eax]" 0f4800 
a "cmp al, 0" 3c00 
a "cmp al, byte [eax]" 3a00 
a "cmp byte [eax], al" 3800 
a "cmp dword [eax], eax" 3900 
a "cmp eax, 33" 83f821
a "cmp eax, dword [eax]" 3b00 
a "cmp eax, ebx" 39d8
a "cmp ebx, eax" 39c3
a "cmp edx, esi" 39f2
a "cmpeqpd xmm0, xmmword [eax]" 660fc20000 
a "cmpeqps xmm0, xmmword [eax]" 0fc20000 
a "cmpeqss xmm0, dword [eax]" f30fc20000 
a "cmplepd xmm0, xmmword [eax]" 660fc20002 
a "cmpleps xmm0, xmmword [eax]" 0fc20002 
a "cmplesd xmm0, qword [eax]" f20fc20002 
a "cmpless xmm0, dword [eax]" f30fc20002 
a "cmpltpd xmm0, xmmword [eax]" 660fc20001 
a "cmpltps xmm0, xmmword [eax]" 0fc20001 
a "cmpltsd xmm0, qword [eax]" f20fc20001 
a "cmpltss xmm0, dword [eax]" f30fc20001 
a "cmpneqpd xmm0, xmmword [eax]" 660fc20004 
a "cmpneqps xmm0, xmmword [eax]" 0fc20004 
a "cmpneqsd xmm0, qword [eax]" f20fc20004 
a "cmpneqss xmm0, dword [eax]" f30fc20004 
a "cmpnlepd xmm0, xmmword [eax]" 660fc20006 
a "cmpnleps xmm0, xmmword [eax]" 0fc20006 
a "cmpnlesd xmm0, qword [eax]" f20fc20006 
a "cmpnless xmm0, dword [eax]" f30fc20006 
a "cmpnltpd xmm0, xmmword [eax]" 660fc20005 
a "cmpnltps xmm0, xmmword [eax]" 0fc20005 
a "cmpnltsd xmm0, qword [eax]" f20fc20005 
a "cmpnltss xmm0, dword [eax]" f30fc20005 
a "cmpordpd xmm0, xmmword [eax]" 660fc20007 
a "cmpordps xmm0, xmmword [eax]" 0fc20007 
a "cmpordsd xmm0, qword [eax]" f20fc20007 
a "cmpordss xmm0, dword [eax]" f30fc20007 
aB "cmpsb byte [esi], byte ptr es:[edi]" a6 
aB "cmpsd dword [esi], dword ptr es:[edi]" a7 
aB "cmpsd xmm0, qword [eax]" f20fc20000 
a "cmpunordpd xmm0, xmmword [eax]" 660fc20003 
a "cmpunordps xmm0, xmmword [eax]" 0fc20003 
a "cmpunordsd xmm0, qword [eax]" f20fc20003 
a "cmpunordss xmm0, dword [eax]" f30fc20003 
aB "cmpxchg16b [eax]" 67480f0c70
aB "cmpxchg8b dword [eax]" 0fc7c0 
a "cmpxchg byte [eax], al" 0fb000 
a "cmpxchg dword [eax], eax" 0fb100 
aB "comisd xmm0, xmmword [eax]" 660f2f00 
aB "comiss xmm0, xmmword [eax]" 0f2f00 
a "cpuid" 0fa2
aB "crc32 eax, byte [eax]" f20f38f0 
aB "crc32 eax, dword [eax]" f20f38f1 
a "cvtdq2pd xmm0, qword [eax]" f30fe600  
a "cvtdq2ps xmm0, xmmword [eax]" 0f5b00 
a "cvtpd2dq xmm0, xmmword [eax]" f20fe600 
a "cvtpd2pi mm0, xmmword [eax]" 660f2d00 
a "cvtpd2ps xmm0, xmmword [eax]" 660f5a00 
a "cvtpi2pd xmm0, qword [eax]" 660f2a00 
a "cvtpi2ps xmm0, qword [eax]" 0f2a00 
a "cvtps2dq xmm0, xmmword [eax]" 660f5b00 
a "cvtps2pd xmm0, qword [eax]" 0f5a00 
a "cvtps2pi mm0, qword [eax]" 0f2d00 
a "cvtsd2si eax, qword [eax]" f20f2d00 
a "cvtsd2ss xmm0, qword [eax]" f20f5a00 
a "cvtsi2sd xmm0, dword [eax]" f20f2a00 
a "cvtsi2ss xmm0, dword [eax]" f30f2a00 
a "cvtss2sd xmm0, dword [eax]" f30f5a00 
a "cvtss2si eax, dword [eax]" f30f2d00 
a "cvttpd2dq xmm0, xmmword [eax]" 660fe600 
a "cvttpd2pi mm0, xmmword [eax]" 660f2c00 
a "cvttps2dq xmm0, xmmword [eax]" f30f5b00 
a "cvttps2pi mm0, qword [eax]" 0f2c00 
a "cvttsd2si eax, qword [eax]" f20f2c00 
a "cvttss2si eax, dword [eax]" f30f2c00 
a "cwd" 6699 
a "cwde" 98 
a "daa" 27 
a "das" 2f 
a "dec byte [eax]" fe08 
a "dec dword [eax]" ff08 
a "dec eax" 48
a "dec ebp" 4d
a "dec ebx" 4b
a "dec ecx" 49
a "dec edi" 4f
a "dec edx" 4a
a "dec esi" 4e
a "dec esp" 4c
a "div byte [eax]" f630
a "divpd xmm0, xmmword [eax]" 660f5e00 
a "divps xmm0, xmmword [eax]" 0f5e00 
a "divsd xmm0, qword [eax]" f20f5e00 
a "divss xmm0, dword [eax]" f30f5e00 
a "dppd xmm0, xmm0, 0" 660f3a41c000 
a "dpps xmm0, xmm0, 0" 660f3a40c000 
a "emms" 0f77 
a "extractps eax, xmm0, 0" 660f3a17c000 
a "extrq xmm0, 0x0, 0x0" 660f78c00000 
aB "extrq xmm0, xmm0" 660f7900 
a "femms" 0f0e 
a "fsincos" d9fb
aB "fxrstor [eax]" 0fae00
a "fxsave [eax]" 0fae00
a "getsec" 0f37 
a "haddpd xmm0, xmmword [eax]" 660f7c00 
a "haddps xmm0, xmmword [eax]" f20f7c00 
a "hlt" f4
a "hsubpd xmm0, xmmword [eax]" 660f7d00 
a "hsubps xmm0, xmmword [eax]" f20f7d00 
a "idiv byte [eax]" f638
a "imul byte [eax]" f628 
a "imul eax, dword [eax], 0" 6b0000 
a "imul eax, dword [eax]" 0faf00 
aB "imul eax, [eax], 0" 690000000000 
aB "in al,0" e4 
a "in al,dx" ec 
a "inc byte [eax]" fe00 
a "inc dword [eax]" ff00
a "inc eax" 40
a "inc ebp" 45
a "inc ebx" 43
a "inc ecx" 41
a "inc edi" 47
a "inc edx" 42
a "inc esi" 46
a "inc esp" 44
aB "in eax,0" e5 
a "in eax, 0x8c" e58c 
a "in eax,dx" ed 
a "insb byte es:[edi], dx" 6c 
a "insd dword es:[edi], dx" 6d 
a "insertps xmm0, xmm0, 0" 660f3a21c000 
a "int 0x21" cd21
a "int 1" cd01
a "int1" f1 
a "int3" cc
a "int 3" cd03
a "into" ce 
a "invd" 0f08 
aB "invlpga" 0f01df 
a "invlpg byte [eax]" 0f0138 
a "iret" 66cf 
a "iretd" cf
a "ja 0x8049300" 0f87fa920408
aB "ja 2" 0f87fcffffff 
aB "ja 6" 0f8700000000 
a "jae 2" 7300 
aB "jae 6" 0f8300000000 
a "jb 0x8049300" 0f82fa920408
aB "jb 2" 0f82fcffffff 
aB "jb 6" 0f8200000000 
a "jbe 2" 7600 
aB "jbe 6" 0f8600000000 
aB "je 2" 0f84fcffffff 
aB "je 6" 0f8400000000 
a "jg 0x8049300" 0f8ffa920408
aB "jg 2" 0f8ffcffffff 
aB "jg 6" 0f8f00000000 
a "jge 0x8048010" 0f8d0a800408
a "jge 0x8049300" 0f8dfa920408
aB "jge 2" 0f8dfcffffff 
aB "jge 6" 0f8d00000000 
a "jl 0x8048010" 0f8c0a800408
a "jl 0x8049300" 0f8cfa920408
aB "jl 2" 0f8cfcffffff 
aB "jl 6" 0f8c00000000 
a "jle 0x8048010" 0f8e0a800408
a "jle 0x8049300" 0f8efa920408
aB "jle 2" 0f8efcffffff 
aB "jle 6" 0f8e00000000 
a "jmp 0" ebfe
a "jmp 0x42" eb40
a "jmp -0x7e" eb80
a "jmp -0x7f" e97cffffff
a "jmp 0x8049200" e9fb910408
a "jmp 0x81" eb7f
a "jmp 0x82" e97d000000
a "jmp 2" eb00
a "jmp 3" eb01
a "jmp ecx" ffe1
aB "jne 6" 0f8500000000 
a "jno 2" 7100 
aB "jno 6" 0f8100000000 
a "jnp 2" 7b00 
aB "jnp 6" 0f8b00000000 
a "jns 2" 7900 
aB "jns 6" 0f8900000000 
aB "jnz 2" 0f85fcffffff 
a "jo 2" 7000 
aB "jo 6" 0f8000000000 
a "jp 2" 7a00 
aB "jp 6" 0f8a00000000 
a "js 2" 7800 
aB "js 6" 0f8800000000 
aB "lahf" 9e 
aB "lar eax, word [eax]" 0f02 
aB "lcall 0, 0" 9a 
aB "lcall [0]" ff1c2500000000 
a "lcall [eax]" ff18 
a "lddqu xmm0, xmmword [eax]" f20ff000 
a "ldmxcsr [eax]" 0fae10 
a "lds eax, [eax]" c500 
a "lea eax, [4]" 8d0504000000
a "lea eax, [eax+4]" 8d4004
a "lea eax, [eax]" 8d00
a "lea eax, [ebp+24]" 8d4518
a "lea eax, [ebx+24]" 8d4318
a "lea eax, [ebx+4]" 8d4304
a "lea eax, [ecx]" 8d01
a "lea eax, [esp]" 8d0424
a "lea ebx, [4]" 8d1d04000000
a "lea ebx, [eax+24]" 8d5818
a "lea ebx, [eax+4]" 8d5804
a "lea ebx, [ebp+324]" 8d9d44010000
a "lea ebx, [ebp]" 8d5d00
a "leave" c9
a "les eax, [eax]" c400 
a "lfence" 0faee8 
a "lfs eax, dword [eax]" 0fb400 
aB "lgdt [eax]" 0f0110
a "lgs eax, dword [eax]" 0fb500 
aB "lidt [eax]" 0f0118
a "lldt ax" 0f00d0
a "lldt word [eax]" 0f0010
a "lmsw ax" 0f01f0
a "lmsw word [eax]" 0f0130
aB "lock and word [fs:bx + si], si" 646766f02130 
aB "lock cmpxchg8b" f00fc7c0 
a "lock mov dword [eax], eax" f08900 
a "lock mov eax, eax" f089c0 
a "lodsb al, byte [esi]" ac 
a "lodsd eax, dword [esi]" ad 
aB "loop 3" 66e200 
aB "lsl eax, dword [eax]" 0f03 
a "lss eax, dword [eax]" 0fb200 
a "ltr ax" 0f00d8 
a "ltr word [eax]" 0f0018 
a "lzcnt eax, dword [eax]" f30fbd00 
aB "maskmovdqu xmm0, xmm0" 660ff7 
aB "maskmovq mm0, mm0" 0ff7 
a "maxpd xmm0, xmmword [eax]" 660f5f00 
a "maxps xmm0, xmmword [eax]" 0f5f00 
a "maxsd xmm0, qword [eax]" f20f5f00 
a "maxss xmm0, dword [eax]" f30f5f00 
a "mfence" 0faef0 
a "minpd xmm0, xmmword [eax]" 660f5d00 
a "minps xmm0, xmmword [eax]" 0f5d00 
a "minsd xmm0, qword [eax]" f20f5d00 
a "minss xmm0, dword [eax]" f30f5d00 
a "monitor" 0f01c8 
a "mov [33], ebp" 892d21000000
a "mov [33], ebx" 891d21000000
a "mov [33], ecx" 890d21000000
a "mov [33], edi" 893d21000000
a "mov [33], edx" 891521000000
a "mov [33], esi" 893521000000
a "mov [33], esp" 892521000000
a "mov ah, 0" b400 
a "mov al, 0" b000 
a "mov al, byte [0]" a000000000 
a "mov al, byte [eax]" 8a00 
a "mov al, [eax]" 8a00 
a "movapd xmm0, xmmword [eax]" 660f2800 
a "movapd xmmword [eax], xmm0" 660f2900 
a "movaps xmm0, xmmword [eax]" 0f2800 
a "movaps xmmword [eax], xmm0" 0f2900 
a "movbe dword [eax], eax" 0f38f100 
a "movbe eax, dword [eax]" 0f38f000 
a "mov bh, 0" b700 
a "mov bl, 0" b300 
a "mov byte [0], al" a200000000 
a "mov byte [eax], 0" c60000
a "mov byte [eax], al" 8800 
a "mov ch, 0" b500 
a "mov cl, 0" b100 
aB "mov cr0, eax" 0f22 
a "movddup xmm0, qword [eax]" f20f1200 
a "movd dword [eax], mm0" 0f7e00 
a "movd dword [eax], xmm0" 660f7e00 
a "mov dh, 0" b600 
a "mov dl, 0" b200 
a "movd mm0, dword [eax]" 0f6e00 
aB "movdq2q mm0, xmm0" f20fd6 
a "movdqa xmm0, xmmword [eax]" 660f6f00 
a "movdqa xmmword [eax], xmm0" 660f7f00 
a "movdqu xmm0, xmmword [eax]" f30f6f00 
a "movdqu xmmword [eax], xmm0" f30f7f00 
aB "mov dr0, eax" 0f23 
a "mov dword [0], eax" a300000000 
a "mov dword cs:[eax], eax" 2e8900 
aB "mov dword ds:[eax], eax" 3e8900 
a "mov dword [eax], 0" c70000000000
a "mov dword [eax], 0x6f77206f" c7006f20776f
a "mov dword [eax+16], 0x6f77206f" c740106f20776f
a "mov dword [eax], 3" c70003000000
a "mov dword [eax+4], 1" c7400401000000
a "mov dword [eax+4], 3" c7400403000000
a "mov dword [eax+450], 0x6f77206f" c780c20100006f20776f
a "mov dword [eax+4], 666" c740049a020000
a "mov dword [eax-512], 421" c78000feffffa5010000
a "mov dword [eax], 666" c7009a020000
a "mov dword [eax], eax" 8900
a "mov dword [ebp-12], 1" c745f401000000
a "mov dword [ebp+16], 0x6f77206f" c745106f20776f
a "mov dword [ebp-312], 3" c785c8feffff03000000
a "mov dword [ebp+4], 1" c7450401000000
a "mov dword [ebp+450], 0x6f77206f" c785c20100006f20776f
a "mov dword es:[eax], eax" 268900 
a "mov dword [esi+4], 33" c7460421000000
a "mov dword [esp-312], 321" c78424c8feffff41010000
a "mov dword [esp], 3" c7042403000000
a "mov dword [esp+4], 1" c744240401000000
a "mov dword fs:[eax], eax" 648900 
a "mov dword gs:[eax], eax" 658900 
a "mov dword ss:[eax], eax" 368900 
a "movd xmm0, dword [eax]" 660f6e00 
a "mov eax, 0" b800000000
a "mov eax, 0x8049000" b800900408
a "mov eax, 1" b801000000
a "mov [eax+2], ebx" 895802
a "mov eax, 300" b82c010000
a "mov eax, 3" b803000000
a "mov [eax+4], eax" 894004
a "mov [eax+4], ecx" 894804
aB "mov eax, cr0" 0f20 
aB "mov eax, dr0" 0f21 
a "mov eax, dword [0]" a100000000 
a "mov eax, dword [eax]" 8b00
a "mov eax, dword [ebp]" 8b4500
a "mov eax, dword [esp]" 8b0424
a "mov eax, dword fs:[ebp]" 648b4500 
a "mov eax, [eax+1337]" 8b8039050000
a "mov eax, [eax-1337]" 8b80c7faffff
a "mov eax,[eax*4+32]" 8b048520000000
a "mov eax,[eax*4-32]" 8b0485e0ffffff
a "mov eax,[eax*4+332]" 8b04854c010000
a "mov eax,[eax*4-332]" 8b0485b4feffff
a "mov eax, [eax+4]" 8b4004
a "mov eax, [eax-4]" 8b40fc
a "mov [eax], eax" 8900
a "mov eax, eax" 89c0
a "mov eax, [eax]" 8b00
a "mov [eax+eax], eax" 890400
a "mov eax,[eax+ebx*4+32]" 8b449820 
a "mov [eax+eax], ebx" 891c00
a "mov [eax+eax], ecx" 890c00
a "mov eax, [ebp]" 8b4500
a "mov [eax], ebx" 8918
a "mov eax, ebx" 89d8
a "mov eax, [ebx]" 8b03
a "mov eax,[ecx*8+64]" 8b04cd40000000
a "mov [eax+ecx], eax" 890408
a "mov eax, [esi]" 8b06
a "mov eax, [esp+4]" 8b442404
a "mov eax, esp" 89e0
a "mov eax, [esp]" 8b0424
a "mov ebp, 0" bd00000000
a "mov [ebp+4], eax" 894504
a "mov [ebp+4], ebx" 895d04
a "mov [ebp+4], ecx" 894d04
a "mov ebx, 0" bb00000000
a "mov [ebx+2], ebx" 895b02
a "mov [ebx-2], ecx" 894bfe
a "mov ebx, -3" bbfdffffff
a "mov [ebx+454], ebx" 899bc6010000
a "mov [ebx-552], edx" 8993d8fdffff
a "mov [ebx], eax" 8903
a "mov ebx, eax" 89c3
a "mov ebx, [eax]" 8b18
a "mov [ebx+eax], eax" 890403
a "mov ecx, 0" b900000000
a "mov ecx, -432" b950feffff
a "mov ecx, [eax]" 8b08
a "mov edi, 0" bf00000000
a "mov edx, 0" ba00000000
a "mov esi, 0" be00000000
a "mov esi, [esi + 8]" 8b7608
a "mov esp, 0" bc00000000
a "mov [esp-12], eax" 894424f4
a "mov [esp+2], ebx" 895c2402
a "mov [esp-2], ebx" 895c24fe
a "mov [esp+454], ebx" 899c24c6010000
a "mov es, word [eax]" 8e00 
aB "movhlps xmm0, xmm0" 0f12 
a "movhpd qword [eax], xmm0" 660f1700 
a "movhpd xmm0, qword [eax]" 660f1600 
aB "movhps qword [eax], xmm0" 0f17 
aB "movhps xmm0, qword [eax]" 0f16 
aB "movlhps xmm0, xmm0" 0f16 
a "movlpd qword [eax], xmm0" 660f1300 
a "movlpd xmm0, qword [eax]" 660f1200 
aB "movlps qword [eax], xmm0" 0f13 
aB "movlps xmm0, qword [eax]" 0f12 
a "movmskpd eax, xmm0" 660f50c0 
a "movmskps eax, xmm0" 0f50c0 
a "movntdqa xmm0, xmmword [eax]" 660f382a00 
a "movntdq xmmword [eax], xmm0" 660fe700 
a "movnti dword [eax], eax" 0fc300 
a "movntpd xmmword [eax], xmm0" 660f2b00 
a "movntps xmmword [eax], xmm0" 0f2b00 
a "movntq qword [eax], mm0" 0fe700 
aB "movq2dq xmm0, mm0" f30fd6 
a "movq mm0, qword [eax]" 0f6f00 
a "movq qword [eax], mm0" 0f7f00 
a "movq qword [eax], xmm0" 660fd600 
a "movq xmm0, qword [eax]" f30f7e00 
aB "movsb byte es:[edi], byte ptr [esi]" a4 
aB "movsd dword es:[edi], dword ptr [esi]" a5 
aB "movsd dword es:[edi], dword ptr fs:[esi]" 64a5 
a "movsd qword [eax], xmm0" f20f1100 
a "movsd xmm0, qword [eax]" f20f1000  
a "movshdup xmm0, xmmword [eax]" f30f1600 
a "movsldup xmm0, xmmword [eax]" f30f1200 
a "movss dword [eax], xmm0" f30f1100 
a "movss xmm0, dword [eax]" f30f1000 
a "movsx eax, byte [eax]" 0fbe00 
a "movsx eax, word [eax]" 0fbf00 
a "movupd xmm0, xmmword [eax]" 660f1000 
a "movupd xmmword [eax], xmm0" 660f1100 
aB "movups xmm0, xmmword [eax]" 0f10 
aB "movups xmmword [eax], xmm0" 0f11 
aB "mov word [eax], es" 8c00 
a "movzx eax, byte [eax]" 0fb600 
a "movzx eax, word [eax]" 0fb700 
a "mpsadbw xmm0, xmm0, 0" 660f3a42c000 
a "mul byte [eax]" f620 
a "mulpd xmm0, xmmword [eax]" 660f5900 
a "mulpd xmm7, xmm7" 660f59ff 
a "mulps xmm0, xmmword [eax]" 0f5900 
a "mulps xmm7, xmm7" 0f59ff 
a "mulsd xmm0, qword [eax]" f20f5900 
aB "mulsd xmm7, xmm7" 66f3f20f59ff 
aB "mulsd xmm7, xmm7" f2660f59ff 
a "mulss xmm0, dword [eax]" f30f5900 
aB "mulss xmm7, xmm7" 66f2f0f59ff0
a "mwait" 0f01c9 
a "neg byte [eax]" f618 
a "nop" 90
a "not byte [eax]" f610 
a "or al, 0" 0c00 
a "or byte [eax], al" 0800 
a "or dword [eax], eax" 0900
a "or eax, dword [eax]" 0b00 
a "orpd xmm0, xmmword [eax]" 660f5600 
a "orps xmm0, xmmword [eax]" 0f5600 
a "out 0, al" e600 
a "out 0, eax" e700 
a "out 0x84, eax" e784 
a "out dx, al" ee 
a "out dx, eax" ef 
a "outsb dx, byte [esi]" 6e 
a "outsd dx, dword [esi]" 6f 
a "pabsb xmm0, xmm0" 660f381cc0 
a "pabsd xmm0, xmm0" 660f381ec0 
a "pabsw xmm0, xmm0" 660f381dc0 
a "packssdw mm0, qword [eax]" 0f6b00 
a "packssdw xmm0, xmmword [eax]" 660f6b00 
a "packsswb mm0, qword [eax]" 0f6300 
a "packsswb xmm0, xmmword [eax]" 660f6300 
a "packusdw xmm0, xmm0" 660f382bc0 
a "packuswb mm0, qword [eax]" 0f6700 
a "packuswb xmm0, xmmword [eax]" 660f6700 
a "paddb mm0, qword [eax]" 0ffc00 
a "paddb xmm0, xmmword [eax]" 660ffc00 
a "paddd mm0, qword [eax]" 0ffe00 
a "paddd xmm0, xmmword [eax]" 660ffe00 
a "paddq xmm0, xmmword [eax]" 660fd400 
a "paddsb mm0, qword [eax]" 0fec00 
a "paddsb xmm0, xmmword [eax]" 660fec00 
a "paddsw mm0, qword [eax]" 0fed00 
a "paddsw xmm0, xmmword [eax]" 660fed00 
a "paddusb mm0, qword [eax]" 0fdc00 
a "paddusb xmm0, xmmword [eax]" 660fdc00 
a "paddusw mm0, qword [eax]" 0fdd00 
a "paddusw xmm0, xmmword [eax]" 660fdd00 
a "paddw mm0, qword [eax]" 0ffd00 
a "paddw xmm0, xmmword [eax]" 660ffd00 
a "palignr mm0, mm0, 0" 0f3a0fc000 
a "palignr xmm0, xmm0, 0" 660f3a0fc000 
a "pand mm0, qword [eax]" 0fdb00 
a "pandn mm0, qword [eax]" 0fdf00 
a "pandn xmm0, xmmword [eax]" 660fdf00 
a "pand xmm0, xmmword [eax]" 660fdb00 
a "pause" f390 
a "pavgb mm0, qword [eax]" 0fe000 
aB "pavgb mm0, qword [eax]" 0fe0 
a "pavgb xmm0, xmmword [eax]" 660fe000 
a "pavgw mm0, qword [eax]" 0fe300 
a "pavgw xmm0, xmmword [eax]" 660fe300 
a "pblendvb xmm0, xmm0" 660f3810c0 
a "pblendw xmm0, xmm0, 0" 660f3a0ec000 
a "pclmulqdq xmm0, xmm0, 0" 660f3a44c000 
a "pcmpeqb mm0, qword [eax]" 0f7400 
a "pcmpeqb xmm0, xmmword [eax]" 660f7400 
a "pcmpeqd mm0, qword [eax]" 0f7600 
a "pcmpeqd xmm0, xmmword [eax]" 660f7600 
a "pcmpeqq xmm0, xmm0" 660f3829c0 
a "pcmpeqw mm0, qword [eax]" 0f7500 
a "pcmpeqw xmm0, xmmword [eax]" 660f7500 
a "pcmpestri xmm0, xmm0, 0" 660f3a61c000 
a "pcmpestrm xmm0, xmm0, 0" 660f3a60c000 
a "pcmpgtb mm0, qword [eax]" 0f6400 
a "pcmpgtb xmm0, xmmword [eax]" 660f6400 
a "pcmpgtd mm0, qword [eax]" 0f6600 
a "pcmpgtd xmm0, xmmword [eax]" 660f6600 
a "pcmpgtq xmm0, xmm0" 660f3837c0 
a "pcmpgtw mm0, qword [eax]" 0f6500 
a "pcmpgtw xmm0, xmmword [eax]" 660f6500 
a "pcmpistri xmm0, xmm0, 0" 660f3a63c000 
a "pcmpistrm xmm0, xmm0, 0" 660f3a62c000 
a "pextrb eax, xmm0, 0" 660f3a14c000 
a "pextrd eax, xmm0, 0" 660f3a16c000 
aB "pextrq dword [eax], xmm0, 0" 660f3a16 
a "pextrw eax, mm0, 0" 0fc5c000 
a "pextrw eax, xmm0, 0" 660fc5c000 
a "phaddd xmm0, xmmword [eax]" 660f380200 
a "phaddsw xmm0, xmmword [eax]" 660f380300 
a "phaddw xmm0, xmmword [eax]" 660f380100 
a "phminposuw xmm0, xmm0" 660f3841c0 
a "phsubd xmm0, xmmword [eax]" 660f380600 
a "phsubsw xmm0, xmmword [eax]" 660f380700 
a "phsubw xmm0, xmmword [eax]" 660f380500 
a "pinsrb xmm0, eax, 0" 660f3a20c000 
aB "pinsrd xmm0, dword [eax], 0" 660f3a22 
aB "pinsrq xmm0, dword [eax], 0" 660f3a22 
a "pinsrw mm0, word [eax], 0x0" 0fc40000 
a "pinsrw xmm0, word [eax], 0x0" 660fc40000 
a "pmaddubsw xmm0, xmmword [eax]" 660f380400 
a "pmaddwd mm0, qword [eax]" 0ff500 
a "pmaddwd xmm0, xmmword [eax]" 660ff500 
a "pmaxsb xmm0, xmm0" 660f383cc0 
a "pmaxsd xmm0, xmm0" 660f383dc0 
a "pmaxsw mm0, qword [eax]" 0fee00 
a "pmaxsw xmm0, xmmword [eax]" 660fee00 
a "pmaxub mm0, qword [eax]" 0fde00 
a "pmaxub xmm0, xmmword [eax]" 660fde00 
a "pmaxud xmm0, xmm0" 660f383fc0 
a "pmaxuw xmm0, xmm0" 660f383ec0 
a "pminsb xmm0, xmm0" 660f3838c0 
a "pminsd xmm0, xmm0" 660f3839c0 
a "pminsw mm0, qword [eax]" 0fea00 
a "pminsw xmm0, xmmword [eax]" 660fea00 
a "pminub mm0, qword [eax]" 0fda00 
a "pminub xmm0, xmmword [eax]" 660fda00 
a "pminud xmm0, xmm0" 660f383bc0 
a "pminuw xmm0, xmm0" 660f383ac0 
aB "pmovmskb eax, mm0" 0fd7 
a "pmovsxbd xmm0, xmm0" 660f3821c0 
a "pmovsxbq xmm0, xmm0" 660f3822c0 
a "pmovsxbw xmm0, xmm0" 660f3820c0 
a "pmovsxdq xmm0, xmm0" 660f3825c0 
a "pmovsxwd xmm0, xmm0" 660f3823c0 
a "pmovsxwq xmm0, xmm0" 660f3824c0 
a "pmovzxbd xmm0, xmm0" 660f3831c0 
a "pmovzxbq xmm0, xmm0" 660f3832c0 
a "pmovzxbw xmm0, xmm0" 660f3830c0 
a "pmovzxdq xmm0, xmm0" 660f3835c0 
a "pmovzxwd xmm0, xmm0" 660f3833c0 
a "pmovzxwq xmm0, xmm0" 660f3834c0 
a "pmuldq xmm0, xmm0" 660f3828c0 
a "pmulhrsw xmm0, xmm0" 660f380bc0 
a "pmulhuw mm0, qword [eax]" 0fe400 
a "pmulhuw xmm0, xmmword [eax]" 660fe400 
a "pmulhw mm0, qword [eax]" 0fe500 
a "pmulhw xmm0, xmmword [eax]" 660fe500 
a "pmulld xmm0, xmm0" 660f3840c0 
a "pmullw mm0, qword [eax]" 0fd500 
a "pmullw xmm0, xmmword [eax]" 660fd500 
a "pmuludq mm0, qword [eax]" 0ff400 
a "pmuludq xmm0, xmmword [eax]" 660ff400 
a "popal" 61 
a "popaw" 6661 
aB "popcnt eax, qword [eax]" f30fb8 
aB "pop ds" 1f 
a "pop dword [eax+4]" 8f4004
a "pop dword [eax]" 8f00
a "pop dword [ebp+4]" 8f4504
a "pop dword [ebp]" 8f4500
a "pop dword [ecx]" 8f01
a "pop dword [edi]" 8f07
a "pop dword [esi]" 8f06
a "pop dword [esp]" 8f0424
a "pop eax" 58
a "pop ebp" 5d
a "pop ebx" 5b
a "pop ecx" 59
a "pop edi" 5f
a "pop edx" 5a
aB "pop es" 07 
a "pop esi" 5e
a "pop esp" 5c
a "popfd" 9d 
a "pop fs" 0fa1
a "pop gs" 0fa9
aB "pop ss" 17 
a "por mm0, qword [eax]" 0feb00 
a "por xmm0, xmmword [eax]" 660feb00 
a "prefetch byte [eax]" 0f0d00 br 
a "prefetchnta byte [eax]" 0f1800 
a "prefetcht0 byte [eax]" 0f1808 
a "prefetcht1 byte [eax]" 0f1810 
a "prefetcht2 byte [eax]" 0f1818 
a "psadbw mm0, qword [eax]" 0ff600 
a "psadbw xmm0, xmmword [eax]" 660ff600 
a "pshufb mm0, qword [eax]" 0f380000 
a "pshufb xmm0, xmmword [eax]" 660f380000 
a "pshufd xmm0, xmmword [eax], 0" 660f700000 
a "pshufhw xmm0, xmmword [eax], 0" f30f700000 
a "pshuflw xmm0, xmmword [eax], 0" f20f700000 
a "pshufw mm0, qword [eax], 0" 0f700000 
a "psignb xmm0, xmm0" 660f3808c0 
a "psignd xmm0, xmm0" 660f380ac0 
a "psignw xmm0, xmm0" 660f3809c0 
a "pslld mm0, 0" 0f72f000 
a "pslld mm0, qword [eax]" 0ff200 
a "pslldq xmm0, 0" 660f73f800 
a "pslld xmm0, 0" 660f72f000 
a "pslld xmm0, xmmword [eax]" 660ff200 
a "psllq mm0, 0" 0f73f000 
a "psllq mm0, qword [eax]" 0ff300 
a "psllq xmm0, 0" 660f73f000 
a "psllq xmm0, xmmword [eax]" 660ff300 
a "psllw mm0, 0" 0f71f000 
a "psllw mm0, qword [eax]" 0ff100 
a "psllw xmm0, 0" 660f71f000 
a "psllw xmm0, xmmword [eax]" 660ff100 
a "psrad mm0, 0" 0f72e000 
a "psrad mm0, qword [eax]" 0fe200 
a "psrad xmm0, 0" 660f72e000 
a "psrad xmm0, xmmword [eax]" 660fe200 
a "psraw mm0, 0" 0f71e000 
a "psraw mm0, qword [eax]" 0fe100 
a "psraw xmm0, 0" 660f71e000 
a "psraw xmm0, xmmword [eax]" 660fe100 
a "psrld mm0, 0" 0f72d000 
a "psrld mm0, qword [eax]" 0fd200 
a "psrldq xmm0, 0" 660f73d800 
a "psrld xmm0, 0" 660f72d000 
a "psrld xmm0, xmmword [eax]" 660fd200 
a "psrlq mm0, 0" 0f73d000 
a "psrlq mm0, qword [eax]" 0fd300 
a "psrlq xmm0, 0" 660f73d000 
a "psrlq xmm0, xmmword [eax]" 660fd300 
a "psrlw mm0, 0" 0f71d000 
a "psrlw mm0, qword [eax]" 0fd100 
a "psrlw xmm0, 0" 660f71d000 
a "psrlw xmm0, xmmword [eax]" 660fd100 
a "psubb mm0, qword [eax]" 0ff800 
a "psubb xmm0, xmmword [eax]" 660ff800 
a "psubd mm0, qword [eax]" 0ffa00 
a "psubd xmm0, xmmword [eax]" 660ffa00 
a "psubq mm0, qword [eax]" 0ffb00 
a "psubq xmm0, xmmword [eax]" 660ffb00 
aB "psubsb mm0, xmmword [eax]" 0fe800 
a "psubsb xmm0, xmmword [eax]" 660fe800 
aB "psubsw mm0, xmmword [eax]" 0fe900 
a "psubsw xmm0, xmmword [eax]" 660fe900 
a "psubusb mm0, qword [eax]" 0fd800 
a "psubusb xmm0, xmmword [eax]" 660fd800 
a "psubusw mm0, qword [eax]" 0fd900 
a "psubusw xmm0, xmmword [eax]" 660fd900 
a "psubw mm0, qword [eax]" 0ff900 
a "psubw xmm0, xmmword [eax]" 660ff900 
a "ptest xmm0, xmm0" 660f3817c0 
a "punpckhbw mm0, qword [eax]" 0f6800 
a "punpckhbw xmm0, xmmword [eax]" 660f6800 
a "punpckhdq mm0, qword [eax]" 0f6a00 
a "punpckhdq xmm0, xmmword [eax]" 660f6a00 
a "punpckhqdq xmm0, xmmword [eax]" 660f6d00 
a "punpckhwd mm0, qword [eax]" 0f6900 
a "punpckhwd xmm0, xmmword [eax]" 660f6900 
a "punpcklbw mm0, qword [eax]" 0f6000 
a "punpcklbw xmm0, xmmword [eax]" 660f6000 
a "punpckldq mm0, qword [eax]" 0f6200 
a "punpckldq xmm0, xmmword [eax]" 660f6200 
a "punpcklqdq xmm0, xmmword [eax]" 660f6c00 
a "punpcklwd mm0, qword [eax]" 0f6100 
a "punpcklwd xmm0, xmmword [eax]" 660f6100 
a "push 0" 6a00
a "pushal" 60 
aB "push cs" 0e 
aB "push ds" 1e 
a "push dword [eax+8]" ff7008
a "push dword [eax]" ff30
a "push dword [ebp+4]" ff7504
a "push dword [ebp]" ff7500
a "push dword [ebx+4]" ff7304
a "push dword [ecx]" ff31
a "push dword [edi]" ff37
a "push dword [esi+4]" ff7604
a "push dword [esi]" ff36
a "push dword [esp+4]" ff742404
a "push dword [esp]" ff3424
a "push eax" 50
a "push ebp" 55
a "push ebx" 53
a "push ecx" 51
a "push edi" 57
a "push edx" 52
aB "push es" 06 
a "push esi" 56
a "push esp" 54
a "pushfd" 9c 
a "push fs" 0fa0
a "push gs" 0fa8
aB "push ss" 16 
a "pxor mm0, qword [eax]" 0fef00 
a "pxor xmm0, xmmword [eax]" 660fef00 
a "rcpps xmm0, xmmword [eax]" 0f5300 
a "rcpss xmm0, dword [eax]" f30f5300 
a "rdmsr" 0f32 
a "rdpmc" 0f33 
a "rdtsc" 0f31
a "rdtscp" 0f01f9 
aB "repne movsb byte es:[edi], byte ptr [esi]" f2a4 
a "repz movsb" f3a4 
a "ret" c3
a "retf 0" ca0000
a "retf" cb
aB "retw" 66c3 
a "rol byte [eax], 0" c00000 
a "rol byte [eax], 1" d000 
a "rol byte [eax], cl" d200 
a "rol dword [eax], 0" c10000 
a "rol dword [eax], 1" d100 
a "rol dword [eax], cl" d300 
a "roundpd xmm0, xmm0, 0" 660f3a09c000 
a "roundps xmm0, xmm0, 0" 660f3a08c000 
a "roundsd xmm0, xmm0, 0" 660f3a0bc000 
a "roundss xmm0, xmm0, 0" 660f3a0ac000 
a "rsm" 0faa 
a "rsqrtps xmm0, xmmword [eax]" 0f5200 
a "rsqrtss xmm0, dword [eax]" f30f5200 
a "sahf" 9e 
a "salc" d6 
a "sbb al, 0" 1c00 
a "sbb al, byte [eax]" 1a00 
a "sbb byte [eax], al" 1800 
a "sbb dword [eax], eax" 1900 
a "sbb eax, dword [eax]" 1b00 
a "scasb al, byte es:[edi]" ae 
a "scasd eax, dword es:[edi]" af 
a "seta byte [eax]" 0f9700
a "setae byte [eax]" 0f9300
a "setb byte [eax]" 0f9200
a "setbe byte [eax]" 0f9600
a "sete byte [eax]" 0f9400
a "setg byte [eax]" 0f9f00
a "setge byte [eax]" 0f9d00
a "setl byte [eax]" 0f9c00
a "setle byte [eax]" 0f9e00
a "setne byte [eax]" 0f9500
a "setno byte [eax]" 0f9100
a "setnp byte [eax]" 0f9b00
a "setns byte [eax]" 0f9900
a "seto byte [eax]" 0f9000
a "setp byte [eax]" 0f9a00
a "sets byte [eax]" 0f9800
a "sfence" 0faef8 
aB "sgdt [eax]" 0f0100 
a "shld dword [eax], eax, 0" 0fa40000 
a "shld dword [eax], eax, cl" 0fa500 
aB "shl edx, 5" c1f205  
a "shrd dword [eax], eax, 0" 0fac0000 
a "shrd dword [eax], eax, cl" 0fad00 
a "shufpd xmm0, xmmword [eax], 0x0" 660fc60000 
a "shufps xmm0, xmmword [eax], 0" 0fc60000 
aB "sidt [eax]" 0f0108 
aB "skinit" 0f01de 
a "sldt word [eax]" 0f0000 
a "smsw ax" 660f01e0 
a "smsw eax" 0f01e0 
a "smsw word [eax]" 0f0120 
a "sqrtpd xmm0, xmmword [eax]" 660f5100 
a "sqrtps xmm0, xmmword [eax]" 0f5100 
a "sqrtsd xmm0, qword [eax]" f20f5100 
a "sqrtss xmm0, dword [eax]" f30f5100 
a "stc" f9 
a "std" fd 
a "stgi" 0f01dc 
a "sti" fb
a "stmxcsr dword [eax]" 0fae18 
a "stosb byte es:[edi], al" aa 
a "stosd dword es:[edi], eax" ab 
a "str word [eax]" 0f0008 
a "sub al, 0" 2c00 
a "sub al, byte [eax]" 2a00 
a "sub byte [eax], al" 2800 
a "sub dword [eax], 1" 832801
a "sub dword [eax+4], -666" 81680466fdffff
a "sub dword [eax+4], 666" 8168049a020000
a "sub dword [eax+666], 666" 81a89a0200009a020000
a "sub dword [eax], 666" 81289a020000
a "sub dword [eax], eax" 2900
a "sub dword [ebp+4], 1" 836d0401
a "sub dword [ebp+555], 1" 83ad2b02000001
a "sub dword [ebp+555], 7357" 81ad2b020000bd1c0000
a "sub dword [ebp-555], 7357" 81add5fdffffbd1c0000
a "sub dword [ebx], 1" 832b01
a "sub eax, 3" 83e803
a "sub eax, -666" 2d66fdffff
a "sub eax, 666" 2d9a020000
a "sub eax, dword [eax]" 2b00 
a "sub eax, eax" 29c0
a "sub eax, ebx" 29d8
a "sub ebx, 3" 83eb03
a "sub ebx, -3" 83ebfd
a "sub ebx, 666" 81eb9a020000
a "sub [ebx], eax" 2903
a "sub ebx, eax" 29c3
a "sub ecx, 666" 81e99a020000
a "sub esi,-334" 81eeb2feffff
a "subpd xmm0, xmmword [eax]" 660f5c00 
a "subps xmm0, xmmword [eax]" 0f5c00 
a "subsd xmm0, qword [eax]" f20f5c00 
a "subss xmm0, dword [eax]" f30f5c00 
aB "swapgs" 0f1ff8 
a "syscall" 0f05
a "sysenter" 0f34 
a "sysexit" 0f35
a "sysret" 0f07
a "test al, 0" a800 
a "test byte [eax], 0" f60000 
aB "test byte [eax], 0" f60800 
a "test byte [eax], al" 8400 
a "test dword [eax], 0" f70000000000 
aB "test dword [eax], 0" f70000 
aB "test dword [eax], 0" f70800 
a "test dword [eax], eax" 8500 
a "test eax, 0" a900000000 
a "test eax, ebx" 85d8
a "test edx, esi" 85f2
a "ucomisd xmm0, qword [eax]" 660f2e00 
a "ucomiss xmm0, dword [eax]" 0f2e00 
a "ud2" 0f0b
a "unpckhpd xmm0, xmmword [eax]" 660f1500 
aB "unpckhps xmm0, xmmword [eax]" 0f15 
a "unpcklpd xmm0, xmmword [eax]" 660f1400 
aB "unpcklps xmm0, xmmword [eax]" 0f14 
a "vaddpd ymm0, ymm0, ymm0" c5fd58c0 
a "vaesdeclast xmm0, xmm0, xmm0" c4e279dfc0 
a "vaesdec xmm0, xmm0, xmm0" c4e279dec0 
a "vaesenclast xmm0, xmm0, xmm0" c4e279ddc0 
a "vaesenc xmm0, xmm0, xmm0" c4e279dcc0 
a "vaesimc xmm0, xmm0" c4e279dbc0 
a "vaeskeygenassist xmm0, xmm0, 0" c4e379dfc000 
a "vaeskeygenassist xmm0, xmm0, 0x0" c4e379dfc000 
a "vbroadcastf128 ymm0, xmmword [0]" c4e27d1a0500000000 
a "vbroadcastsd ymm0, qword [0]" c4e27d190500000000 
a "vbroadcastss ymm0, dword [eax]" c4e27d1800 
aB "vcvtph2ps xmm0, xmm0, 0" 8fe878a0c000 
aB "vcvtps2ph xmm0, xmm0, 0" 8fe878a1c000 
a "verr ax" 0f00e0 
a "verr [eax]" 0f0020 
a "verw ax" 0f00e8 
a "verw word [eax]" 0f0028 
a "vextractf128 xmm0, ymm0, 0" c4e37d19c000 
a "vextractf128 xmm0, ymm0, 0x0" c4e37d19c000 
a "vfmadd132pd xmm0, xmm0, xmm0" c4e2f998c0 
a "vfmadd213pd xmm0, xmm0, xmm0" c4e2f9a8c0 
a "vfmadd231pd xmm0, xmm0, xmm0" c4e2f9b8c0 
aB "vfmaddpd xmm0, xmm0, xmm0, xmm0" c4e37969c000 
aB "vfmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d69c000 
aB "vfmaddps xmm0, xmm0, xmm0, xmm0" c4e37968c000 
aB "vfmaddps ymm0, ymm0, ymm0, ymm0" c4e37d68c000 
aB "vfmaddsd xmm0, xmm0, xmm0, xmm0" c4e3796bc000 
aB "vfmaddss xmm0, xmm0, xmm0, xmm0" c4e3796ac000 
aB "vfmaddsubpd xmm0, xmm0, xmm0, xmm0" c4e3795dc000 
aB "vfmaddsubpd ymm0, ymm0, ymm0, ymm0" c4e37d5dc000 
aB "vfmaddsubps xmm0, xmm0, xmm0, xmm0" c4e3795cc000 
aB "vfmaddsubps ymm0, ymm0, ymm0, ymm0" c4e37d5cc000 
aB "vfmsubaddpd xmm0, xmm0, xmm0, xmm0" c4e3795fc000 
aB "vfmsubaddpd ymm0, ymm0, ymm0, ymm0" c4e37d5fc000 
aB "vfmsubaddps xmm0, xmm0, xmm0, xmm0" c4e3795ec000 
aB "vfmsubaddps ymm0, ymm0, ymm0, ymm0" c4e37d5ec000 
aB "vfmsubpd xmm0, xmm0, xmm0, xmm0" c4e3796dc000 
aB "vfmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d6dc000 
aB "vfmsubps xmm0, xmm0, xmm0, xmm0" c4e3796cc000 
aB "vfmsubps ymm0, ymm0, ymm0, ymm0" c4e37d6cc000 
aB "vfmsubsd xmm0, xmm0, xmm0, xmm0" c4e3796fc000 
aB "vfmsubss xmm0, xmm0, xmm0, xmm0" c4e3796ec000 
aB "vfnmaddpd xmm0, xmm0, xmm0, xmm0" c4e37979c000 
aB "vfnmaddpd ymm0, ymm0, ymm0, ymm0" c4e37d79c000 
aB "vfnmaddps xmm0, xmm0, xmm0, xmm0" c4e37978c000 
aB "vfnmaddps ymm0, ymm0, ymm0, ymm0" c4e37d78c000 
aB "vfnmaddsd xmm0, xmm0, xmm0, xmm0" c4e3797bc000 
aB "vfnmaddss xmm0, xmm0, xmm0, xmm0" c4e3797ac000 
aB "vfnmsubpd xmm0, xmm0, xmm0, xmm0" c4e3797dc000 
aB "vfnmsubpd ymm0, ymm0, ymm0, ymm0" c4e37d7dc000 
aB "vfnmsubps xmm0, xmm0, xmm0, xmm0" c4e3797cc000 
aB "vfnmsubps ymm0, ymm0, ymm0, ymm0" c4e37d7cc000 
aB "vfnmsubsd xmm0, xmm0, xmm0, xmm0" c4e3797fc000 
aB "vfnmsubss xmm0, xmm0, xmm0, xmm0" c4e3797ec000 
a "vfrczpd xmm0, xmm0" 8fe97881c0 
a "vfrczps xmm0, xmm0" 8fe97880c0 
a "vfrczsd xmm0, xmm0" 8fe97883c0 
a "vfrczss xmm0, xmm0" 8fe97882c0 
a "vinsertf128 ymm0, ymm0, xmm0, 0" c4e37d18c000 
a "vinsertf128 ymm0, ymm0, xmm0, 0x0" c4e37d18c000 
a "vmaskmovpd ymm0, ymm0, ymmword [0]" c4e27d2d0500000000 
a "vmaskmovps ymm0, ymm0, ymmword [0]" c4e27d2c0500000000 
a "vmcall" 0f01c1 
a "vmclear qword [eax]" 660fc730 
a "vmlaunch" 0f01c2 
aB "vmload" 0f01da 
a "vmmcall" 0f01d9 
a "vmptrld qword [eax]" 0fc730 
a "vmptrst qword [eax]" 0fc738 
a "vmresume" 0f01c3 
aB "vmrun" 0f01d8 
aB "vmsave" 0f01db 
a "vmxoff" 0f01c4 
a "vmxon qword [eax]" f30fc730 
a "vpcmov xmm0, xmm0, xmm0, xmm0" 8fe878a2c000 
a "vpcomb xmm0, xmm0, xmm0, 0" 8fe878ccc000 
a "vpcomd xmm0, xmm0, xmm0, 0" 8fe878cec000 
a "vpcomq xmm0, xmm0, xmm0, 0" 8fe878cfc000 
a "vpcomub xmm0, xmm0, xmm0, 0" 8fe878ecc000 
a "vpcomud xmm0, xmm0, xmm0, 0" 8fe878eec000 
a "vpcomuq xmm0, xmm0, xmm0, 0" 8fe878efc000 
a "vpcomuw xmm0, xmm0, xmm0, 0" 8fe878edc000 
a "vpcomw xmm0, xmm0, xmm0, 0" 8fe878cdc000 
a "vperm2f128 ymm0, ymm0, ymm0, 0" c4e37d06c000 
a "vperm2f128 ymm0, ymm0, ymm0, 0x0" c4e37d06c000  
a "vpermilpd ymm0, ymm0, ymmword [0]" c4e27d0d0500000000 
a "vpermilps ymm0, ymm0, ymmword [0]" c4e27d0c0500000000 
a "vphaddbd xmm0, xmm0" 8fe978c2c0 
a "vphaddbq xmm0, xmm0" 8fe978c3c0 
a "vphaddbw xmm0, xmm0" 8fe978c1c0 
a "vphadddq xmm0, xmm0" 8fe978cbc0 
a "vphaddubd xmm0, xmm0" 8fe978d2c0 
a "vphaddubq xmm0, xmm0" 8fe978d3c0 
a "vphaddubw xmm0, xmm0" 8fe978d1c0 
a "vphaddudq xmm0, xmm0" 8fe978dbc0 
a "vphadduwd xmm0, xmm0" 8fe978d6c0 
a "VPHADDUWQ xmm0, xmm0" 8fe978d7c0 
a "vphaddwd xmm0, xmm0" 8fe978c6c0 
a "vphaddwq xmm0, xmm0" 8fe978c7c0 
a "vphsubbw xmm0, xmm0" 8fe978e1c0 
a "vphsubdq xmm0, xmm0" 8fe978e3c0 
a "vphsubwd xmm0, xmm0" 8fe978e2c0 
aB "vpmacsddxmm0, xmm0, xmm0, xmm0" 8fe8789ec000 
a "vpmacsdqh xmm0, xmm0, xmm0, xmm0" 8fe8789fc000 
a "vpmacsdql xmm0, xmm0, xmm0, xmm0" 8fe87897c000 
a "vpmacssdd xmm0, xmm0, xmm0, xmm0" 8fe8788ec000 
a "vpmacssdqh xmm0, xmm0, xmm0, xmm0" 8fe8788fc000 
a "vpmacssdql xmm0, xmm0, xmm0, xmm0" 8fe87887c000 
a "vpmacsswd xmm0, xmm0, xmm0, xmm0" 8fe87886c000 
a "vpmacssww xmm0, xmm0, xmm0, xmm0" 8fe87885c000 
a "vpmacswd xmm0, xmm0, xmm0, xmm0" 8fe87896c000 
a "vpmacsww xmm0, xmm0, xmm0, xmm0" 8fe87895c000 
a "vpmadcsswd xmm0, xmm0, xmm0, xmm0" 8fe878a6c000 
a "VPMADCSSWD xmm0, xmm0, xmm0, xmm0" 8fe878a6c000 
a "vpmadcswd xmm0, xmm0, xmm0, xmm0" 8fe878b6c000 
a "vpperm xmm0, xmm0, xmm0, xmm0" 8fe878a3c000 
a "vprotb xmm0, xmm0, xmm0" 8fe97890c0 
a "vprotd xmm0, xmm0, xmm0" 8fe97892c0 
a "vprotq xmm0, xmm0, xmm0" 8fe97893c0 
a "vprotw xmm0, xmm0, xmm0" 8fe97891c0 
a "vpshab xmm0, xmm0, xmm0" 8fe97898c0 
a "vpshad xmm0, xmm0, xmm0" 8fe9789ac0 
a "vpshaq xmm0, xmm0, xmm0" 8fe9789bc0 
a "vpshaw xmm0, xmm0, xmm0" 8fe97899c0 
a "vpshlb xmm0, xmm0, xmm0" 8fe97894c0 
a "vpshld xmm0, xmm0, xmm0" 8fe97896c0 
a "vpshlq xmm0, xmm0, xmm0" 8fe97897c0 
a "vpshlw xmm0, xmm0, xmm0" 8fe97895c0 
a "vtestpd ymm0, ymm0" c4e27d0fc0 
a "vtestps ymm0, ymm0" c4e27d0ec0 
a "vzeroall" c5fc77 
a "vzeroupper" c5f877 
a "wbinvd" 0f09 
a "wrmsr" 0f30 
a "xadd byte [eax], al" 0fc000 
a "xadd dword [eax], eax" 0fc100 
a "xchg byte [eax], al" 8600 
a "xchg dword [eax], eax" 8700 
a "xchg eax, eax" 90
a "xchg eax, ebp" 95 
aB "xchg eax, ebx" 87d8 
a "xchg eax, ebx" 93 
a "xchg eax, ecx" 91 
a "xchg eax, edi" 97 
a "xchg eax, edx" 92 
a "xchg eax, esi" 96 
aB "xchg eax, esp" 87e0 
a "xchg eax, esp" 94 
a "xchg ebx, ecx" 87cb
a "xchg ecx, ebp" 87e9
a "xchg ecx, ebx" 87d9
aB "xchg ecx, ecx" 90 
a "xgetbv" 0f01d0 
a "xlatb" d7 
a "xor al, 0" 3400 
a "xor al, byte [eax]" 3200 
a "xor byte [eax], al" 3000 
a "xor dword [eax], eax" 3100
a "xor eax, dword [eax]" 3300 
a "xor [eax], eax" 3100
a "xor eax, eax" 31c0
a "xor eax, ebx" 31d8
a "xor ebx, eax" 31c3
a "xor esi, ebp" 31ee
a "xor esp,esp" 31e4
a "xorpd xmm0, xmmword [eax]" 660f5700 
a "xorps xmm0, xmmword [eax]" 0f5700 
a "xrstor [eax]" 0fae28 
a "xsave [eax]" 0fae20 
a "xsetbv" 0f01d1 
